[preset00]
fRating=1.0
fGammaAdj=1.980001
fDecay=0.5
fVideoEchoZoom=0.999998
fVideoEchoAlpha=0.5
nVideoEchoOrientation=3
nWaveMode=6
bAdditiveWaves=1
bWaveDots=0
bWaveThick=1
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=1
bSolarize=0
bInvert=0
fWaveAlpha=0.311600
fWaveScale=1.228910
fWaveSmoothing=0.0
fWaveParam=0.2
fModWaveAlphaStart=0.710000
fModWaveAlphaEnd=1.3
fWarpAnimSpeed=1.459526
fWarpScale=2.006761
fZoomExponent=1.0
fShader=0.0
zoom=0.999902
rot=0.0
cx=0.5
cy=0.5
dx=0.0
dy=-1.0
warp=0.010000
sx=0.999998
sy=1.0
wave_r=0.0
wave_g=0.0
wave_b=0.0
wave_x=0.5
wave_y=0.5
ob_size=0.0
ob_r=1.0
ob_g=1.0
ob_b=1.0
ob_a=0.050000
ib_size=0.260000
ib_r=0.25
ib_g=0.25
ib_b=0.25
ib_a=0.0
nMotionVectorsX=64.0
nMotionVectorsY=48.0
mv_dx=0.0
mv_dy=0.0
mv_l=1.850000
mv_r=0.499900
mv_g=0.499900
mv_b=0.499900
mv_a=0.0
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=0.891519
wavecode_0_smoothing=0.820000
wavecode_0_r=1.0
wavecode_0_g=1.0
wavecode_0_b=1.0
wavecode_0_a=0.1
wave_0_init1=t1 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init2=t2 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init3=t3 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init4=t4 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init5=t5 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init6=t6 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init7=t7 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init8=t8 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_0_init9=
wave_0_per_frame1=tm = time*.1;
wave_0_per_frame2=t1 = t1*sin(tm*t4) + (1-t1)*sin(tm*t7);
wave_0_per_frame3=t2 = t2*sin(tm*t5) + (1-t2)*sin(tm*t8);
wave_0_per_frame4=t3 = t3*sin(tm*t6) + (1-t3)*sin(tm*1);
wave_0_per_frame5=
wave_0_per_frame6=tic = min(time - tin,1);
wave_0_per_frame7=tin = time;
wave_0_per_frame8=
wave_0_per_frame9=tva = (tic*q1*.5);
wave_0_per_frame10=tvb = (tic*q2*.5);
wave_0_per_frame11=tvc = (tic*q3*.5);
wave_0_per_frame12=
wave_0_per_frame13=q1 = tva;
wave_0_per_frame14=q2 = tvb;
wave_0_per_frame15=q3 = tvc;
wave_0_per_frame16=
wave_0_per_frame17=sz = .5;
wave_0_per_frame18=len = q4;
wave_0_per_frame19=t4 = len;
wave_0_per_point1=ang = 0;
wave_0_per_point2=len = t4;
wave_0_per_point3=mad = .6;
wave_0_per_point4=
wave_0_per_point5=it = if(above(sample,0),(it+equal(lev,7)),1);
wave_0_per_point6=ita = (ita + 1)*above(sample,0);
wave_0_per_point7=
wave_0_per_point8=mod = if(equal(it%2,0),1,  if(equal((it+1)%4,0),2,  if(equal((it+3)%8,0),3,  if(equal((it+7)%16,0),4,  if(equal((it+15)%32,0),5,  if(equal((it+31)%64,0),6,  if(equal((it+63)%128,0),7,7)  ))))));
wave_0_per_point9=
wave_0_per_point10=sw = sw - 1;
wave_0_per_point11=sw = if(equal(lev,7),mod,sw)*above(sample,0);
wave_0_per_point12=
wave_0_per_point13=lev = if(above(sample,0),if(above(sw,0),lev-1,lev+1),7);
wave_0_per_point14=a = lev*.1*1.46;
wave_0_per_point15=
wave_0_per_point16=ar = if(above(sample,0),ar,1);
wave_0_per_point17=ar = if(equal(lev,0),ar*-1,ar);
wave_0_per_point18=br = if(above(sample,0),br,1);
wave_0_per_point19=br = if(equal(lev,1),br*-1,br);
wave_0_per_point20=cr = if(above(sample,0),cr,1);
wave_0_per_point21=cr = if(equal(lev,2),cr*-1,cr);
wave_0_per_point22=dr = if(above(sample,0),dr,1);
wave_0_per_point23=dr = if(equal(lev,3),dr*-1,dr);
wave_0_per_point24=er = if(above(sample,0),er,1);
wave_0_per_point25=er = if(equal(lev,4),er*-1,er);
wave_0_per_point26=fr = if(above(sample,0),fr,1);
wave_0_per_point27=fr = if(equal(lev,5),fr*-1,fr);
wave_0_per_point28=gr = if(above(sample,0),gr,1);
wave_0_per_point29=gr = if(equal(lev,6),gr*-1,gr);
wave_0_per_point30=
wave_0_per_point31=mlev = lev*above(sample,0);
wave_0_per_point32=
wave_0_per_point33=swi = equal(q4,0)*equal(sample,0);
wave_0_per_point34=
wave_0_per_point35=ha = if(swi,1-2*rand(2),ha);
wave_0_per_point36=hb = if(swi,1-2*rand(2),hb);
wave_0_per_point37=hc = if(swi,1-2*rand(2),hc);
wave_0_per_point38=hd = if(swi,1-2*rand(2),hd);
wave_0_per_point39=he = if(swi,1-2*rand(2),he);
wave_0_per_point40=hf = if(swi,1-2*rand(2),hf);
wave_0_per_point41=hg = if(swi,1-2*rand(2),hg);
wave_0_per_point42=
wave_0_per_point43=aang = if(above(sample,0),aang,aang + (q1*.8 + q2*.1 + q3*.1)*ha*1);
wave_0_per_point44=bang = if(above(sample,0),bang,bang + (q1*.57 + q2*.33 + q3*.1)*hb*1.33);
wave_0_per_point45=cang = if(above(sample,0),cang,cang + (q1*.33 + q2*.57 + q3*.1)*hc*1.67);
wave_0_per_point46=dang = if(above(sample,0),dang,dang + (q1*.1 + q2*.8 + q3*.1)*hd*2);
wave_0_per_point47=eang = if(above(sample,0),eang,eang + (q1*.1 + q2*.57 + q3*.33)*he*2.33);
wave_0_per_point48=fang = if(above(sample,0),fang,fang + (q1*.1 + q2*.33 + q3*.57)*hf*2.67);
wave_0_per_point49=gang = if(above(sample,0),gang,gang + (q1*.1 + q2*.1 + q3*.8)*hg*3);
wave_0_per_point50=
wave_0_per_point51=aang = 1.57;
wave_0_per_point52=bang = 1.57;
wave_0_per_point53=cang = 1.57;
wave_0_per_point54=dang = 1.57;
wave_0_per_point55=eang = 1.57;
wave_0_per_point56=fang = 1.57;
wave_0_per_point57=gang = 1.57;
wave_0_per_point58=
wave_0_per_point59=oz = 0;
wave_0_per_point60=
wave_0_per_point61=len = len*mad;
wave_0_per_point62=ox = above(lev,0)*sin(aang)*len*ar;
wave_0_per_point63=oy = above(lev,0)*cos(aang)*len;
wave_0_per_point64=
wave_0_per_point65=an = (ar*aang + br*bang)*br;
wave_0_per_point66=len = len*mad;
wave_0_per_point67=oy = oy + above(lev,1)*sin(an)*len*br;
wave_0_per_point68=oz = oz + above(lev,1)*cos(an)*len;
wave_0_per_point69=
wave_0_per_point70=an = (ar*aang + br*bang + cr*cang)*cr;
wave_0_per_point71=len = len*mad;
wave_0_per_point72=ox = ox + above(lev,2)*sin(an)*len*cr;
wave_0_per_point73=oz = oz + above(lev,2)*cos(an)*len;
wave_0_per_point74=
wave_0_per_point75=an = (ar*aang + br*bang + cr*cang + dr*dang)*dr;
wave_0_per_point76=len = len*mad;
wave_0_per_point77=ox = ox + above(lev,3)*sin(an)*len*dr;
wave_0_per_point78=oy = oy + above(lev,3)*cos(an)*len;
wave_0_per_point79=
wave_0_per_point80=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang)*er;
wave_0_per_point81=len = len*mad;
wave_0_per_point82=ox = ox + above(lev,4)*sin(an)*len*er;
wave_0_per_point83=oz = oz + above(lev,4)*cos(an)*len;
wave_0_per_point84=
wave_0_per_point85=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang + fr*fang)*fr;
wave_0_per_point86=len = len*mad;
wave_0_per_point87=ox = ox + above(lev,5)*sin(an)*len*fr;
wave_0_per_point88=oz = oz + above(lev,5)*cos(an)*len;
wave_0_per_point89=
wave_0_per_point90=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang + fr*fang + gr*gang)*gr;
wave_0_per_point91=len = len*mad;
wave_0_per_point92=oy = oy + above(lev,6)*sin(an)*len*gr;
wave_0_per_point93=ox = ox + above(lev,6)*cos(an)*len;
wave_0_per_point94=
wave_0_per_point95=
wave_0_per_point96=xang = time*1.132;
wave_0_per_point97=xang = q5;
wave_0_per_point98=yang = time*1.153;
wave_0_per_point99=yang = q6;
wave_0_per_point100=zang = time*1.110;
wave_0_per_point101=zang = q7;
wave_0_per_point102=fov = .5;
wave_0_per_point103=
wave_0_per_point104=mx = ox*cos(zang) - oy*sin(zang);
wave_0_per_point105=my = ox*sin(zang) + oy*cos(zang);
wave_0_per_point106=ox = mx;
wave_0_per_point107=oy = my;
wave_0_per_point108=mx = ox*cos(yang) + oz*sin(yang);
wave_0_per_point109=mz = - ox*sin(yang) + oz*cos(yang);
wave_0_per_point110=ox = mx;
wave_0_per_point111=oz = mz;
wave_0_per_point112=my = oy*cos(xang) - oz*sin(xang);
wave_0_per_point113=mz = oy*sin(xang) + oz*cos(xang);
wave_0_per_point114=oy = my;
wave_0_per_point115=oz = mz;
wave_0_per_point116=
wave_0_per_point117=oz = oz - 2;
wave_0_per_point118=x = ox*fov/oz + 0.5;
wave_0_per_point119=x = (x-.5)*0.75 + 0.5;
wave_0_per_point120=y = oy*fov/oz + 0.5;
wave_0_per_point121=
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=0.891519
wavecode_1_smoothing=0.820000
wavecode_1_r=1.0
wavecode_1_g=1.0
wavecode_1_b=1.0
wavecode_1_a=0.1
wave_1_init1=t1 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init2=t2 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init3=t3 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init4=t4 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init5=t5 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init6=t6 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init7=t7 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init8=t8 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_1_init9=
wave_1_per_frame1=tm = time*.1;
wave_1_per_frame2=t1 = t1*sin(tm*t4) + (1-t1)*sin(tm*t7);
wave_1_per_frame3=t2 = t2*sin(tm*t5) + (1-t2)*sin(tm*t8);
wave_1_per_frame4=t3 = t3*sin(tm*t6) + (1-t3)*sin(tm*1);
wave_1_per_frame5=
wave_1_per_frame6=tic = min(time - tin,1);
wave_1_per_frame7=tin = time;
wave_1_per_frame8=
wave_1_per_frame9=tva = (tic*q1*.5);
wave_1_per_frame10=tvb = (tic*q2*.5);
wave_1_per_frame11=tvc = (tic*q3*.5);
wave_1_per_frame12=
wave_1_per_frame13=q1 = tva;
wave_1_per_frame14=q2 = tvb;
wave_1_per_frame15=q3 = tvc;
wave_1_per_frame16=
wave_1_per_frame17=sz = .5;
wave_1_per_frame18=len = q4;
wave_1_per_frame19=t4 = len;
wave_1_per_point1=ang = 0;
wave_1_per_point2=len = t4;
wave_1_per_point3=mad = .6;
wave_1_per_point4=
wave_1_per_point5=it = if(above(sample,0),(it+equal(lev,7)),1);
wave_1_per_point6=ita = (ita + 1)*above(sample,0);
wave_1_per_point7=
wave_1_per_point8=mod = if(equal(it%2,0),1,  if(equal((it+1)%4,0),2,  if(equal((it+3)%8,0),3,  if(equal((it+7)%16,0),4,  if(equal((it+15)%32,0),5,  if(equal((it+31)%64,0),6,  if(equal((it+63)%128,0),7,7)  ))))));
wave_1_per_point9=
wave_1_per_point10=sw = sw - 1;
wave_1_per_point11=sw = if(equal(lev,7),mod,sw)*above(sample,0);
wave_1_per_point12=
wave_1_per_point13=lev = if(above(sample,0),if(above(sw,0),lev-1,lev+1),7);
wave_1_per_point14=a = lev*.1*1.46;
wave_1_per_point15=
wave_1_per_point16=ar = if(above(sample,0),ar,1);
wave_1_per_point17=ar = if(equal(lev,0),ar*-1,ar);
wave_1_per_point18=br = if(above(sample,0),br,1);
wave_1_per_point19=br = if(equal(lev,1),br*-1,br);
wave_1_per_point20=cr = if(above(sample,0),cr,1);
wave_1_per_point21=cr = if(equal(lev,2),cr*-1,cr);
wave_1_per_point22=dr = if(above(sample,0),dr,1);
wave_1_per_point23=dr = if(equal(lev,3),dr*-1,dr);
wave_1_per_point24=er = if(above(sample,0),er,1);
wave_1_per_point25=er = if(equal(lev,4),er*-1,er);
wave_1_per_point26=fr = if(above(sample,0),fr,1);
wave_1_per_point27=fr = if(equal(lev,5),fr*-1,fr);
wave_1_per_point28=gr = if(above(sample,0),gr,1);
wave_1_per_point29=gr = if(equal(lev,6),gr*-1,gr);
wave_1_per_point30=
wave_1_per_point31=mlev = lev*above(sample,0);
wave_1_per_point32=
wave_1_per_point33=swi = equal(q4,0)*equal(sample,0);
wave_1_per_point34=
wave_1_per_point35=ha = if(swi,1-2*rand(2),ha);
wave_1_per_point36=hb = if(swi,1-2*rand(2),hb);
wave_1_per_point37=hc = if(swi,1-2*rand(2),hc);
wave_1_per_point38=hd = if(swi,1-2*rand(2),hd);
wave_1_per_point39=he = if(swi,1-2*rand(2),he);
wave_1_per_point40=hf = if(swi,1-2*rand(2),hf);
wave_1_per_point41=hg = if(swi,1-2*rand(2),hg);
wave_1_per_point42=
wave_1_per_point43=aang = if(above(sample,0),aang,aang + (q1*.8 + q2*.1 + q3*.1)*ha*1);
wave_1_per_point44=bang = if(above(sample,0),bang,bang + (q1*.57 + q2*.33 + q3*.1)*hb*1.33);
wave_1_per_point45=cang = if(above(sample,0),cang,cang + (q1*.33 + q2*.57 + q3*.1)*hc*1.67);
wave_1_per_point46=dang = if(above(sample,0),dang,dang + (q1*.1 + q2*.8 + q3*.1)*hd*2);
wave_1_per_point47=eang = if(above(sample,0),eang,eang + (q1*.1 + q2*.57 + q3*.33)*he*2.33);
wave_1_per_point48=fang = if(above(sample,0),fang,fang + (q1*.1 + q2*.33 + q3*.57)*hf*2.67);
wave_1_per_point49=gang = if(above(sample,0),gang,gang + (q1*.1 + q2*.1 + q3*.8)*hg*3);
wave_1_per_point50=
wave_1_per_point51=aang = 1.57;
wave_1_per_point52=bang = 1.57;
wave_1_per_point53=cang = 1.57;
wave_1_per_point54=dang = 1.57;
wave_1_per_point55=eang = 1.57;
wave_1_per_point56=fang = 1.57;
wave_1_per_point57=gang = 1.57;
wave_1_per_point58=
wave_1_per_point59=oz = 0;
wave_1_per_point60=
wave_1_per_point61=len = len*mad;
wave_1_per_point62=ox = above(lev,0)*sin(aang)*len*ar;
wave_1_per_point63=oy = above(lev,0)*cos(aang)*len;
wave_1_per_point64=
wave_1_per_point65=an = (ar*aang + br*bang)*br;
wave_1_per_point66=len = len*mad;
wave_1_per_point67=oy = oy + above(lev,1)*sin(an)*len*br;
wave_1_per_point68=oz = oz + above(lev,1)*cos(an)*len;
wave_1_per_point69=
wave_1_per_point70=an = (ar*aang + br*bang + cr*cang)*cr;
wave_1_per_point71=len = len*mad;
wave_1_per_point72=ox = ox + above(lev,2)*sin(an)*len*cr;
wave_1_per_point73=oz = oz + above(lev,2)*cos(an)*len;
wave_1_per_point74=
wave_1_per_point75=an = (ar*aang + br*bang + cr*cang + dr*dang)*dr;
wave_1_per_point76=len = len*mad;
wave_1_per_point77=ox = ox + above(lev,3)*sin(an)*len*dr;
wave_1_per_point78=oy = oy + above(lev,3)*cos(an)*len;
wave_1_per_point79=
wave_1_per_point80=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang)*er;
wave_1_per_point81=len = len*mad;
wave_1_per_point82=ox = ox + above(lev,4)*sin(an)*len*er;
wave_1_per_point83=oz = oz + above(lev,4)*cos(an)*len;
wave_1_per_point84=
wave_1_per_point85=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang + fr*fang)*fr;
wave_1_per_point86=len = len*mad;
wave_1_per_point87=ox = ox + above(lev,5)*sin(an)*len*fr;
wave_1_per_point88=oz = oz + above(lev,5)*cos(an)*len;
wave_1_per_point89=
wave_1_per_point90=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang + fr*fang + gr*gang)*gr;
wave_1_per_point91=len = len*mad;
wave_1_per_point92=oy = oy + above(lev,6)*sin(an)*len*gr;
wave_1_per_point93=ox = ox + above(lev,6)*cos(an)*len;
wave_1_per_point94=
wave_1_per_point95=
wave_1_per_point96=xang = time*1.132;
wave_1_per_point97=xang = q5;
wave_1_per_point98=yang = time*1.153;
wave_1_per_point99=yang = q6;
wave_1_per_point100=zang = time*1.110;
wave_1_per_point101=zang = q7 + 1.57;
wave_1_per_point102=fov = .5;
wave_1_per_point103=
wave_1_per_point104=mx = ox*cos(zang) - oy*sin(zang);
wave_1_per_point105=my = ox*sin(zang) + oy*cos(zang);
wave_1_per_point106=ox = mx;
wave_1_per_point107=oy = my;
wave_1_per_point108=mx = ox*cos(yang) + oz*sin(yang);
wave_1_per_point109=mz = - ox*sin(yang) + oz*cos(yang);
wave_1_per_point110=ox = mx;
wave_1_per_point111=oz = mz;
wave_1_per_point112=my = oy*cos(xang) - oz*sin(xang);
wave_1_per_point113=mz = oy*sin(xang) + oz*cos(xang);
wave_1_per_point114=oy = my;
wave_1_per_point115=oz = mz;
wave_1_per_point116=
wave_1_per_point117=oz = oz - 2;
wave_1_per_point118=x = ox*fov/oz + 0.5;
wave_1_per_point119=x = (x-.5)*0.75 + 0.5;
wave_1_per_point120=y = oy*fov/oz + 0.5;
wave_1_per_point121=
wavecode_2_enabled=0
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=0.891519
wavecode_2_smoothing=0.820000
wavecode_2_r=1.0
wavecode_2_g=1.0
wavecode_2_b=1.0
wavecode_2_a=0.1
wave_2_init1=t1 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init2=t2 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init3=t3 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init4=t4 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init5=t5 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init6=t6 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init7=t7 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init8=t8 = 1 + (rand(101)*.01 - rand(101)*.01)*.3;
wave_2_init9=
wave_2_per_frame1=tm = time*.1;
wave_2_per_frame2=t1 = t1*sin(tm*t4) + (1-t1)*sin(tm*t7);
wave_2_per_frame3=t2 = t2*sin(tm*t5) + (1-t2)*sin(tm*t8);
wave_2_per_frame4=t3 = t3*sin(tm*t6) + (1-t3)*sin(tm*1);
wave_2_per_frame5=
wave_2_per_frame6=tic = min(time - tin,1);
wave_2_per_frame7=tin = time;
wave_2_per_frame8=
wave_2_per_frame9=tva = (tic*q1*.5);
wave_2_per_frame10=tvb = (tic*q2*.5);
wave_2_per_frame11=tvc = (tic*q3*.5);
wave_2_per_frame12=
wave_2_per_frame13=q1 = tva;
wave_2_per_frame14=q2 = tvb;
wave_2_per_frame15=q3 = tvc;
wave_2_per_frame16=
wave_2_per_frame17=sz = .5;
wave_2_per_frame18=len = 1;
wave_2_per_frame19=t4 = len;
wave_2_per_point1=ang = 0;
wave_2_per_point2=len = t4;
wave_2_per_point3=mad = .6;
wave_2_per_point4=
wave_2_per_point5=it = if(above(sample,0),(it+equal(lev,7)),1);
wave_2_per_point6=ita = (ita + 1)*above(sample,0);
wave_2_per_point7=
wave_2_per_point8=mod = if(equal(it%2,0),1,  if(equal((it+1)%4,0),2,  if(equal((it+3)%8,0),3,  if(equal((it+7)%16,0),4,  if(equal((it+15)%32,0),5,  if(equal((it+31)%64,0),6,  if(equal((it+63)%128,0),7,7)  ))))));
wave_2_per_point9=
wave_2_per_point10=sw = sw - 1;
wave_2_per_point11=sw = if(equal(lev,7),mod,sw)*above(sample,0);
wave_2_per_point12=
wave_2_per_point13=lev = if(above(sample,0),if(above(sw,0),lev-1,lev+1),7);
wave_2_per_point14=a = lev*.1*1.46;
wave_2_per_point15=
wave_2_per_point16=ar = if(above(sample,0),ar,1);
wave_2_per_point17=ar = if(equal(lev,0),ar*-1,ar);
wave_2_per_point18=br = if(above(sample,0),br,1);
wave_2_per_point19=br = if(equal(lev,1),br*-1,br);
wave_2_per_point20=cr = if(above(sample,0),cr,1);
wave_2_per_point21=cr = if(equal(lev,2),cr*-1,cr);
wave_2_per_point22=dr = if(above(sample,0),dr,1);
wave_2_per_point23=dr = if(equal(lev,3),dr*-1,dr);
wave_2_per_point24=er = if(above(sample,0),er,1);
wave_2_per_point25=er = if(equal(lev,4),er*-1,er);
wave_2_per_point26=fr = if(above(sample,0),fr,1);
wave_2_per_point27=fr = if(equal(lev,5),fr*-1,fr);
wave_2_per_point28=gr = if(above(sample,0),gr,1);
wave_2_per_point29=gr = if(equal(lev,6),gr*-1,gr);
wave_2_per_point30=
wave_2_per_point31=mlev = lev*above(sample,0);
wave_2_per_point32=
wave_2_per_point33=swi = equal(q4,0)*equal(sample,0);
wave_2_per_point34=
wave_2_per_point35=ha = if(swi,1-2*rand(2),ha);
wave_2_per_point36=hb = if(swi,1-2*rand(2),hb);
wave_2_per_point37=hc = if(swi,1-2*rand(2),hc);
wave_2_per_point38=hd = if(swi,1-2*rand(2),hd);
wave_2_per_point39=he = if(swi,1-2*rand(2),he);
wave_2_per_point40=hf = if(swi,1-2*rand(2),hf);
wave_2_per_point41=hg = if(swi,1-2*rand(2),hg);
wave_2_per_point42=
wave_2_per_point43=aang = if(above(sample,0),aang,aang + (q1*.8 + q2*.1 + q3*.1)*ha*1);
wave_2_per_point44=bang = if(above(sample,0),bang,bang + (q1*.57 + q2*.33 + q3*.1)*hb*1.33);
wave_2_per_point45=cang = if(above(sample,0),cang,cang + (q1*.33 + q2*.57 + q3*.1)*hc*1.67);
wave_2_per_point46=dang = if(above(sample,0),dang,dang + (q1*.1 + q2*.8 + q3*.1)*hd*2);
wave_2_per_point47=eang = if(above(sample,0),eang,eang + (q1*.1 + q2*.57 + q3*.33)*he*2.33);
wave_2_per_point48=fang = if(above(sample,0),fang,fang + (q1*.1 + q2*.33 + q3*.57)*hf*2.67);
wave_2_per_point49=gang = if(above(sample,0),gang,gang + (q1*.1 + q2*.1 + q3*.8)*hg*3);
wave_2_per_point50=
wave_2_per_point51=aang = 1.57;
wave_2_per_point52=bang = 1.57;
wave_2_per_point53=cang = 1.57;
wave_2_per_point54=dang = 1.57;
wave_2_per_point55=eang = 1.57;
wave_2_per_point56=fang = 1.57;
wave_2_per_point57=gang = 1.57;
wave_2_per_point58=
wave_2_per_point59=oz = 0;
wave_2_per_point60=
wave_2_per_point61=len = len*mad;
wave_2_per_point62=ox = above(lev,0)*sin(aang)*len*ar;
wave_2_per_point63=oy = above(lev,0)*cos(aang)*len;
wave_2_per_point64=
wave_2_per_point65=an = (ar*aang + br*bang)*br;
wave_2_per_point66=len = len*mad;
wave_2_per_point67=oy = oy + above(lev,1)*sin(an)*len*br;
wave_2_per_point68=oz = oz + above(lev,1)*cos(an)*len;
wave_2_per_point69=
wave_2_per_point70=an = (ar*aang + br*bang + cr*cang)*cr;
wave_2_per_point71=len = len*mad;
wave_2_per_point72=ox = ox + above(lev,2)*sin(an)*len*cr;
wave_2_per_point73=oz = oz + above(lev,2)*cos(an)*len;
wave_2_per_point74=
wave_2_per_point75=an = (ar*aang + br*bang + cr*cang + dr*dang)*dr;
wave_2_per_point76=len = len*mad;
wave_2_per_point77=ox = ox + above(lev,3)*sin(an)*len*dr;
wave_2_per_point78=oy = oy + above(lev,3)*cos(an)*len;
wave_2_per_point79=
wave_2_per_point80=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang)*er;
wave_2_per_point81=len = len*mad;
wave_2_per_point82=ox = ox + above(lev,4)*sin(an)*len*er;
wave_2_per_point83=oz = oz + above(lev,4)*cos(an)*len;
wave_2_per_point84=
wave_2_per_point85=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang + fr*fang)*fr;
wave_2_per_point86=len = len*mad;
wave_2_per_point87=ox = ox + above(lev,5)*sin(an)*len*fr;
wave_2_per_point88=oz = oz + above(lev,5)*cos(an)*len;
wave_2_per_point89=
wave_2_per_point90=an = (ar*aang + br*bang + cr*cang + dr*dang + er*eang + fr*fang + gr*gang)*gr;
wave_2_per_point91=len = len*mad;
wave_2_per_point92=oy = oy + above(lev,6)*sin(an)*len*gr;
wave_2_per_point93=ox = ox + above(lev,6)*cos(an)*len;
wave_2_per_point94=
wave_2_per_point95=
wave_2_per_point96=xang = time*1.132;
wave_2_per_point97=xang = q5;
wave_2_per_point98=yang = time*1.153;
wave_2_per_point99=yang = q6;
wave_2_per_point100=zang = time*1.110;
wave_2_per_point101=zang = q7;
wave_2_per_point102=fov = .5;
wave_2_per_point103=
wave_2_per_point104=mx = ox*cos(zang) - oy*sin(zang);
wave_2_per_point105=my = ox*sin(zang) + oy*cos(zang);
wave_2_per_point106=ox = mx;
wave_2_per_point107=oy = my;
wave_2_per_point108=mx = ox*cos(yang) + oz*sin(yang);
wave_2_per_point109=mz = - ox*sin(yang) + oz*cos(yang);
wave_2_per_point110=ox = mx;
wave_2_per_point111=oz = mz;
wave_2_per_point112=my = oy*cos(xang) - oz*sin(xang);
wave_2_per_point113=mz = oy*sin(xang) + oz*cos(xang);
wave_2_per_point114=oy = my;
wave_2_per_point115=oz = mz;
wave_2_per_point116=
wave_2_per_point117=
wave_2_per_point118=oz = oz - 2;
wave_2_per_point119=x = ox*fov/oz + 0.5;
wave_2_per_point120=x = (x-.5)*0.75 + 0.5;
wave_2_per_point121=y = oy*fov/oz + 0.5;
wave_2_per_point122=
wavecode_3_enabled=0
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=0
wavecode_3_bAdditive=0
wavecode_3_scaling=1.0
wavecode_3_smoothing=0.5
wavecode_3_r=1.0
wavecode_3_g=1.0
wavecode_3_b=1.0
wavecode_3_a=1.0
wave_3_per_point1=ra = .8;
wave_3_per_point2=rb = .5;
wave_3_per_point3=pib = 6.28318530718;
wave_3_per_point4=
wave_3_per_point5=
wave_3_per_point6=tic = min(time-tin,.1);
wave_3_per_point7=tin = if(equal(sample,0),time,tin);
wave_3_per_point8=
wave_3_per_point9=mod = 1.5 + .5*sin(time*.15);
wave_3_per_point10=med = 1.5 + .5*sin(time*.134);
wave_3_per_point11=med = 5;
wave_3_per_point12=amod = 3;
wave_3_per_point13=
wave_3_per_point14=vr = rand(10001)*.0001;
wave_3_per_point15=rb = rb + rand(10001)*.0001*.1;
wave_3_per_point16=
wave_3_per_point17=a = vr;
wave_3_per_point18=
wave_3_per_point19=sa = vr*pib*.5;
wave_3_per_point20=sp = sa*mod + q1*1.3;
wave_3_per_point21=sam = sa*med - q1*.219;
wave_3_per_point22=
wave_3_per_point23=ox = ra*sin(sam*pib);
wave_3_per_point24=oy = ra*cos(sam*pib);
wave_3_per_point25=ox = ox + rb*-cos(sp)*sin(sam*pib);
wave_3_per_point26=oz = rb*-sin(sp);
wave_3_per_point27=oy = oy + rb*-cos(sp)*cos(sam*pib);
wave_3_per_point28=
wave_3_per_point29=
wave_3_per_point30=xang = time*.132;
wave_3_per_point31=xang = q2;
wave_3_per_point32=yang = time*.153;
wave_3_per_point33=yang = q3;
wave_3_per_point34=zang = time*.110;
wave_3_per_point35=zang = q4;
wave_3_per_point36=fov = 0.6 + 0.2*sin(time);
wave_3_per_point37=fov = .5;
wave_3_per_point38=
wave_3_per_point39=mx = ox*cos(zang) - oy*sin(zang);
wave_3_per_point40=my = ox*sin(zang) + oy*cos(zang);
wave_3_per_point41=ox = mx;
wave_3_per_point42=oy = my;
wave_3_per_point43=mx = ox*cos(yang) + oz*sin(yang);
wave_3_per_point44=mz = - ox*sin(yang) + oz*cos(yang);
wave_3_per_point45=ox = mx;
wave_3_per_point46=oz = mz;
wave_3_per_point47=my = oy*cos(xang) - oz*sin(xang);
wave_3_per_point48=mz = oy*sin(xang) + oz*cos(xang);
wave_3_per_point49=oy = my;
wave_3_per_point50=oz = mz;
wave_3_per_point51=
wave_3_per_point52=oz = oz - 2;
wave_3_per_point53=x = ox*fov/oz + 0.5;
wave_3_per_point54=x = (x-.5)*0.75 + 0.5;
wave_3_per_point55=y = oy*fov/oz + 0.5;
wave_3_per_point56=
shapecode_0_enabled=1
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=1
shapecode_0_textured=1
shapecode_0_x=0.5
shapecode_0_y=0.5
shapecode_0_rad=1.854834
shapecode_0_ang=1.570796
shapecode_0_tex_ang=0.0
shapecode_0_tex_zoom=0.539067
shapecode_0_r=1.0
shapecode_0_g=0.940000
shapecode_0_b=0.890000
shapecode_0_a=1.0
shapecode_0_r2=0.840000
shapecode_0_g2=0.930000
shapecode_0_b2=1.0
shapecode_0_a2=1.0
shapecode_0_border_r=1.0
shapecode_0_border_g=1.0
shapecode_0_border_b=0.0
shapecode_0_border_a=0.0
shape_0_per_frame1=x = .4998;
shape_0_per_frame2=y = .5002;
shape_0_per_frame3=
shape_0_per_frame4=ti = time*.3;
shape_0_per_frame5=r = .925 + .05*sin(ti*1.721);
shape_0_per_frame6=g = .925 + .05*sin(ti*1.838);
shape_0_per_frame7=b = .925 + .05*sin(ti*1.968);
shape_0_per_frame8=
shape_0_per_frame9=r2 = 1.875 - r;
shape_0_per_frame10=g2 = 1.875 - g;
shape_0_per_frame11=b2 = 1.875 - b;
shape_0_per_frame12=
shapecode_1_enabled=1
shapecode_1_sides=63
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=1
shapecode_1_x=0.5
shapecode_1_y=0.5
shapecode_1_rad=1.998625
shapecode_1_ang=0.0
shapecode_1_tex_ang=0.0
shapecode_1_tex_zoom=0.499805
shapecode_1_r=1.0
shapecode_1_g=1.0
shapecode_1_b=1.0
shapecode_1_a=0.1
shapecode_1_r2=1.0
shapecode_1_g2=1.0
shapecode_1_b2=1.0
shapecode_1_a2=0.6
shapecode_1_border_r=0.5
shapecode_1_border_g=0.5
shapecode_1_border_b=0.5
shapecode_1_border_a=0.0
shapecode_2_enabled=1
shapecode_2_sides=63
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=1
shapecode_2_x=0.123000
shapecode_2_y=0.0
shapecode_2_rad=0.273185
shapecode_2_ang=0.0
shapecode_2_tex_ang=0.0
shapecode_2_tex_zoom=0.499805
shapecode_2_r=1.0
shapecode_2_g=1.0
shapecode_2_b=1.0
shapecode_2_a=1.0
shapecode_2_r2=1.0
shapecode_2_g2=1.0
shapecode_2_b2=1.0
shapecode_2_a2=0.0
shapecode_2_border_r=0.5
shapecode_2_border_g=0.5
shapecode_2_border_b=0.5
shapecode_2_border_a=0.0
shapecode_3_enabled=1
shapecode_3_sides=63
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=1
shapecode_3_x=0.5
shapecode_3_y=1.0
shapecode_3_rad=0.548217
shapecode_3_ang=0.0
shapecode_3_tex_ang=0.0
shapecode_3_tex_zoom=0.499805
shapecode_3_r=1.0
shapecode_3_g=1.0
shapecode_3_b=1.0
shapecode_3_a=1.0
shapecode_3_r2=1.0
shapecode_3_g2=1.0
shapecode_3_b2=1.0
shapecode_3_a2=0.0
shapecode_3_border_r=0.5
shapecode_3_border_g=0.5
shapecode_3_border_b=0.5
shapecode_3_border_a=0.0
per_frame_1=warp = 0;
per_frame_2=zoom=1.;
per_frame_3=decay=.5;
per_frame_4=
per_frame_5=tic = min(time-tin,.1);
per_frame_6=tin = time;
per_frame_7=
per_frame_8=ra = 10;
per_frame_9=treb_avg = tic*(treb_avg*(1/tic - ra) + ra*treb);
per_frame_10=mid_avg = tic*(mid_avg*(1/tic - ra) + ra*mid);
per_frame_11=bass_avg = tic*(bass_avg*(1/tic - ra) + ra*bass);
per_frame_12=vav = tic*(vav*(1/tic - ra) + ra*(bass+treb+mid)*.33333);
per_frame_13=
per_frame_14=tt = tt + tic*treb_avg;
per_frame_15=mt = mt + tic*mid_avg;
per_frame_16=bt = bt + tic*bass_avg;
per_frame_17=vt = vt + tic*vav;
per_frame_18=
per_frame_19=ob_size = min((pow(bass_avg+1,6)-1)*.0001,.7);
per_frame_20=
per_frame_21=sp = abs(vav - slide)*.1;
per_frame_22=
per_frame_23=slide = if(above(slide,vav),slide-tic*sp,slide+tic*sp) + (1-toc)*vav;
per_frame_24=toc = 1;
per_frame_25=
per_frame_26=
per_frame_27=q1 = treb_avg;
per_frame_28=q2 = mid_avg;
per_frame_29=q3 = bass_avg;
per_frame_30=
per_frame_31=q4 = min(slide*1.2,1.5);
per_frame_32=
per_frame_33=q5 = tt*.4;
per_frame_34=q6 = mt*.4;
per_frame_35=q7 = bt*.4;
