[preset00]
fRating=3.000000
fGammaAdj=1.000000
fDecay=0.898999
fVideoEchoZoom=0.999993
fVideoEchoAlpha=0.000000
nVideoEchoOrientation=0
nWaveMode=0
bAdditiveWaves=0
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001000
fWaveScale=0.411715
fWaveSmoothing=0.900000
fWaveParam=-0.180000
fModWaveAlphaStart=0.750000
fModWaveAlphaEnd=0.950000
fWarpAnimSpeed=1.000000
fWarpScale=1.000000
fZoomExponent=1.000000
fShader=0.000000
zoom=0.999999
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=1.000000
sy=1.000000
wave_r=0.000000
wave_g=0.000000
wave_b=0.000000
wave_x=0.500000
wave_y=0.500000
ob_size=0.005000
ob_r=0.000000
ob_g=0.000000
ob_b=0.000000
ob_a=0.920000
ib_size=0.000000
ib_r=0.000000
ib_g=0.000000
ib_b=0.000000
ib_a=0.000000
nMotionVectorsX=12.000000
nMotionVectorsY=9.000000
mv_dx=0.000000
mv_dy=0.000000
mv_l=0.900000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=1
wavecode_0_scaling=1.001827
wavecode_0_smoothing=0.000000
wavecode_0_r=1.000000
wavecode_0_g=1.000000
wavecode_0_b=1.000000
wavecode_0_a=1.000000
wave_0_per_frame1=speed=.015;
wave_0_per_frame2=length=.1;
wave_0_per_frame3=crosssectionrad=.1;
wave_0_per_frame4=
wave_0_per_frame5=t1= speed*time-int(speed*time);
wave_0_per_frame6=t2= length;
wave_0_per_frame7=t3= crosssectionrad;
wave_0_per_frame8=
wave_0_per_frame9=t=t1*6.2831;
wave_0_per_frame10=t6=cos(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_0_per_frame11=t7=cos(1.9+.7*t)*sin(t);
wave_0_per_frame12=t8=cos(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_0_per_frame13=
wave_0_per_frame14=q1=2*cos(t)*(1+3.1415*cos(2.98+2*t))*cos(.43+2*t+3.1415*sin(2.98+2*t))-sin(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_0_per_frame15=q2=cos(1.9+.7*t)*cos(t)-.7*sin(1.9+.7*t)*sin(t);
wave_0_per_frame16=q3=cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))*(2-6.2831*sin(1.01+2*t))-2*sin(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_0_per_frame17=invFDmag=1/sqrt( q1*q1 + q2*q2 + q3*q3 );
wave_0_per_frame18=
wave_0_per_frame19=sdX=-4*cos(.43+2*t+3.1415*sin(2.98+2*t))*(sin(t)+3.1415*sin(2.98+3*t))-cos(t)*(5+25.132*cos(2.98+2*t)+39.4761*sqr(cos(2.98+2*t)))*sin( .43+2*t+3.1415*sin(2.98+2*t));
wave_0_per_frame20=sdY=-1.4*cos(t)*sin(1.9+.7*t)-1.49*cos(1.9+.7*t)*sin(t);
wave_0_per_frame21=sdZ=-12.566*cos(1.01+2*t)*cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))+8*cos(2*t+3.1415*cos(1.01+2*t))*(-1+3.1415*sin(1.01+2*t))*sin(1.54+2*t) - 4*cos(1.54+2*t)*(2-6.2831*sin(1.01+2*t)+9.869*sqr(sin(1.01+2*t)))*sin(2*t+3.1415*cos(1.01+2*t));
wave_0_per_frame22=
wave_0_per_frame23=q4=q2*sdZ-sdY*q3;
wave_0_per_frame24=q5=q3*sdX-q1*sdZ;
wave_0_per_frame25=q6=q1*sdY-q2*sdX;
wave_0_per_frame26=invSNmag=1/sqrt( q4*q4+q5*q5+q6*q6 );
wave_0_per_frame27=q4=q4*invSNmag;
wave_0_per_frame28=q5=q5*invSNmag;
wave_0_per_frame29=q6=q6*invSNmag;
wave_0_per_frame30=
wave_0_per_frame31=q1=q1*invFDmag;
wave_0_per_frame32=q2=q2*invFDmag;
wave_0_per_frame33=q3=q3*invFDmag;
wave_0_per_frame34=
wave_0_per_frame35=q7=q5*q3-q2*q6;
wave_0_per_frame36=q8=q6*q1-q4*q3;
wave_0_per_frame37=
wave_0_per_point1=t=(t1+(0+sqr(sample))*t2);
wave_0_per_point2=t=if(above(t,1),t-1,t);
wave_0_per_point3=t=t*6.2831;
wave_0_per_point4=
wave_0_per_point5=mx=cos(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_0_per_point6=my=cos(1.9+.7*t)*sin(t);
wave_0_per_point7=mz=cos(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_0_per_point8=
wave_0_per_point9=fdX=2*cos(t)*(1+3.1415*cos(2.98+2*t))*cos(.43+2*t+3.1415*sin(2.98+2*t))-sin(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_0_per_point10=fdY=cos(1.9+.7*t)*cos(t)-.7*sin(1.9+.7*t)*sin(t);
wave_0_per_point11=fdZ=cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))*(2-6.2831*sin(1.01+2*t))-2*sin(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_0_per_point12=invFDmag=1/sqrt( fdX*fdX + fdY*fdY + fdZ*fdZ );
wave_0_per_point13=
wave_0_per_point14=sdX=-4*cos(.43+2*t+3.1415*sin(2.98+2*t))*(sin(t)+3.1415*sin(2.98+3*t))-cos(t)*(5+25.132*cos(2.98+2*t)+39.4761*sqr(cos(2.98+2*t)))*sin( .43+2*t+3.1415*sin(2.98+2*t));
wave_0_per_point15=sdY=-1.4*cos(t)*sin(1.9+.7*t)-1.49*cos(1.9+.7*t)*sin(t);
wave_0_per_point16=sdZ=-12.566*cos(1.01+2*t)*cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))+8*cos(2*t+3.1415*cos(1.01+2*t))*(-1+3.1415*sin(1.01+2*t))*sin(1.54+2*t) - 4*cos(1.54+2*t)*(2-6.2831*sin(1.01+2*t)+9.869*sqr(sin(1.01+2*t)))*sin(2*t+3.1415*cos(1.01+2*t));
wave_0_per_point17=
wave_0_per_point18=snX=fdY*sdZ-sdY*fdZ;
wave_0_per_point19=snY=fdZ*sdX-fdX*sdZ;
wave_0_per_point20=snZ=fdX*sdY-fdY*sdX;
wave_0_per_point21=invSNmag=1/sqrt( snX*snX+snY*snY+snZ*snZ );
wave_0_per_point22=snX=snX*invSNmag;
wave_0_per_point23=snY=snY*invSNmag;
wave_0_per_point24=snZ=snZ*invSNmag;
wave_0_per_point25=
wave_0_per_point26=fdX=fdX*invFDmag;
wave_0_per_point27=fdY=fdY*invFDmag;
wave_0_per_point28=fdZ=fdZ*invFDmag;
wave_0_per_point29=
wave_0_per_point30=fnX=snY*fdZ-fdY*snZ;
wave_0_per_point31=fnY=snZ*fdX-snX*fdZ;
wave_0_per_point32=fnZ=snX*fdY-snY*fdX;
wave_0_per_point33=
wave_0_per_point34=angl=t*188.493;
wave_0_per_point35=c=sqrt(1-sample);
wave_0_per_point36=mx=mx+t3*c*(snX*cos(angl)+fnX*sin(angl));
wave_0_per_point37=my=my+t3*c*(snY*cos(angl)+fnY*sin(angl));
wave_0_per_point38=mz=mz+t3*c*(snZ*cos(angl)+fnZ*sin(angl));
wave_0_per_point39=
wave_0_per_point40=qq9=q4*q2-q5*q1;
wave_0_per_point41=vx=(q7*mx+q8*my+qq9*mz-(t6*q7+t7*q8+t8*qq9));
wave_0_per_point42=vy=(q4*mx+q5*my+q6*mz-(t6*q4+t7*q5+t8*q6));
wave_0_per_point43=vw=q1*mx+q2*my+q3*mz-(t6*q1+t7*q2+t8*q3);
wave_0_per_point44=
wave_0_per_point45=ox=(vx/vw)*.15;
wave_0_per_point46=oy=(vy/vw)*.15;
wave_0_per_point47=x=.5-oy;
wave_0_per_point48=y=.5+ox*1.25;
wave_0_per_point49=a=above(vw,.02)*pow(1-min(vw,1),2);
wave_0_per_point50=
wave_0_per_point51=hue=vw;
wave_0_per_point52=h=6*(hue-int(hue));
wave_0_per_point53=sw1=below(h,1); sw2=(1-sw1)*below(h,2); sw3=(1-sw1)*(1-sw2)*below(h,3); sw4=(1-sw1)*(1-sw2)*(1-sw3)*below(h,4);
wave_0_per_point54=sw6=above(h,5); sw5=(1-sw1)*(1-sw2)*(1-sw3)*(1-sw4)*(1-sw6);
wave_0_per_point55=r=sw1+sw2*(2-h)+sw5*(h-4)+sw6;
wave_0_per_point56=g=sw1*h+sw2+sw3+sw4*(4-h);
wave_0_per_point57=b=sw3*(h-2)+sw4+sw5+sw6*(6-h);
wavecode_1_enabled=0
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=0
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.500000
wavecode_1_r=1.000000
wavecode_1_g=1.000000
wavecode_1_b=1.000000
wavecode_1_a=1.000000
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=1
wavecode_2_scaling=0.999998
wavecode_2_smoothing=0.000000
wavecode_2_r=1.000000
wavecode_2_g=1.000000
wavecode_2_b=1.000000
wavecode_2_a=1.000000
wave_2_per_frame1=speed=.015;
wave_2_per_frame2=
wave_2_per_frame3=t= 6.2831*(speed*time-int(speed*time));
wave_2_per_frame4=
wave_2_per_frame5=t1=2*cos(t)*(1+3.1415*cos(2.98+2*t))*cos(.43+2*t+3.1415*sin(2.98+2*t))-sin(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_2_per_frame6=t2=cos(1.9+.7*t)*cos(t)-.7*sin(1.9+.7*t)*sin(t);
wave_2_per_frame7=t3=cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))*(2-6.2831*sin(1.01+2*t))-2*sin(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_2_per_frame8=invFDmag=1/sqrt( t1*t1 + t2*t2 + t3*t3 );
wave_2_per_frame9=
wave_2_per_frame10=sdX=-4*cos(.43+2*t+3.1415*sin(2.98+2*t))*(sin(t)+3.1415*sin(2.98+3*t))-cos(t)*(5+25.132*cos(2.98+2*t)+39.4761*sqr(cos(2.98+2*t)))*sin( .43+2*t+3.1415*sin(2.98+2*t));
wave_2_per_frame11=sdY=-1.4*cos(t)*sin(1.9+.7*t)-1.49*cos(1.9+.7*t)*sin(t);
wave_2_per_frame12=sdZ=-12.566*cos(1.01+2*t)*cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))+8*cos(2*t+3.1415*cos(1.01+2*t))*(-1+3.1415*sin(1.01+2*t))*sin(1.54+2*t) - 4*cos(1.54+2*t)*(2-6.2831*sin(1.01+2*t)+9.869*sqr(sin(1.01+2*t)))*sin(2*t+3.1415*cos(1.01+2*t));
wave_2_per_frame13=
wave_2_per_frame14=t4=t2*sdZ-sdY*t3;
wave_2_per_frame15=t5=t3*sdX-t1*sdZ;
wave_2_per_frame16=t6=t1*sdY-t2*sdX;
wave_2_per_frame17=invSNmag=1/sqrt( t4*t4+t5*t5+t6*t6 );
wave_2_per_frame18=t4=t4*invSNmag;
wave_2_per_frame19=t5=t5*invSNmag;
wave_2_per_frame20=t6=t6*invSNmag;
wave_2_per_frame21=
wave_2_per_frame22=t1=t1*invFDmag;
wave_2_per_frame23=t2=t2*invFDmag;
wave_2_per_frame24=t3=t3*invFDmag;
wave_2_per_frame25=
wave_2_per_frame26=t7=t5*t3-t2*t6;
wave_2_per_frame27=t8=t6*t1-t4*t3;
wave_2_per_point1=sw=int(3*sample);
wave_2_per_point2=fnZ=t4*t2-t5*t1;
wave_2_per_point3=
wave_2_per_point4=p1=3*equal(sw,0)*sample;
wave_2_per_point5=p2=equal(sw,1)*3*(sample-.333);
wave_2_per_point6=p3=equal(sw,2)*3*(sample-.666);
wave_2_per_point7=
wave_2_per_point8=n1 = t2*fnZ-t8*t3;
wave_2_per_point9=n2 = -(t1*fnZ-t7*t3);
wave_2_per_point10=n3 = t1*t8-t2*t7;
wave_2_per_point11=
wave_2_per_point12=mx=p1*t7 +p2*n1 +p3*t1;
wave_2_per_point13=my=p1*t8 +p2*n2 +p3*t2;
wave_2_per_point14=mz=p1*fnZ+p2*n3 +p3*t3;
wave_2_per_point15=
wave_2_per_point16=x=.14+.05*mx;
wave_2_per_point17=y=.14+.05*my*1.25;
wave_2_per_point18=a=1-( above(sample,.33)*below(sample,.34) + above(sample,.66)*below(sample,.67));
wave_2_per_point19=
wave_2_per_point20=r=equal(sw,0);
wave_2_per_point21=g=equal(sw,1);
wave_2_per_point22=b=equal(sw,2);
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.500000
wavecode_3_r=1.000000
wavecode_3_g=1.000000
wavecode_3_b=1.000000
wavecode_3_a=1.000000
wave_3_per_frame1=speed=.015;
wave_3_per_frame2=length=.1;
wave_3_per_frame3=crosssectionrad=.07;
wave_3_per_frame4=
wave_3_per_frame5=t1=( speed*time-int(speed*time));
wave_3_per_frame6=t2= length;
wave_3_per_frame7=t3= crosssectionrad;
wave_3_per_frame8=
wave_3_per_frame9=t=t1*6.2831;
wave_3_per_frame10=t6=cos(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_3_per_frame11=t7=cos(1.9+.7*t)*sin(t);
wave_3_per_frame12=t8=cos(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_3_per_frame13=
wave_3_per_frame14=q1=2*cos(t)*(1+3.1415*cos(2.98+2*t))*cos(.43+2*t+3.1415*sin(2.98+2*t))-sin(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_3_per_frame15=q2=cos(1.9+.7*t)*cos(t)-.7*sin(1.9+.7*t)*sin(t);
wave_3_per_frame16=q3=cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))*(2-6.2831*sin(1.01+2*t))-2*sin(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_3_per_frame17=invFDmag=1/sqrt( q1*q1 + q2*q2 + q3*q3 );
wave_3_per_frame18=
wave_3_per_frame19=sdX=-4*cos(.43+2*t+3.1415*sin(2.98+2*t))*(sin(t)+3.1415*sin(2.98+3*t))-cos(t)*(5+25.132*cos(2.98+2*t)+39.4761*sqr(cos(2.98+2*t)))*sin( .43+2*t+3.1415*sin(2.98+2*t));
wave_3_per_frame20=sdY=-1.4*cos(t)*sin(1.9+.7*t)-1.49*cos(1.9+.7*t)*sin(t);
wave_3_per_frame21=sdZ=-12.566*cos(1.01+2*t)*cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))+8*cos(2*t+3.1415*cos(1.01+2*t))*(-1+3.1415*sin(1.01+2*t))*sin(1.54+2*t) - 4*cos(1.54+2*t)*(2-6.2831*sin(1.01+2*t)+9.869*sqr(sin(1.01+2*t)))*sin(2*t+3.1415*cos(1.01+2*t));
wave_3_per_frame22=
wave_3_per_frame23=q4=q2*sdZ-sdY*q3;
wave_3_per_frame24=q5=q3*sdX-q1*sdZ;
wave_3_per_frame25=q6=q1*sdY-q2*sdX;
wave_3_per_frame26=invSNmag=1/sqrt( q4*q4+q5*q5+q6*q6 );
wave_3_per_frame27=q4=q4*invSNmag;
wave_3_per_frame28=q5=q5*invSNmag;
wave_3_per_frame29=q6=q6*invSNmag;
wave_3_per_frame30=
wave_3_per_frame31=q1=q1*invFDmag;
wave_3_per_frame32=q2=q2*invFDmag;
wave_3_per_frame33=q3=q3*invFDmag;
wave_3_per_frame34=
wave_3_per_frame35=q7=q5*q3-q2*q6;
wave_3_per_frame36=q8=q6*q1-q4*q3;
wave_3_per_frame37=
wave_3_per_point1=t=(t1+(0+sample)*t2);
wave_3_per_point2=t=if(above(t,1),t-1,t);
wave_3_per_point3=t=t*6.2831;
wave_3_per_point4=
wave_3_per_point5=mx=cos(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_3_per_point6=my=cos(1.9+.7*t)*sin(t);
wave_3_per_point7=mz=cos(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_3_per_point8=
wave_3_per_point9=fdX=2*cos(t)*(1+3.1415*cos(2.98+2*t))*cos(.43+2*t+3.1415*sin(2.98+2*t))-sin(t)*sin(.43+2*t+3.1415*sin(2.98+2*t));
wave_3_per_point10=fdY=cos(1.9+.7*t)*cos(t)-.7*sin(1.9+.7*t)*sin(t);
wave_3_per_point11=fdZ=cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))*(2-6.2831*sin(1.01+2*t))-2*sin(1.54+2*t)*sin(2*t+3.1415*cos(1.01+2*t));
wave_3_per_point12=invFDmag=1/sqrt( fdX*fdX + fdY*fdY + fdZ*fdZ );
wave_3_per_point13=
wave_3_per_point14=sdX=-4*cos(.43+2*t+3.1415*sin(2.98+2*t))*(sin(t)+3.1415*sin(2.98+3*t))-cos(t)*(5+25.132*cos(2.98+2*t)+39.4761*sqr(cos(2.98+2*t)))*sin( .43+2*t+3.1415*sin(2.98+2*t));
wave_3_per_point15=sdY=-1.4*cos(t)*sin(1.9+.7*t)-1.49*cos(1.9+.7*t)*sin(t);
wave_3_per_point16=sdZ=-12.566*cos(1.01+2*t)*cos(1.54+2*t)*cos(2*t+3.1415*cos(1.01+2*t))+8*cos(2*t+3.1415*cos(1.01+2*t))*(-1+3.1415*sin(1.01+2*t))*sin(1.54+2*t) - 4*cos(1.54+2*t)*(2-6.2831*sin(1.01+2*t)+9.869*sqr(sin(1.01+2*t)))*sin(2*t+3.1415*cos(1.01+2*t));
wave_3_per_point17=
wave_3_per_point18=snX=fdY*sdZ-sdY*fdZ;
wave_3_per_point19=snY=fdZ*sdX-fdX*sdZ;
wave_3_per_point20=snZ=fdX*sdY-fdY*sdX;
wave_3_per_point21=invSNmag=1/sqrt( snX*snX+snY*snY+snZ*snZ );
wave_3_per_point22=snX=snX*invSNmag;
wave_3_per_point23=snY=snY*invSNmag;
wave_3_per_point24=snZ=snZ*invSNmag;
wave_3_per_point25=
wave_3_per_point26=fdX=fdX*invFDmag;
wave_3_per_point27=fdY=fdY*invFDmag;
wave_3_per_point28=fdZ=fdZ*invFDmag;
wave_3_per_point29=
wave_3_per_point30=fnX=snY*fdZ-fdY*snZ;
wave_3_per_point31=fnY=snZ*fdX-snX*fdZ;
wave_3_per_point32=fnZ=snX*fdY-snY*fdX;
wave_3_per_point33=
wave_3_per_point34=angl=6.2831*cos(628.3185*sample+2.54+40*sin(62.8318*sample+.56));
wave_3_per_point35=rr=t3*(.1+2*abs(sin(628.3185*sample+2.54+40*cos(62.8318*10*sample+.56))));
wave_3_per_point36=mx=mx+rr*cos(angl);
wave_3_per_point37=my=my+rr*(cos(angl)/sin(angl));
wave_3_per_point38=mz=mz+rr*sin(angl);
wave_3_per_point39=
wave_3_per_point40=qq9=q4*q2-q5*q1;
wave_3_per_point41=vx=(q7*mx+q8*my+qq9*mz-(t6*q7+t7*q8+t8*qq9));
wave_3_per_point42=vy=(q4*mx+q5*my+q6*mz-(t6*q4+t7*q5+t8*q6));
wave_3_per_point43=vw=q1*mx+q2*my+q3*mz-(t6*q1+t7*q2+t8*q3);
wave_3_per_point44=
wave_3_per_point45=ox=(vx/vw)*.15;
wave_3_per_point46=oy=(vy/vw)*.15*1.25;
wave_3_per_point47=x=.5-oy;
wave_3_per_point48=y=.5+ox*1.25;
wave_3_per_point49=a=above(vw,.01)*pow(2*(.5-min(vw,.5)),2);
shapecode_0_enabled=1
shapecode_0_sides=60
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_x=0.140000
shapecode_0_y=0.140000
shapecode_0_rad=0.133451
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.000000
shapecode_0_tex_zoom=1.000000
shapecode_0_r=0.000000
shapecode_0_g=0.000000
shapecode_0_b=0.000000
shapecode_0_a=1.000000
shapecode_0_r2=0.000000
shapecode_0_g2=0.000000
shapecode_0_b2=0.000000
shapecode_0_a2=1.000000
shapecode_0_border_r=1.000000
shapecode_0_border_g=1.000000
shapecode_0_border_b=1.000000
shapecode_0_border_a=1.000000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.500000
shapecode_1_y=0.500000
shapecode_1_rad=0.100000
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=1.000000
shapecode_1_r=1.000000
shapecode_1_g=0.000000
shapecode_1_b=0.000000
shapecode_1_a=1.000000
shapecode_1_r2=0.000000
shapecode_1_g2=1.000000
shapecode_1_b2=0.000000
shapecode_1_a2=0.000000
shapecode_1_border_r=1.000000
shapecode_1_border_g=1.000000
shapecode_1_border_b=1.000000
shapecode_1_border_a=0.100000
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_x=0.500000
shapecode_2_y=0.500000
shapecode_2_rad=0.100000
shapecode_2_ang=0.000000
shapecode_2_tex_ang=0.000000
shapecode_2_tex_zoom=1.000000
shapecode_2_r=1.000000
shapecode_2_g=0.000000
shapecode_2_b=0.000000
shapecode_2_a=1.000000
shapecode_2_r2=0.000000
shapecode_2_g2=1.000000
shapecode_2_b2=0.000000
shapecode_2_a2=0.000000
shapecode_2_border_r=1.000000
shapecode_2_border_g=1.000000
shapecode_2_border_b=1.000000
shapecode_2_border_a=0.100000
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.500000
shapecode_3_y=0.500000
shapecode_3_rad=0.100000
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.000000
shapecode_3_tex_zoom=1.000000
shapecode_3_r=1.000000
shapecode_3_g=0.000000
shapecode_3_b=0.000000
shapecode_3_a=1.000000
shapecode_3_r2=0.000000
shapecode_3_g2=1.000000
shapecode_3_b2=0.000000
shapecode_3_a2=0.000000
shapecode_3_border_r=1.000000
shapecode_3_border_g=1.000000
shapecode_3_border_b=1.000000
shapecode_3_border_a=0.100000
per_frame_1=decay=.81;
per_frame_2=
per_frame_3=dt=1/FPS;
per_frame_4=contvol=max(.4, (1-.6*dt)*contvol+.2*dt*(bass+mid+treb) );
per_frame_5=
per_frame_6=monitor=30*6.2831;
