MILKDROP_PRESET_VERSION=201
PSVERSION=3
PSVERSION_WARP=3
PSVERSION_COMP=3
[preset00]
fRating=3.000000
fGammaAdj=1.000
fDecay=1.000
fVideoEchoZoom=1.000
fVideoEchoAlpha=0.000
nVideoEchoOrientation=3
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=1
bSolarize=0
bInvert=0
fWaveAlpha=4.100
fWaveScale=1.157
fWaveSmoothing=0.630
fWaveParam=0.000
fModWaveAlphaStart=0.710
fModWaveAlphaEnd=1.300
fWarpAnimSpeed=1.000
fWarpScale=1.000
fZoomExponent=0.22705
fShader=1.000
zoom=1.01000
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.00000
sx=1.00000
sy=1.00000
wave_r=0.650
wave_g=0.650
wave_b=0.650
wave_x=0.500
wave_y=0.500
ob_size=0.000
ob_r=0.000
ob_g=0.000
ob_b=0.000
ob_a=0.000
ib_size=0.000
ib_r=0.000
ib_g=0.000
ib_b=0.000
ib_a=0.000
nMotionVectorsX=12.000
nMotionVectorsY=9.000
mv_dx=0.000
mv_dy=0.000
mv_l=0.900
mv_r=1.000
mv_g=1.000
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=0
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=1
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=0
wavecode_0_scaling=0.04575
wavecode_0_smoothing=0.00000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wavecode_1_enabled=0
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=1
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=0
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.00000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_1_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_1_per_frame3=vg = vol_avg*.1;
wave_1_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_1_per_point1=tm = q1;
wave_1_per_point2=sp = sample*6.28*8*6;
wave_1_per_point3=
wave_1_per_point4=vol = (value1+value2)*.5;
wave_1_per_point5=it = it*above(sample,0);
wave_1_per_point6=it = it + 1;
wave_1_per_point7=rad = .5 + vol + .02;
wave_1_per_point8=ra = rad*sin(sample*3.14);
wave_1_per_point9=ox = ra*sin(sp);
wave_1_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_1_per_point11=oz = ra*cos(sp);
wave_1_per_point12=
wave_1_per_point13=xang = tm*.132;
wave_1_per_point14=sxang = 0;
wave_1_per_point15=yang = tm*.153;
wave_1_per_point16=ayang = 0;
wave_1_per_point17=zang = tm*.110;
wave_1_per_point18=azang = 0;
wave_1_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_1_per_point20=fov = .5;
wave_1_per_point21=
wave_1_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_1_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_1_per_point24=ox = mx;
wave_1_per_point25=oy = my;
wave_1_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_1_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_1_per_point28=ox = mx;
wave_1_per_point29=oz = mz;
wave_1_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_1_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_1_per_point32=oy = my;
wave_1_per_point33=oz = mz;
wave_1_per_point34=
wave_1_per_point35=oz = oz - 2;
wave_1_per_point36=x = ox*fov/oz + 0.5;
wave_1_per_point37=x = (x-.5)*0.75 + 0.5;
wave_1_per_point38=y = oy*fov/oz + 0.5;
wave_1_per_point39=
wave_1_per_point40=r = 1;
wave_1_per_point41=g = .25+.25*sin(sp);
wave_1_per_point42=b = 0;
wave_1_per_point43=a = .5 + (oz+2)*.5;
wave_1_per_point44=a = a*below(z,2);
wave_1_per_point45=minrgb = min(r,min(g,b));
wave_1_per_point46=maxrgb = max(r,max(g,b));
wave_1_per_point47=l = (maxrgb-minrgb)*.5;
wave_1_per_point48=diff = maxrgb-minrgb;
wave_1_per_point49=sum = maxrgb+minrgb;
wave_1_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_1_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_1_per_point52=h = h*0.1666666;
wave_1_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_1_per_point54=
wave_1_per_point55=h = h + time*0.05*1.324 + .1;
wave_1_per_point56=h = h - int(h);
wave_1_per_point57=
wave_1_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_1_per_point59=tmpa = 2*l - tmpb;
wave_1_per_point60=hvr = h + .333333;
wave_1_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_1_per_point62=hvg = h;
wave_1_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_1_per_point64=hvb = h - .333333;
wave_1_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_1_per_point66=
wave_1_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_1_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_1_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
wavecode_2_enabled=0
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=1
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.00000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_2_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_2_per_frame3=vg = vol_avg*.1;
wave_2_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_2_per_point1=tm = q1;
wave_2_per_point2=sp = sample*6.28*8*6;
wave_2_per_point3=
wave_2_per_point4=vol = (value1+value2)*.5;
wave_2_per_point5=it = it*above(sample,0);
wave_2_per_point6=it = it + 1;
wave_2_per_point7=rad = .5 + vol + .01;
wave_2_per_point8=ra = rad*sin(sample*3.14);
wave_2_per_point9=ox = ra*sin(sp);
wave_2_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_2_per_point11=oz = ra*cos(sp);
wave_2_per_point12=
wave_2_per_point13=xang = tm*.132;
wave_2_per_point14=sxang = 0;
wave_2_per_point15=yang = tm*.153;
wave_2_per_point16=ayang = 0;
wave_2_per_point17=zang = tm*.110;
wave_2_per_point18=azang = 0;
wave_2_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_2_per_point20=fov = .5;
wave_2_per_point21=
wave_2_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_2_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_2_per_point24=ox = mx;
wave_2_per_point25=oy = my;
wave_2_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_2_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_2_per_point28=ox = mx;
wave_2_per_point29=oz = mz;
wave_2_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_2_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_2_per_point32=oy = my;
wave_2_per_point33=oz = mz;
wave_2_per_point34=
wave_2_per_point35=oz = oz - 2;
wave_2_per_point36=x = ox*fov/oz + 0.5;
wave_2_per_point37=x = (x-.5)*0.75 + 0.5;
wave_2_per_point38=y = oy*fov/oz + 0.5;
wave_2_per_point39=
wave_2_per_point40=r = 1;
wave_2_per_point41=g = .25+.25*sin(sp);
wave_2_per_point42=b = 0;
wave_2_per_point43=a = .5 + (oz+2)*.5;
wave_2_per_point44=a = a*below(z,2);
wave_2_per_point45=minrgb = min(r,min(g,b));
wave_2_per_point46=maxrgb = max(r,max(g,b));
wave_2_per_point47=l = (maxrgb-minrgb)*.5;
wave_2_per_point48=diff = maxrgb-minrgb;
wave_2_per_point49=sum = maxrgb+minrgb;
wave_2_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_2_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_2_per_point52=h = h*0.1666666;
wave_2_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_2_per_point54=
wave_2_per_point55=h = h + time*0.05*1.324 + .05;
wave_2_per_point56=h = h - int(h);
wave_2_per_point57=
wave_2_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_2_per_point59=tmpa = 2*l - tmpb;
wave_2_per_point60=hvr = h + .333333;
wave_2_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_2_per_point62=hvg = h;
wave_2_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_2_per_point64=hvb = h - .333333;
wave_2_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_2_per_point66=
wave_2_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_2_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_2_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
wavecode_3_enabled=0
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=0
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.00000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_per_frame1=vol = (bass_att + mid_att + treb_att)*.333333;
wave_3_per_frame2=vol_avg = .1*(vol_avg*9 + vol);
wave_3_per_frame3=vg = vol_avg*.1;
wave_3_per_frame4=t1 = if(above(vg,1.8),1.8,vg);
wave_3_per_point1=tm = q1;
wave_3_per_point2=sp = sample*6.28*8*6;
wave_3_per_point3=
wave_3_per_point4=vol = (value1+value2)*.5;
wave_3_per_point5=it = it*above(sample,0);
wave_3_per_point6=it = it + 1;
wave_3_per_point7=rad = .5 + vol;
wave_3_per_point8=ra = rad*sin(sample*3.14);
wave_3_per_point9=ox = ra*sin(sp);
wave_3_per_point10=oy = sin(sample*3.14-1.57)*rad;
wave_3_per_point11=oz = ra*cos(sp);
wave_3_per_point12=
wave_3_per_point13=xang = tm*.132;
wave_3_per_point14=sxang = 0;
wave_3_per_point15=yang = tm*.153;
wave_3_per_point16=ayang = 0;
wave_3_per_point17=zang = tm*.110;
wave_3_per_point18=azang = 0;
wave_3_per_point19=fov = 0.6 + 0.2*sin(tm);
wave_3_per_point20=fov = .5;
wave_3_per_point21=
wave_3_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_3_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_3_per_point24=ox = mx;
wave_3_per_point25=oy = my;
wave_3_per_point26=mx = ox*cos(yang) + oz*sin(yang);
wave_3_per_point27=mz = - ox*sin(yang) + oz*cos(yang);
wave_3_per_point28=ox = mx;
wave_3_per_point29=oz = mz;
wave_3_per_point30=my = oy*cos(xang) - oz*sin(xang);
wave_3_per_point31=mz = oy*sin(xang) + oz*cos(xang);
wave_3_per_point32=oy = my;
wave_3_per_point33=oz = mz;
wave_3_per_point34=
wave_3_per_point35=oz = oz - 2;
wave_3_per_point36=x = ox*fov/oz + 0.5;
wave_3_per_point37=x = (x-.5)*0.75 + 0.5;
wave_3_per_point38=y = oy*fov/oz + 0.5;
wave_3_per_point39=
wave_3_per_point40=r = 1;
wave_3_per_point41=g = .25+.25*sin(sp);
wave_3_per_point42=b = 0;
wave_3_per_point43=a = .5 + (oz+2)*.5;
wave_3_per_point44=a = a*below(z,2);
wave_3_per_point45=minrgb = min(r,min(g,b));
wave_3_per_point46=maxrgb = max(r,max(g,b));
wave_3_per_point47=l = (maxrgb-minrgb)*.5;
wave_3_per_point48=diff = maxrgb-minrgb;
wave_3_per_point49=sum = maxrgb+minrgb;
wave_3_per_point50=s = if(above(l,0.5),diff/(2-sum),diff/sum)*(1-equal(l,0));
wave_3_per_point51=h = if(equal(r,maxrgb),(g-b)/diff,if(equal(g,maxrgb),2+(b-r)/diff,4+(r-g)/diff));
wave_3_per_point52=h = h*0.1666666;
wave_3_per_point53=h = if(below(h,0),0,if(above(h,1),1,h));
wave_3_per_point54=
wave_3_per_point55=h = h + time*0.05*1.324;
wave_3_per_point56=h = h - int(h);
wave_3_per_point57=
wave_3_per_point58=tmpb = if(below(l,0.5),l*(1+s),(l+s)-(s*l));
wave_3_per_point59=tmpa = 2*l - tmpb;
wave_3_per_point60=hvr = h + .333333;
wave_3_per_point61=hvr = if(below(hvr,0),hvr+1,if(above(hvr,1),hvr-1,hvr));
wave_3_per_point62=hvg = h;
wave_3_per_point63=hvg = if(below(hvg,0),hvg+1,if(above(hvg,1),hvg-1,hvg));
wave_3_per_point64=hvb = h - .333333;
wave_3_per_point65=hvb = if(below(hvb,0),hvb+1,if(above(hvb,1),hvb-1,hvb));
wave_3_per_point66=
wave_3_per_point67=r = if(below(6*hvr,1),tmpa+(tmpb-tmpa)*6*hvr, if(below(2*hvr,1),tmpb, if(below(hvr*3,2),tmpa+(tmpb-tmpa)*(.666666-hvr)*6,tmpa)));
wave_3_per_point68=g = if(below(6*hvg,1),tmpa+(tmpb-tmpa)*6*hvg, if(below(2*hvg,1),tmpb, if(below(hvg*3,2),tmpa+(tmpb-tmpa)*(.666666-hvg)*6,tmpa)));
wave_3_per_point69=b = if(below(6*hvb,1),tmpa+(tmpb-tmpa)*6*hvb, if(below(2*hvb,1),tmpb, if(below(hvb*3,2),tmpa+(tmpb-tmpa)*(.666666-hvb)*6,tmpa)));
shapecode_0_enabled=1
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=1
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=0.44484
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=0.99999
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=1.000
shapecode_0_a=1.000
shapecode_0_r2=1.000
shapecode_0_g2=1.000
shapecode_0_b2=1.000
shapecode_0_a2=1.000
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=1.000
shape_0_per_frame1=bd=above(bass+treb+mid,6)+bd*.975;
shape_0_per_frame2=sides=cos(time*.02+(bd*.1))*20+20;
shape_0_per_frame3=border_r=sin(time*.331+.3)*.5+.5;
shape_0_per_frame4=border_g=sin(time*.559+.3)*.5+.5;
shape_0_per_frame5=border_b=sin(time*.772+.4)*.5+.5;
shape_0_per_frame6=
shapecode_1_enabled=1
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=1
shapecode_1_textured=1
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.44484
shapecode_1_ang=2.89026
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.22019
shapecode_1_r=1.000
shapecode_1_g=1.000
shapecode_1_b=1.000
shapecode_1_a=1.000
shapecode_1_r2=1.000
shapecode_1_g2=1.000
shapecode_1_b2=1.000
shapecode_1_a2=1.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=1.000
shape_1_per_frame1=bd=above(bass+treb+mid,6)+bd*.975;
shape_1_per_frame2=sides=cos(time*.02+(bd*.1))*20+20;
shape_1_per_frame3=r=sin(time*.331)*.5+.5;
shape_1_per_frame4=g=sin(time*.559)*.5+.5;
shape_1_per_frame5=b=sin(time*.772)*.5+.5;
shape_1_per_frame6=border_r=r;
shape_1_per_frame7=border_g=g;
shape_1_per_frame8=border_b=b;
shape_1_per_frame9=rad=sin(time*.4)*.2+.5;
shape_1_per_frame10=
shapecode_2_enabled=1
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=1
shapecode_2_num_inst=1
shapecode_2_x=0.900
shapecode_2_y=0.880
shapecode_2_rad=1.97884
shapecode_2_ang=0.62832
shapecode_2_tex_ang=6.28319
shapecode_2_tex_zoom=0.51341
shapecode_2_r=1.000
shapecode_2_g=1.000
shapecode_2_b=1.000
shapecode_2_a=1.000
shapecode_2_r2=1.000
shapecode_2_g2=1.000
shapecode_2_b2=1.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.000
shape_2_per_frame1=tex_ang=sin(time*.0001)*628+628;
shape_2_per_frame2=y=cos(time*.003)*.5+.5;
shapecode_3_enabled=0
shapecode_3_sides=100
shapecode_3_additive=1
shapecode_3_thickOutline=0
shapecode_3_textured=1
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.89269
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=1.000
shapecode_3_b=1.000
shapecode_3_a=0.070
shapecode_3_r2=0.000
shapecode_3_g2=0.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.000
per_frame_1=chng=sin(time*.5);
per_frame_2=cthr=.9999;
per_frame_3=mq21=if(above(chng,cthr),rand(3),mq21);
per_frame_4=mq22=if(above(chng,cthr),rand(3),mq22);
per_frame_5=mq23=if(above(chng,cthr),rand(3),mq23);
per_frame_6=mq24=if(above(chng,cthr),rand(2),mq24);
per_frame_7=mq25=if(above(chng,cthr),rand(2),mq25);
per_frame_8=mq26=if(above(chng,cthr),rand(2),mq26);
per_frame_9=mq27=if(above(chng,cthr),rand(1),mq27);
per_frame_10=mq28=if(above(chng,cthr),rand(1),mq28);
per_frame_11=mq29=if(above(chng,cthr),rand(1)*.3,mq29);
per_frame_12=mq31=if(above(chng,cthr),rand(1)*.3,mq31);
per_frame_13=monitor=chng;
per_frame_14=q21=mq21;q22=mq22;q23=mq23;q24=mq24;q25=mq25;q26=mq26;
per_frame_15=q27=mq27;q28=mq28;q29=mq29;q31=mq31;
per_frame_16=
per_frame_17=monitor=mq1;
per_frame_18=vol=bass+treb+mid;
per_frame_19=atime=atime+vol;
per_frame_20=q11=.4+sin(atime*.006        )*.4;
per_frame_21=q12=.4+cos(atime*.00613828348)*.4;
per_frame_22=q13=.4+sin(atime*.00598593455)*.4;
per_frame_23=monitor=q13;
per_frame_24=wave_r=wave_r+(0.6*sin(bass*2.500)+0.4*sin(time*0.70));
per_frame_25=wave_b=wave_b+(0.6*sin(treb*2.500)+0.4*sin(time*0.89));
per_frame_26=wave_g=wave_g+(0.6*sin(mid*2.500)+0.4*sin(time*0.74));
per_frame_27=q1=rot+0.005*sin(time*0.5);
per_pixel_1=rot=q1*2*rad*pow(0&(4+2*sin(rad*20+time))*.1,6);
warp_1=`sampler sampler_pw_noise_lq;
warp_2=`float3 color, mus, neu, ret1, noise, noise2;
warp_3=`float2 uv1, rs0, rs, uv2, uv3, dz, hor, ver;
warp_4=`float dx,dy,speed;
warp_5=`shader_body {
warp_6=`speed = .3;
warp_7=`uv1 = uv-float2(0.5,q5);
warp_8=`float z = 1/(uv1.y);
warp_9=`rs0.x = (uv1.x)*z;
warp_10=`rs0.y = z;
warp_11=`rs.x = rs0.x *1;
warp_12=`rs.y = rs0.y + time*speed;
warp_13=`
warp_14=`
warp_15=`//Kacheln
warp_16=`noise = lum(tex2D(sampler_pw_noise_lq,rs/63 ));
warp_17=`noise *= lum(tex2D(sampler_pw_noise_lq,rs/12 ))+.5;
warp_18=`noise *= saturate(10*noise - 8) * saturate(2/z);
warp_19=`noise2 = saturate(8* (lum(tex2D(sampler_pw_noise_lq,uv))-.5));
warp_20=`
warp_21=`speed *= 2;
warp_22=`float3 copy = + GetPixel(float2(uv.x,uv.y-.04*speed/z));
warp_23=`copy +=GetPixel(float2(uv.x,uv.y-.02*speed/z));
warp_24=`copy +=GetPixel(float2(uv.x,uv.y-.01*speed/z));
warp_25=`
warp_26=`ret = noise*1 + copy/3*(1+slow_roam_cos)/2*.99-.005;
warp_27=`float4 noise9 = tex3D(sampler_noisevol_hq, 
warp_28=`                      ((uv1.xyy*q27
warp_29=`                       )*texsize.xyy*texsize_noisevol_hq.zww
warp_30=`                      ).xyz*
warp_31=`                      float3(1,1,0)*0.05 + 
warp_32=`                      time*float3(0,0,1)*q29
warp_33=`                     );
warp_34=`if(ret.x> q21*q13         && ret.x<= q24*q11        )ret.y += (noise9).x*.5; 
warp_35=`if(ret.y> q22*q11         && ret.y<= q25*q12        )ret.z += (noise9).y*.5; 
warp_36=`if(ret.z> q23*q12         && ret.z<= q26*q13        )ret.x += (noise9).z*.5; 
warp_37=`
warp_38=`
warp_39=`}
comp_1=`shader_body
comp_2=`{
comp_3=`
comp_4=`
comp_5=`
comp_6=`float2 uva = uv;
comp_7=`float2 uvb = float2(1-uv.x,uv.y);
comp_8=`
comp_9=`ret = tex2D(sampler_main, uva).x + tex2D(sampler_main, uvb).x;
comp_10=`
comp_11=`float3 blurs = GetBlur1(uva).x + GetBlur3(uva).x;
comp_12=`blurs += GetBlur1(uvb).x + GetBlur3(uvb).x;
comp_13=`
comp_14=`
comp_15=`float2 uv3 = (uv-.5)*(1-GetBlur1(uv).zzz)+.5;
comp_16=`ret += saturate(pow(tex2D(sampler_main, uv3).zzz,.5)*(1-ret.x*2)),
comp_17=`ret += saturate(pow(GetBlur1(uv3).zzz,.5)*(1-ret.x*2)),
comp_18=`
comp_19=`
comp_20=`ret = lerp (
comp_21=`blurs,
comp_22=`ret,
comp_23=`pow(ret,1));
comp_24=`
comp_25=`ret = pow(ret,float3(5,1,.5));
comp_26=`
comp_27=`ret += pow(tex2D(sampler_main, float2(uv.x,1-uv.y)).yyy+tex2D(sampler_main, 1-uv).yyy,float3(.6,.95,5));
comp_28=`float4 noise9 = tex3D(sampler_noisevol_hq, 
comp_29=`                      ((uv3.xyy*q28
comp_30=`                       )*texsize.xyy*texsize_noisevol_hq.zww
comp_31=`                      ).xyz*
comp_32=`                      float3(1,1,0)*0.05 + 
comp_33=`                      time*float3(0,0,1)*q31
comp_34=`                     );
comp_35=`if(ret.x> q26*q13         && ret.x<= q23*q11        )ret.z -= (noise9).x*.5; 
comp_36=`if(ret.y> q25*q11         && ret.y<= q22*q12        )ret.x -= (noise9).y*.5; 
comp_37=`if(ret.z> q24*q12         && ret.z<= q21*q13        )ret.y -= (noise9).z*.5; 
comp_38=`
comp_39=`ret-=slow_roam_sin*roam_cos.zxy*.5;
comp_40=`
comp_41=`}
