MILKDROP_PRESET_VERSION=201
PSVERSION=3
PSVERSION_WARP=3
PSVERSION_COMP=3
[preset00]
fRating=4.000
fGammaAdj=1.980
fDecay=0.500
fVideoEchoZoom=1.000
fVideoEchoAlpha=0.500
nVideoEchoOrientation=3
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=1
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=1.286
fWaveSmoothing=0.630
fWaveParam=0.000
fModWaveAlphaStart=0.710
fModWaveAlphaEnd=1.300
fWarpAnimSpeed=0.626
fWarpScale=1.331
fZoomExponent=1.00001
fShader=0.000
zoom=0.99951
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.08925
sx=1.00000
sy=1.00000
wave_r=0.650
wave_g=0.650
wave_b=0.650
wave_x=0.500
wave_y=0.500
ob_size=0.005
ob_r=0.000
ob_g=0.000
ob_b=0.000
ob_a=1.000
ib_size=0.260
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=20.160
mv_dx=0.000
mv_dy=0.000
mv_l=0.400
mv_r=1.000
mv_g=0.400
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=1
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_init1=ma=.5;
wave_0_init2=my=.5;
wave_0_init3=md=0; //direction 0 1 2 3
wave_0_per_point1=oldmd=md;
wave_0_per_point2=md=(md+rand(4))%4;
wave_0_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_0_per_point4=
wave_0_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_0_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_0_per_point7=my=my+(equal(md,2)*.002*treb);
wave_0_per_point8=my=my-(equal(md,3)*.002*treb);
wave_0_per_point9=
wave_0_per_point10=mx=if(above(mx,.9),.5,mx);
wave_0_per_point11=mx=if(below(mx,.1),.5,mx);
wave_0_per_point12=my=if(above(my,.9),.5,my);
wave_0_per_point13=my=if(below(my,.1),.5,my);
wave_0_per_point14=
wave_0_per_point15=x=mx;
wave_0_per_point16=y=my;
wave_0_per_point17=a=bass*.1;
wave_0_per_point18=
wave_0_per_point19=r=bass*.5;
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=1
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_init1=mx=.5;
wave_1_init2=my=.5;
wave_1_init3=md=1;
wave_1_per_point1=oldmd=md;
wave_1_per_point2=md=(md+rand(4))%4;
wave_1_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_1_per_point4=
wave_1_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_1_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_1_per_point7=my=my+(equal(md,2)*.002*treb);
wave_1_per_point8=my=my-(equal(md,3)*.002*treb);
wave_1_per_point9=
wave_1_per_point10=mx=if(above(mx,.9),.5,mx);
wave_1_per_point11=mx=if(below(mx,.1),.5,mx);
wave_1_per_point12=my=if(above(my,.9),.5,my);
wave_1_per_point13=my=if(below(my,.1),.5,my);
wave_1_per_point14=
wave_1_per_point15=x=mx;
wave_1_per_point16=y=my;
wave_1_per_point17=a=bass*.1;
wave_1_per_point18=
wave_1_per_point19=g=treb*.5;
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=1
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_init1=mx=.5;
wave_2_init2=my=.5;
wave_2_init3=md=2;
wave_2_per_point1=oldmd=md;
wave_2_per_point2=md=(md+rand(4))%4;
wave_2_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_2_per_point4=
wave_2_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_2_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_2_per_point7=my=my+(equal(md,2)*.002*treb);
wave_2_per_point8=my=my-(equal(md,3)*.002*treb);
wave_2_per_point9=
wave_2_per_point10=mx=if(above(mx,.9),.5,mx);
wave_2_per_point11=mx=if(below(mx,.1),.5,mx);
wave_2_per_point12=my=if(above(my,.9),.5,my);
wave_2_per_point13=my=if(below(my,.1),.5,my);
wave_2_per_point14=
wave_2_per_point15=x=mx;
wave_2_per_point16=y=my;
wave_2_per_point17=a=bass*.1;
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_init1=mx=.5;
wave_3_init2=my=.4;
wave_3_init3=md=3;
wave_3_per_point1=oldmd=md;
wave_3_per_point2=md=(md+rand(4))%4;
wave_3_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_3_per_point4=
wave_3_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_3_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_3_per_point7=my=my+(equal(md,2)*.002*treb);
wave_3_per_point8=my=my-(equal(md,3)*.002*treb);
wave_3_per_point9=
wave_3_per_point10=mx=if(above(mx,.9),.5,mx);
wave_3_per_point11=mx=if(below(mx,.1),.5,mx);
wave_3_per_point12=my=if(above(my,.9),.5,my);
wave_3_per_point13=my=if(below(my,.1),.5,my);
wave_3_per_point14=
wave_3_per_point15=x=mx;
wave_3_per_point16=y=my;
wave_3_per_point17=a=bass*.1;
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=1.20321
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=1.22019
shapecode_0_r=1.000
shapecode_0_g=0.000
shapecode_0_b=0.000
shapecode_0_a=0.000
shapecode_0_r2=0.000
shapecode_0_g2=1.000
shapecode_0_b2=0.000
shapecode_0_a2=0.500
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.10000
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=0.000
shapecode_1_b=0.000
shapecode_1_a=1.000
shapecode_1_r2=0.000
shapecode_1_g2=1.000
shapecode_1_b2=0.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.100
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.10000
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=1.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.100
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.10000
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=1.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.100
per_frame_init_1=x1 = 0.5;
per_frame_init_2=y1 = 0.6;
per_frame_init_3=
per_frame_init_4=x2 = 0.9;
per_frame_init_5=y2 = 0.14;
per_frame_init_6=
per_frame_init_7=x3 = 0.5;
per_frame_init_8=y3 = 0.2;
per_frame_init_9=
per_frame_init_10=vr1 = 0.50001;
per_frame_init_11=vr2 = 0.0;
per_frame_init_12=vr3 = 0.0;
per_frame_init_13=
per_frame_init_14=vx1 = 0;
per_frame_init_15=vx2 = 0.4;
per_frame_init_16=vx3 = 0.9;
per_frame_1=zoom = 1;
per_frame_2=warp = .01;
per_frame_3=wave_a = 1;
per_frame_4=
per_frame_5=r = 0.04+ (bass_att+treb_att)*0.01;
per_frame_6=monitor = aspecty;
per_frame_7=vr = sin(vr1)*r;
per_frame_8=bounce = below(y1,r-(aspectx-1)*0.5);y1 = y1+vy1;vy1 = if(bounce, abs(vy1)*0.96 + (r-y1-(aspectx-1)*0.5)*0.1, vy1-0.0003*60/fps);
per_frame_9=vx1 = if(bounce, vx1 + (vr-vx1)*0.15, vx1);vr = if(bounce, vr + (vx1-vr)*0.85 , vr);vr1 = asin(vr/r);
per_frame_10=bounce = above(x1,1-r+(aspecty-1)*0.5);vx1 = if(bounce, - abs(vx1)*0.96 + (1-r-x1+(aspecty-1)*0.5)*0.1, vx1);
per_frame_11=vy1 = if(bounce, vy1 + (vr-vy1)*0.15, vy1);vr = if(bounce, vr + (vy1-vr)*0.85 , vr);vr1 = asin(vr/r);
per_frame_12=bounce = below(x1,r-(aspecty-1)*0.5);x1 = x1+vx1;vx1 = if(bounce, abs(vx1)*0.96 + (r-x1-(aspecty-1)*0.5)*0.1, vx1);
per_frame_13=vy1 = if(bounce, vy1 + (-vr-vy1)*0.15, vy1);vr = if(bounce, vr - (vy1+vr)*0.85 , vr);vr1 = asin(vr/r);
per_frame_14=
per_frame_15=vr = sin(vr2)*r;
per_frame_16=bounce = below(y2,r-(aspectx-1)*0.5);y2 = y2+vy2;vy2 = if(bounce, abs(vy2)*0.96 + (r-y2-(aspectx-1)*0.5)*0.1, vy2-0.0003*60/fps);
per_frame_17=vx2 = if(bounce, vx2 + (vr-vx2)*0.15, vx2);vr = if(bounce, vr + (vx2-vr)*0.85 , vr);vr2 = asin(vr/r);
per_frame_18=bounce = above(x2,1-r+(aspecty-1)*0.5);vx2 = if(bounce, - abs(vx2)*0.96 + (1-r-x2+(aspecty-1)*0.5)*0.1, vx2);
per_frame_19=vy2 = if(bounce, vy2 + (vr-vy2)*0.15, vy2);vr = if(bounce, vr + (vy2-vr)*0.85 , vr);vr2 = asin(vr/r);
per_frame_20=bounce = below(x2,r-(aspecty-1)*0.5);x2 = x2+vx2;vx2 = if(bounce, abs(vx2)*0.96 + (r-x2-(aspecty-1)*0.5)*0.1, vx2);
per_frame_21=vy2 = if(bounce, vy2 + (-vr-vy2)*0.15, vy2);vr = if(bounce, vr - (vy2+vr)*0.85 , vr);vr2 = asin(vr/r);
per_frame_22=
per_frame_23=vr = sin(vr3)*r;
per_frame_24=bounce = below(y3,r-(aspectx-1)*0.5);y3 = y3+vy3;vy3 = if(bounce, abs(vy3)*0.96 + (r-y3-(aspectx-1)*0.5)*0.1, vy3-0.0003*60/fps);
per_frame_25=vx3 = if(bounce, vx3 + (vr-vx3)*0.15, vx3);vr = if(bounce, vr + (vx3-vr)*0.85 , vr);vr3 = asin(vr/r);
per_frame_26=bounce = above(x3,1-r+(aspecty-1)*0.5);vx3 = if(bounce, - abs(vx3)*0.96 + (1-r-x3+(aspecty-1)*0.5)*0.1, vx3);
per_frame_27=vy3 = if(bounce, vy3 + (vr-vy3)*0.15, vy3);vr = if(bounce, vr + (vy3-vr)*0.85 , vr);vr3 = asin(vr/r);
per_frame_28=bounce = below(x3,r-(aspecty-1)*0.5);x3 = x3+vx3;vx3 = if(bounce, abs(vx3)*0.96 + (r-x3-(aspecty-1)*0.5)*0.1, vx3);
per_frame_29=vy3 = if(bounce, vy3 + (-vr-vy3)*0.15, vy3);vr = if(bounce, vr - (vy3+vr)*0.85 , vr);vr3 = asin(vr/r);
per_frame_30=
per_frame_31=bounce = below( sqrt( sqr(x1+vx1-x2-vx2) + sqr(y1+vy1-y2-vy2)), 2*r);
per_frame_32=bounce = bounce*below(sqrt( sqr(x1+vx1-x2-vx2) + sqr(y1+vy1-y2-vy2)),sqrt( sqr(x1-x2) + sqr(y1-y2)));
per_frame_33=ref_ang = atan2(x2-x1,y2-y1)+asin(1); // common tangent
per_frame_34=v1 = sqrt(vx1*vx1+vy1*vy1);v2 = sqrt(vx2*vx2+vy2*vy2);w1 = atan2(vx1,vy1);w2 = atan2(vx2,vy2);
per_frame_35=vr = sin(vr1)*r; v2r=sin(vr2)*r;
per_frame_36=vx1 = if(bounce,sin(ref_ang)*v1*cos(w1-ref_ang) + ((vr-v2r)-sin(ref_ang)*v1*cos(w1-ref_ang))*0.1
per_frame_37=              + sin(ref_ang+asin(1))*v2*cos(w2-ref_ang-asin(1)), vx1);
per_frame_38=vy1 = if(bounce,cos(ref_ang)*v1*cos(w1-ref_ang) + ((vr-v2r)-cos(ref_ang)*v1*cos(w1-ref_ang))*0.1
per_frame_39=              + cos(ref_ang+asin(1))*v2*cos(w2-ref_ang-asin(1)), vy1);
per_frame_40=vx2 = if(bounce,sin(ref_ang)*v2*cos(w2-ref_ang) + ((v2r-vr)-sin(ref_ang)*v2*cos(w2-ref_ang))*0.1
per_frame_41=              + sin(ref_ang+asin(1))*v1*cos(w1-ref_ang-asin(1)), vx2);
per_frame_42=vy2 = if(bounce,cos(ref_ang)*v2*cos(w2-ref_ang) + ((v2r-vr)-cos(ref_ang)*v2*cos(w2-ref_ang))*0.1
per_frame_43=              + cos(ref_ang+asin(1))*v1*cos(w1-ref_ang-asin(1)), vy2);
per_frame_44=vr = if(bounce, vr + (cos(w1-ref_ang)*(v1-v2)-vr)*0.9 , vr);vr1 = asin(vr/r);
per_frame_45=v2r = if(bounce, v2r + (cos(w2-ref_ang)*(v2-v1)-v2r)*0.9 , v2r);vr2 = asin(v2r/r);
per_frame_46=
per_frame_47=bounce = below( sqrt( sqr(x1+vx1-x3-vx3) + sqr(y1+vy1-y3-vy3)), 2*r);
per_frame_48=bounce = bounce*below(sqrt( sqr(x1+vx1-x3-vx3) + sqr(y1+vy1-y3-vy3)),sqrt( sqr(x1-x3) + sqr(y1-y3)));
per_frame_49=ref_ang = atan2(x3-x1,y3-y1)+asin(1); // common tangent
per_frame_50=v1 = sqrt(vx1*vx1+vy1*vy1);v2 = sqrt(vx3*vx3+vy3*vy3);w1 = atan2(vx1,vy1);w2 = atan2(vx3,vy3);
per_frame_51=vr = sin(vr1)*r; v2r=sin(vr3)*r;
per_frame_52=vx1 = if(bounce,sin(ref_ang)*v1*cos(w1-ref_ang) + ((vr-v2r)-sin(ref_ang)*v1*cos(w1-ref_ang))*0.1
per_frame_53=              + sin(ref_ang+asin(1))*v2*cos(w2-ref_ang-asin(1)), vx1);
per_frame_54=vy1 = if(bounce,cos(ref_ang)*v1*cos(w1-ref_ang) + ((vr-v2r)-cos(ref_ang)*v1*cos(w1-ref_ang))*0.1
per_frame_55=              + cos(ref_ang+asin(1))*v2*cos(w2-ref_ang-asin(1)), vy1);
per_frame_56=vx3 = if(bounce,sin(ref_ang)*v2*cos(w2-ref_ang) + ((v2r-vr)-sin(ref_ang)*v2*cos(w2-ref_ang))*0.1
per_frame_57=              + sin(ref_ang+asin(1))*v1*cos(w1-ref_ang-asin(1)), vx3);
per_frame_58=vy3 = if(bounce,cos(ref_ang)*v2*cos(w2-ref_ang) + ((v2r-vr)-cos(ref_ang)*v2*cos(w2-ref_ang))*0.1
per_frame_59=              + cos(ref_ang+asin(1))*v1*cos(w1-ref_ang-asin(1)), vy3);
per_frame_60=vr = if(bounce, vr + (cos(w1-ref_ang)*(v1-v2)-vr)*0.9 , vr);vr1 = asin(vr/r);
per_frame_61=v2r = if(bounce, v2r + (cos(w2-ref_ang)*(v2-v1)-v2r)*0.9 , v2r);vr3 = asin(v2r/r);
per_frame_62=
per_frame_63=bounce = below( sqrt( sqr(x3+vx3-x2-vx2) + sqr(y3+vy3-y2-vy2)), 2*r);
per_frame_64=bounce = bounce*below(sqrt( sqr(x2+vx2-x3-vx3) + sqr(y2+vy2-y3-vy3)),sqrt( sqr(x2-x3) + sqr(y2-y3)));
per_frame_65=ref_ang = atan2(x2-x3,y2-y3)+asin(1); // common tangent
per_frame_66=v1 = sqrt(vx3*vx3+vy3*vy3);v2 = sqrt(vx2*vx2+vy2*vy2);w1 = atan2(vx3,vy3);w2 = atan2(vx2,vy2);
per_frame_67=vr = sin(vr3)*r; v2r=sin(vr2)*r;
per_frame_68=vx3 = if(bounce,sin(ref_ang)*v1*cos(w1-ref_ang) + ((vr-v2r)-sin(ref_ang)*v1*cos(w1-ref_ang))*0.1
per_frame_69=              + sin(ref_ang+asin(1))*v2*cos(w2-ref_ang-asin(1)), vx3);
per_frame_70=vy3 = if(bounce,cos(ref_ang)*v1*cos(w1-ref_ang) + ((vr-v2r)-cos(ref_ang)*v1*cos(w1-ref_ang))*0.1
per_frame_71=              + cos(ref_ang+asin(1))*v2*cos(w2-ref_ang-asin(1)), vy3);
per_frame_72=vx2 = if(bounce,sin(ref_ang)*v2*cos(w2-ref_ang) + ((v2r-vr)-sin(ref_ang)*v2*cos(w2-ref_ang))*0.1
per_frame_73=              + sin(ref_ang+asin(1))*v1*cos(w1-ref_ang-asin(1)), vx2);
per_frame_74=vy2 = if(bounce,cos(ref_ang)*v2*cos(w2-ref_ang) + ((v2r-vr)-cos(ref_ang)*v2*cos(w2-ref_ang))*0.1
per_frame_75=              + cos(ref_ang+asin(1))*v1*cos(w1-ref_ang-asin(1)), vy2);
per_frame_76=vr = if(bounce, vr + (cos(w1-ref_ang)*(v1-v2)-vr)*0.9 , vr);vr3 = asin(vr/r);
per_frame_77=v2r = if(bounce, v2r + (cos(w2-ref_ang)*(v2-v1)-v2r)*0.9 , v2r);vr2 = asin(v2r/r);
per_frame_78=
per_frame_79=
per_frame_80=
per_frame_81=
per_frame_82=q1 = aspectx;
per_frame_83=q2 = aspecty;
per_frame_84=q3 = r*2;
per_frame_85=
per_frame_86=q4  = x1;  q5 = y1;  q6 = vr1;
per_frame_87=q7  = x2;  q8 = y2;  q9 = vr2;
per_frame_88=q10 = x3; q11 = y3; q12 = vr3;
per_frame_89=
per_frame_90=q13 = atan2( (x1+x2+x3)/3 - 0.5, (y1+y2+y3)/3-0.5);
per_frame_91=q14 = sigmoid(sqrt( sqr((x1+x2+x3)/3 - 0.5) + sqr((y1+y2+y3)/3-0.5) ),2)*0.2;
warp_1=`shader_body
warp_2=`{
warp_3=`    // sample previous frame
warp_4=`    ret = tex2D( sampler_fc_main, uv ).xyz;
warp_5=`    
warp_6=`    // motion blur by Geiss
warp_7=`    // 'v' points exactly one pixel, in the direction of motion
warp_8=`    float2 v = normalize(uv-uv_orig)*texsize.zw;
warp_9=`    float3 s;
warp_10=`    ret = max(ret, tex2D(sampler_main, uv+v)*0.97);
warp_11=`    ret = max(ret, tex2D(sampler_main, uv-v)*0.97);
warp_12=`    ret = max(ret, tex2D(sampler_main, uv+v*2)*0.90);
warp_13=`    ret = max(ret, tex2D(sampler_main, uv-v*2)*0.90);
warp_14=`
warp_15=`    // darken (decay) over time
warp_16=`    ret = (ret-0.005)*0.98; //or try: ret -= 0.004;
warp_17=`}
comp_1=`shader_body
comp_2=`{
comp_3=`float2 uv1 = (uv-0.5)*aspect.xy;
comp_4=`
comp_5=`float rad2 = length(uv1) + .05;
comp_6=`float rad1 = .1/rad2 ;
comp_7=`
comp_8=`float2 uv2 = float2 (ang/3.14, rad1*1.5);
comp_9=`uv2.y = uv2.y  +0.1*time;
comp_10=`uv2.x = uv2.x  +.02*time;
comp_11=`
comp_12=`float2 uv3 = float2 (ang/3.14, rad1);
comp_13=`uv3.y = uv3.y  + q30 ;
comp_14=`uv3.x = uv3.x  + time/32;
comp_15=`
comp_16=`
comp_17=`float3 crisp = GetPixel(uv2) + 2*GetPixel(uv3);
comp_18=`crisp += 2*GetBlur2(frac(uv2)) + 2*GetBlur2(frac(uv3));
comp_19=`
comp_20=`float3 lay1 = float3 (1,0,1)*uv.y*pow(1-rad,8);
comp_21=`
comp_22=`crisp = 3*crisp * pow(rad,1);
comp_23=`
comp_24=`float mask = saturate(1-4*rad);
comp_25=`
comp_26=`ret = crisp + lay1*mask + mask * GetPixel(uv);
comp_27=`
comp_28=`}