MILKDROP_PRESET_VERSION=201
PSVERSION=3
PSVERSION_WARP=3
PSVERSION_COMP=2
[preset00]
fRating=5.000000
fGammaAdj=1.700
fDecay=0.500
fVideoEchoZoom=0.594
fVideoEchoAlpha=0.500
nVideoEchoOrientation=2
nWaveMode=2
bAdditiveWaves=0
bWaveDots=1
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=1
bRedBlueStereo=0
bBrighten=1
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=0.012
fWaveSmoothing=0.900
fWaveParam=0.000
fModWaveAlphaStart=0.750
fModWaveAlphaEnd=0.950
fWarpAnimSpeed=1.000
fWarpScale=2.853
fZoomExponent=1.23219
fShader=0.000
zoom=1.08017
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.01678
sx=1.00000
sy=1.00000
wave_r=0.500
wave_g=0.400
wave_b=0.300
wave_x=0.500
wave_y=0.500
ob_size=0.000
ob_r=0.000
ob_g=0.000
ob_b=0.000
ob_a=0.000
ib_size=0.010
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=0.000
nMotionVectorsY=43.200
mv_dx=0.000
mv_dy=0.000
mv_l=1.000
mv_r=1.000
mv_g=0.910
mv_b=0.710
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=0
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=0.100
wavecode_0_g=1.000
wavecode_0_b=0.700
wavecode_0_a=1.000
wave_0_per_frame1=t1=sin(time)*0.5+0.5;
wave_0_per_frame2=t2=sin(time+2.1)*0.5+0.5;
wave_0_per_frame3=t3=sin(time+4.2)*0.5+0.5;
wave_0_per_frame4=
wave_0_per_frame5=t4=sin(time+1.1)*0.5+0.5;
wave_0_per_frame6=t5=sin(time+3.1)*0.5+0.5;
wave_0_per_frame7=t6=sin(time+5.2)*0.5+0.5;
wave_0_per_point1=n=sample*6.283;
wave_0_per_point2=phs=-sample * 0.2;
wave_0_per_point3=tm=q1 + phs;
wave_0_per_point4=
wave_0_per_point5=flip=flip+1;
wave_0_per_point6=flip=flip*below(flip,2);
wave_0_per_point7=
wave_0_per_point8=xp=0;
wave_0_per_point9=yp=flip*0.1 + (sin(tm)*0.5 + 0.5)*0.2;
wave_0_per_point10=zp=0;
wave_0_per_point11=
wave_0_per_point12=//wrist movement;
wave_0_per_point13=ang=sin(tm*2 )*0.5 +0.5;
wave_0_per_point14=
wave_0_per_point15=xq=xp;
wave_0_per_point16=sinang=sin(ang);cosang=cos(ang);
wave_0_per_point17=yq=yp*sinang + zp*cosang;
wave_0_per_point18=zq=yp*cosang - zp*sinang;
wave_0_per_point19=yq=yp;
wave_0_per_point20=zq=zp;
wave_0_per_point21=
wave_0_per_point22=ang=tm*8;
wave_0_per_point23=sinang=sin(ang);cosang=cos(ang);
wave_0_per_point24=xp=xq*sinang + yq*cosang;
wave_0_per_point25=yp=xq*cosang - yq*sinang;
wave_0_per_point26=zp=zq;
wave_0_per_point27=
wave_0_per_point28=//forearm movement;
wave_0_per_point29=zp=zp-0.3;
wave_0_per_point30=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_0_per_point31=sinang=sin(ang);cosang=cos(ang);
wave_0_per_point32=xq=xp;
wave_0_per_point33=yq=yp*sinang + zp*cosang;
wave_0_per_point34=zq=yp*cosang - zp*sinang;
wave_0_per_point35=
wave_0_per_point36=//upper arm twist
wave_0_per_point37=ang=-1.0 + cos(tm*3.1 + 0.5);
wave_0_per_point38=sinang=sin(ang);cosang=cos(ang);
wave_0_per_point39=xp=xq*sinang + yq*cosang;
wave_0_per_point40=yp=xq*cosang - yq*sinang;
wave_0_per_point41=zp=zq;
wave_0_per_point42=
wave_0_per_point43=//upper arm outward;
wave_0_per_point44=zp=zp-0.35;
wave_0_per_point45=ang=cos(tm*2.3)*1.75 - 1.05;
wave_0_per_point46=sinang=sin(ang);cosang=cos(ang);
wave_0_per_point47=xq=xp*sinang + zp*cosang;
wave_0_per_point48=yq=yp;
wave_0_per_point49=zq=xp*cosang - zp*sinang;
wave_0_per_point50=
wave_0_per_point51=//upper arm up down;
wave_0_per_point52=ang=cos(tm)*0.5 - 0.5;
wave_0_per_point53=sinang=sin(ang);cosang=cos(ang);
wave_0_per_point54=xp=xq;
wave_0_per_point55=yp=yq*cosang - zq*sinang;
wave_0_per_point56=zp=yq*sinang + zq*cosang;
wave_0_per_point57=
wave_0_per_point58=//xp=xq;yp=yq;zp=zq;
wave_0_per_point59=
wave_0_per_point60=
wave_0_per_point61=//project into screenspace and draw on screen
wave_0_per_point62=zp=zp+2;
wave_0_per_point63=xs=xp/zp;
wave_0_per_point64=ys=yp/zp;
wave_0_per_point65=
wave_0_per_point66=x=xs+0.5;
wave_0_per_point67=y=ys*1.3+0.5;
wave_0_per_point68=
wave_0_per_point69=
wave_0_per_point70=a=if( equal(q8,1) , (1-sample) , sample);
wave_0_per_point71=a=a*a;
wave_0_per_point72=
wave_0_per_point73=b=b+pow(1-sample,2)*0.3;
wave_0_per_point74=
wave_0_per_point75=
wave_0_per_point76=
wave_0_per_point77=r1=t1;
wave_0_per_point78=g1=t2;
wave_0_per_point79=b1=t3;
wave_0_per_point80=r2=t4;
wave_0_per_point81=g2=t5;
wave_0_per_point82=b2=t6;
wave_0_per_point83=
wave_0_per_point84=r=r1*flip + r2*(1-flip);
wave_0_per_point85=g=g1*flip + g2*(1-flip);
wave_0_per_point86=b=b1*flip + b2*(1-flip);
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=0
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=0.200
wavecode_1_g=1.000
wavecode_1_b=0.600
wavecode_1_a=1.000
wave_1_per_frame1=t1=sin(time)*0.5+0.5;
wave_1_per_frame2=t2=sin(time+2.1)*0.5+0.5;
wave_1_per_frame3=t3=sin(time+4.2)*0.5+0.5;
wave_1_per_frame4=
wave_1_per_frame5=t4=sin(time+1.1)*0.5+0.5;
wave_1_per_frame6=t5=sin(time+3.1)*0.5+0.5;
wave_1_per_frame7=t6=sin(time+5.2)*0.5+0.5;
wave_1_per_point1=n=sample*6.283;
wave_1_per_point2=phs=-sample * 0.2;
wave_1_per_point3=tm=q1 + phs;
wave_1_per_point4=
wave_1_per_point5=flip=flip+1;
wave_1_per_point6=flip=flip*below(flip,2);
wave_1_per_point7=
wave_1_per_point8=xp=0;
wave_1_per_point9=yp=flip*0.1 + (sin(tm)*0.5 + 0.5)*0.2 +0.1;
wave_1_per_point10=yp=-yp;
wave_1_per_point11=zp=0;
wave_1_per_point12=
wave_1_per_point13=//wrist movement;
wave_1_per_point14=ang=sin(tm*2)*0.5 +0.5;
wave_1_per_point15=
wave_1_per_point16=sinang=sin(ang);cosang=cos(ang);
wave_1_per_point17=xq=xp;
wave_1_per_point18=yq=yp*sinang + zp*cosang;
wave_1_per_point19=zq=yp*cosang - zp*sinang;
wave_1_per_point20=yq=yp;
wave_1_per_point21=zq=zp;
wave_1_per_point22=
wave_1_per_point23=ang=tm*8;
wave_1_per_point24=sinang=sin(ang);cosang=cos(ang);
wave_1_per_point25=xp=xq*sinang + yq*cosang;
wave_1_per_point26=yp=xq*cosang - yq*sinang;
wave_1_per_point27=zp=zq;
wave_1_per_point28=
wave_1_per_point29=//forearm movement;
wave_1_per_point30=zp=zp-0.3;
wave_1_per_point31=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_1_per_point32=sinang=sin(ang);cosang=cos(ang);
wave_1_per_point33=xq=xp;
wave_1_per_point34=yq=yp*sinang + zp*cosang;
wave_1_per_point35=zq=yp*cosang - zp*sinang;
wave_1_per_point36=
wave_1_per_point37=//upper arm twist
wave_1_per_point38=ang=-1.0 + cos(tm*3.1 + 0.5);
wave_1_per_point39=sinang=sin(ang);cosang=cos(ang);
wave_1_per_point40=xp=xq*sinang + yq*cosang;
wave_1_per_point41=yp=xq*cosang - yq*sinang;
wave_1_per_point42=zp=zq;
wave_1_per_point43=
wave_1_per_point44=//upper arm outward;
wave_1_per_point45=zp=zp-0.35;
wave_1_per_point46=ang=cos(tm*2.3)*1.75 - 1.05;
wave_1_per_point47=sinang=sin(ang);cosang=cos(ang);
wave_1_per_point48=xq=xp*sinang + zp*cosang;
wave_1_per_point49=yq=yp;
wave_1_per_point50=zq=xp*cosang - zp*sinang;
wave_1_per_point51=
wave_1_per_point52=//upper arm up down;
wave_1_per_point53=ang=cos(tm)*0.5 - 0.5;
wave_1_per_point54=sinang=sin(ang);cosang=cos(ang);
wave_1_per_point55=xp=xq;
wave_1_per_point56=yp=yq*cosang - zq*sinang;
wave_1_per_point57=zp=yq*sinang + zq*cosang;
wave_1_per_point58=
wave_1_per_point59=//xp=xq;yp=yq;zp=zq;
wave_1_per_point60=
wave_1_per_point61=
wave_1_per_point62=//project into screenspace and draw on screen
wave_1_per_point63=zp=zp+2;
wave_1_per_point64=xs=xp/zp;
wave_1_per_point65=ys=yp/zp;
wave_1_per_point66=
wave_1_per_point67=x=xs+0.5;
wave_1_per_point68=y=ys*1.3+0.5;
wave_1_per_point69=
wave_1_per_point70=
wave_1_per_point71=a=if( equal(q8,1) , (1-sample) , sample);
wave_1_per_point72=a=a*a;
wave_1_per_point73=
wave_1_per_point74=
wave_1_per_point75=b=b+pow(1-sample,2)*0.3;
wave_1_per_point76=
wave_1_per_point77=r1=t1;
wave_1_per_point78=g1=t2;
wave_1_per_point79=b1=t3;
wave_1_per_point80=r2=t4;
wave_1_per_point81=g2=t5;
wave_1_per_point82=b2=t6;
wave_1_per_point83=
wave_1_per_point84=r=r1*flip + r2*(1-flip);
wave_1_per_point85=g=g1*flip + g2*(1-flip);
wave_1_per_point86=b=b1*flip + b2*(1-flip);
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=1
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=0.600
wavecode_2_b=0.100
wavecode_2_a=1.000
wave_2_per_frame1=t1=sin(time)*0.5+0.5;
wave_2_per_frame2=t2=sin(time+2.1)*0.5+0.5;
wave_2_per_frame3=t3=sin(time+4.2)*0.5+0.5;
wave_2_per_frame4=
wave_2_per_frame5=t4=sin(time+1.1)*0.5+0.5;
wave_2_per_frame6=t5=sin(time+3.1)*0.5+0.5;
wave_2_per_frame7=t6=sin(time+5.2)*0.5+0.5;
wave_2_per_frame8=
wave_2_per_frame9=
wave_2_per_frame10=t8= int( sin(time*2)*2 + 3);
wave_2_per_point1=n=sample*6.283;
wave_2_per_point2=phs=-sample * 0.2;
wave_2_per_point3=tm=q1 + phs;
wave_2_per_point4=
wave_2_per_point5=flip=flip+1;
wave_2_per_point6=flip=flip*below(flip,2);
wave_2_per_point7=
wave_2_per_point8=xp=0;
wave_2_per_point9=yp=flip*0.1 + (sin(tm)*0.5 + 0.5)*0.2;
wave_2_per_point10=zp=0;
wave_2_per_point11=
wave_2_per_point12=//wrist movement;
wave_2_per_point13=ang=sin(tm*2)*0.5 +0.5;
wave_2_per_point14=
wave_2_per_point15=xq=xp;
wave_2_per_point16=sinang=sin(ang);cosang=cos(ang);
wave_2_per_point17=yq=yp*sinang + zp*cosang;
wave_2_per_point18=zq=yp*cosang - zp*sinang;
wave_2_per_point19=yq=yp;
wave_2_per_point20=zq=zp;
wave_2_per_point21=
wave_2_per_point22=ang=tm*8 + 1;
wave_2_per_point23=sinang=sin(ang);cosang=cos(ang);
wave_2_per_point24=xp=xq*sinang + yq*cosang;
wave_2_per_point25=yp=xq*cosang - yq*sinang;
wave_2_per_point26=zp=zq;
wave_2_per_point27=
wave_2_per_point28=//forearm movement;
wave_2_per_point29=zp=zp-0.3;
wave_2_per_point30=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_2_per_point31=sinang=sin(ang);cosang=cos(ang);
wave_2_per_point32=xq=xp;
wave_2_per_point33=yq=yp*sinang + zp*cosang;
wave_2_per_point34=zq=yp*cosang - zp*sinang;
wave_2_per_point35=
wave_2_per_point36=//upper arm twist
wave_2_per_point37=ang=-1.0 + cos(tm*3.1 + 0.5);
wave_2_per_point38=sinang=sin(ang);cosang=cos(ang);
wave_2_per_point39=xp=xq*sinang + yq*cosang;
wave_2_per_point40=yp=xq*cosang - yq*sinang;
wave_2_per_point41=zp=zq;
wave_2_per_point42=
wave_2_per_point43=//upper arm outward;
wave_2_per_point44=zp=zp-0.35;
wave_2_per_point45=ang=cos(tm*2.3)*1.75 - 1.05;
wave_2_per_point46=sinang=sin(ang);cosang=cos(ang);
wave_2_per_point47=xq=xp*sinang + zp*cosang;
wave_2_per_point48=yq=yp;
wave_2_per_point49=zq=xp*cosang - zp*sinang;
wave_2_per_point50=
wave_2_per_point51=//upper arm up down;
wave_2_per_point52=ang=cos(tm)*0.5 - 0.5;
wave_2_per_point53=sinang=sin(ang);cosang=cos(ang);
wave_2_per_point54=xp=xq;
wave_2_per_point55=yp=yq*cosang - zq*sinang;
wave_2_per_point56=zp=yq*sinang + zq*cosang;
wave_2_per_point57=
wave_2_per_point58=//xp=xq;yp=yq;zp=zq;
wave_2_per_point59=
wave_2_per_point60=
wave_2_per_point61=//project into screenspace and draw on screen
wave_2_per_point62=zp=zp+2;
wave_2_per_point63=xs=xp/zp;
wave_2_per_point64=ys=yp/zp;
wave_2_per_point65=
wave_2_per_point66=x=xs+0.5;
wave_2_per_point67=y=ys*1.3+0.5;
wave_2_per_point68=
wave_2_per_point69=a=if( equal(q8,1) , (1-sample) , sample);
wave_2_per_point70=
wave_2_per_point71=
wave_2_per_point72=a=a* above( sin(tm*128*t8) , 0 );
wave_2_per_point73=
wave_2_per_point74=
wave_2_per_point75=r=t4;
wave_2_per_point76=g=t5;
wave_2_per_point77=b=t6;
wave_2_per_point78=
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=0.300
wavecode_3_b=0.100
wavecode_3_a=1.000
wave_3_per_frame1=t1=sin(time)*0.5+0.5;
wave_3_per_frame2=t2=sin(time+2.1)*0.5+0.5;
wave_3_per_frame3=t3=sin(time+4.2)*0.5+0.5;
wave_3_per_frame4=
wave_3_per_frame5=t4=sin(time+1.1)*0.5+0.5;
wave_3_per_frame6=t5=sin(time+3.1)*0.5+0.5;
wave_3_per_frame7=t6=sin(time+5.2)*0.5+0.5;
wave_3_per_frame8=
wave_3_per_frame9=
wave_3_per_frame10=t8= int( sin(time*2)*2 + 3);
wave_3_per_point1=n=sample*6.283;
wave_3_per_point2=phs=-sample * 0.2;
wave_3_per_point3=tm=q1 + phs;
wave_3_per_point4=
wave_3_per_point5=flip=flip+1;
wave_3_per_point6=flip=flip*below(flip,2);
wave_3_per_point7=
wave_3_per_point8=xp=0;
wave_3_per_point9=yp=flip*0.1 + (sin(tm)*0.5 + 0.5)*0.2 +0.1;
wave_3_per_point10=yp=-yp;
wave_3_per_point11=zp=0;
wave_3_per_point12=
wave_3_per_point13=//wrist movement;
wave_3_per_point14=ang=sin(tm*2)*0.5 +0.5;
wave_3_per_point15=
wave_3_per_point16=sinang=sin(ang);cosang=cos(ang);
wave_3_per_point17=xq=xp;
wave_3_per_point18=yq=yp*sinang + zp*cosang;
wave_3_per_point19=zq=yp*cosang - zp*sinang;
wave_3_per_point20=yq=yp;
wave_3_per_point21=zq=zp;
wave_3_per_point22=
wave_3_per_point23=ang=tm*8+1;
wave_3_per_point24=sinang=sin(ang);cosang=cos(ang);
wave_3_per_point25=xp=xq*sinang + yq*cosang;
wave_3_per_point26=yp=xq*cosang - yq*sinang;
wave_3_per_point27=zp=zq;
wave_3_per_point28=
wave_3_per_point29=//forearm movement;
wave_3_per_point30=zp=zp-0.3;
wave_3_per_point31=ang=3.14 + sin(tm*2 - 0.5)*1.5;
wave_3_per_point32=sinang=sin(ang);cosang=cos(ang);
wave_3_per_point33=xq=xp;
wave_3_per_point34=yq=yp*sinang + zp*cosang;
wave_3_per_point35=zq=yp*cosang - zp*sinang;
wave_3_per_point36=
wave_3_per_point37=//upper arm twist
wave_3_per_point38=ang=-1.0 + cos(tm*3.1 + 0.5);
wave_3_per_point39=sinang=sin(ang);cosang=cos(ang);
wave_3_per_point40=xp=xq*sinang + yq*cosang;
wave_3_per_point41=yp=xq*cosang - yq*sinang;
wave_3_per_point42=zp=zq;
wave_3_per_point43=
wave_3_per_point44=//upper arm outward;
wave_3_per_point45=zp=zp-0.35;
wave_3_per_point46=ang=cos(tm*2.3)*1.75 - 1.05;
wave_3_per_point47=sinang=sin(ang);cosang=cos(ang);
wave_3_per_point48=xq=xp*sinang + zp*cosang;
wave_3_per_point49=yq=yp;
wave_3_per_point50=zq=xp*cosang - zp*sinang;
wave_3_per_point51=
wave_3_per_point52=//upper arm up down;
wave_3_per_point53=ang=cos(tm)*0.5 - 0.5;
wave_3_per_point54=sinang=sin(ang);cosang=cos(ang);
wave_3_per_point55=xp=xq;
wave_3_per_point56=yp=yq*cosang - zq*sinang;
wave_3_per_point57=zp=yq*sinang + zq*cosang;
wave_3_per_point58=
wave_3_per_point59=//xp=xq;yp=yq;zp=zq;
wave_3_per_point60=
wave_3_per_point61=
wave_3_per_point62=//project into screenspace and draw on screen
wave_3_per_point63=zp=zp+2;
wave_3_per_point64=xs=xp/zp;
wave_3_per_point65=ys=yp/zp;
wave_3_per_point66=
wave_3_per_point67=x=xs+0.5;
wave_3_per_point68=y=ys*1.3+0.5;
wave_3_per_point69=
wave_3_per_point70=
wave_3_per_point71=a=if( equal(q8,1) , (1-sample) , sample);
wave_3_per_point72=a=a*a;
wave_3_per_point73=
wave_3_per_point74=a=a* above( sin(tm*128*t8) , 0 );
wave_3_per_point75=
wave_3_per_point76=
wave_3_per_point77=r=t4;
wave_3_per_point78=g=t5;
wave_3_per_point79=b=t6;
shapecode_0_enabled=0
shapecode_0_sides=5
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=1.06779
shapecode_0_ang=0.75398
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=0.77977
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=1.000
shapecode_0_a=1.000
shapecode_0_r2=1.000
shapecode_0_g2=1.000
shapecode_0_b2=1.000
shapecode_0_a2=0.000
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shape_0_per_frame1=ang=sin(q1*0.15);
shape_0_per_frame2=x=sin(q1*0.5) * 0.05 + 0.5;
shape_0_per_frame3=y=cos(q1*0.63)* 0.05 + 0.5
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.10000
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=0.000
shapecode_1_b=0.000
shapecode_1_a=1.000
shapecode_1_r2=0.000
shapecode_1_g2=1.000
shapecode_1_b2=0.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.100
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.10000
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=1.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.100
shapecode_3_enabled=0
shapecode_3_sides=5
shapecode_3_additive=1
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.03809
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=1.000
shapecode_3_b=1.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=0.600
shapecode_3_b2=1.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.100
shape_3_per_frame1=tm=q1;
shape_3_per_frame2=
shape_3_per_frame3=xp=0;
shape_3_per_frame4=yp=0.1;
shape_3_per_frame5=zp=0;
shape_3_per_frame6=
shape_3_per_frame7=//wrist movement;
shape_3_per_frame8=ang=sin(tm*2 )*0.5 +0.5;
shape_3_per_frame9=
shape_3_per_frame10=xq=xp;
shape_3_per_frame11=sinang=sin(ang);cosang=cos(ang);
shape_3_per_frame12=yq=yp*sinang + zp*cosang;
shape_3_per_frame13=zq=yp*cosang - zp*sinang;
shape_3_per_frame14=yq=yp;
shape_3_per_frame15=zq=zp;
shape_3_per_frame16=
shape_3_per_frame17=ang=tm*8;
shape_3_per_frame18=sinang=sin(ang);cosang=cos(ang);
shape_3_per_frame19=xp=xq*sinang + yq*cosang;
shape_3_per_frame20=yp=xq*cosang - yq*sinang;
shape_3_per_frame21=zp=zq;
shape_3_per_frame22=
shape_3_per_frame23=//forearm movement;
shape_3_per_frame24=zp=zp-0.3;
shape_3_per_frame25=ang=3.14 + sin(tm*2 - 0.5)*1.5;
shape_3_per_frame26=sinang=sin(ang);cosang=cos(ang);
shape_3_per_frame27=xq=xp;
shape_3_per_frame28=yq=yp*sinang + zp*cosang;
shape_3_per_frame29=zq=yp*cosang - zp*sinang;
shape_3_per_frame30=
shape_3_per_frame31=//upper arm twist
shape_3_per_frame32=ang=-1.0 + cos(tm*3.1 + 0.5);
shape_3_per_frame33=sinang=sin(ang);cosang=cos(ang);
shape_3_per_frame34=xp=xq*sinang + yq*cosang;
shape_3_per_frame35=yp=xq*cosang - yq*sinang;
shape_3_per_frame36=zp=zq;
shape_3_per_frame37=
shape_3_per_frame38=//upper arm outward;
shape_3_per_frame39=zp=zp-0.35;
shape_3_per_frame40=ang=cos(tm*2.3)*1.75 - 1.05;
shape_3_per_frame41=sinang=sin(ang);cosang=cos(ang);
shape_3_per_frame42=xq=xp*sinang + zp*cosang;
shape_3_per_frame43=yq=yp;
shape_3_per_frame44=zq=xp*cosang - zp*sinang;
shape_3_per_frame45=
shape_3_per_frame46=//upper arm up down;
shape_3_per_frame47=ang=cos(tm)*0.5 - 0.5;
shape_3_per_frame48=sinang=sin(ang);cosang=cos(ang);
shape_3_per_frame49=xp=xq;
shape_3_per_frame50=yp=yq*cosang - zq*sinang;
shape_3_per_frame51=zp=yq*sinang + zq*cosang;
shape_3_per_frame52=
shape_3_per_frame53=//xp=xq;yp=yq;zp=zq;
shape_3_per_frame54=
shape_3_per_frame55=
shape_3_per_frame56=//project into screenspace and draw on screen
shape_3_per_frame57=zp=zp+2;
shape_3_per_frame58=xs=xp/zp;
shape_3_per_frame59=ys=yp/zp;
shape_3_per_frame60=
shape_3_per_frame61=x=xs+0.5;
shape_3_per_frame62=y=ys*1.3+0.5;
shape_3_per_frame63=
shape_3_per_frame64=
shape_3_per_frame65=
shape_3_per_frame66=
per_frame_1=wave_r = wave_r + 0.400*( 0.60*sin(0.933*time) + 0.40*sin(1.045*time) );
per_frame_2=wave_g = wave_g + 0.100*( 0.60*sin(0.900*time) + 0.40*sin(0.956*time) );
per_frame_3=wave_b = wave_b + 0.100*( 0.60*sin(0.910*time) + 0.40*sin(0.920*time) );
per_frame_4=mv_r = wave_r;
per_frame_5=mv_b = wave_b;
per_frame_6=mv_g = wave_g;
per_frame_7=q1 = 0.05*(pow(1+1.2*bass+0.4*bass_att+0.1*treb+0.1*treb_att+0.1*mid+0.1*mid_att,6)/fps);
per_frame_8=//q1 = 0.6*(bass+bass_att);
per_frame_9=mv_a = if(above(bass-1.2,1),1,bass-1.2);
per_frame_10=q2 = oldq2 + 0.05*(pow(1+1.2*treb+0.4*treb_att+0.1*treb+0.1*treb_att+0.1*mid+0.1*mid_att,6)/fps);
per_frame_11=
per_frame_12=//q2 = oldq2 +q1;
per_frame_13=oldq2 = q2 ;
per_frame_14=monitor = q2;
per_pixel_1=zoom = zoom + rad*0.1*q1;
per_pixel_2=
warp_1=`shader_body
warp_2=`{
warp_3=`  float2 uv2 = lerp(uv_orig, uv, 0.2);
warp_4=`
warp_5=`  // diffused version:
warp_6=`  float ss = 0.3;
warp_7=`  float3 blur = 0.25*(
warp_8=`    tex2D(sampler_main, uv2+ss*texsize.zw*float2( 1, 1)).xyz +
warp_9=`    tex2D(sampler_main, uv2+ss*texsize.zw*float2(-1, 1)).xyz +
warp_10=`    tex2D(sampler_main, uv2+ss*texsize.zw*float2( 1,-1)).xyz +
warp_11=`    tex2D(sampler_main, uv2+ss*texsize.zw*float2(-1,-1)).xyz
warp_12=`  );
warp_13=`
warp_14=`  // diffusion:  
warp_15=`  ret = tex2D(sampler_main,uv2);//blur;
warp_16=`
warp_17=`  float F2 = 0.035;
warp_18=`  float k2 = 0.060;
warp_19=`  float s = 0.025;
warp_20=`  float scale = 9;
warp_21=`
warp_22=`  // reaction:
warp_23=`  float3 z = ret;
warp_24=`  float uvv = ret.x*ret.y*ret.y;
warp_25=`  z.x += (-uvv + F2*(1-ret.x) + 0.0007)*scale;
warp_26=`  z.y += (uvv - (F2+k2)*ret.y)*scale;
warp_27=`  //z.x += s*(16-ret.x*ret.y);
warp_28=`  //z.y += s*(ret.x*ret.y - ret.y - ret.z);
warp_29=`  z.z -= 0.02;
warp_30=`
warp_31=`  // apply laplacian:
warp_32=`  z.x += (blur - GetPixel(uv2))*0.2*scale;
warp_33=`
warp_34=`  ret = z;  
warp_35=`  //ret *= 0.98 + 0.02*saturate( (0.75 - rad )*10 );
warp_36=`  //ret *= 0.99;
warp_37=`
warp_38=`  // add noise:
warp_39=`  ret.x += 0.09*(tex2d(sampler_noise_lq, uv*texsize.xy*texsize_noise_lq.zw + rand_frame.xy).xyz*2-1);
warp_40=`
warp_41=`  // darken (decay) over time
warp_42=`  //ret = (ret - 0.002)*0.99;
warp_43=`}
comp_1=`shader_body
comp_2=`{
comp_3=`    float rad_lq = rad * length(texsize.xy)*0.5;
comp_4=`    float ang_lq = ang;
comp_5=`    float2 uv_temp1 = (uv - 0.5) * texsize.xy;
comp_6=`    float rad_hq = length(uv_temp1);
comp_7=`    float ang_hq = atan2(-uv_temp1.y, uv_temp1.x);
comp_8=`
comp_9=`    float2 uv2 = (uv - 0.5);
comp_10=`    float rad2 = rad_lq*0.8;
comp_11=`    float ang2 = ang_lq * M_INV_PI_2 + rad_lq*0.000 + time*0.00;
comp_12=`
comp_13=`
comp_14=`        // FIN TYPE
comp_15=`        float fins = 6;
comp_16=`        ang2 = frac(ang2*fins)/fins;
comp_17=`              // ENABLE THIS TO MAKE THE FINS ALTERNATE: (seamless!)
comp_18=`              ang2 = abs(ang2 - 0.5/fins);
comp_19=`
comp_20=`
comp_21=`    ang2 *= M_PI_2;
comp_22=`    uv = 0.5 + rad2*float2(cos(ang2),sin(ang2))*texsize.zw;
comp_23=`
comp_24=`    ret = 1.4*pow(saturate(GetBlur1(uv))*((tex2D(sampler_pc_main,uv)-GetBlur3(uv))),0.5); //invert
comp_25=`}
