[preset00]
fRating=3.000000
fGammaAdj=1.000000
fDecay=0.980000
fVideoEchoZoom=0.999609
fVideoEchoAlpha=0.500000
nVideoEchoOrientation=3
nWaveMode=0
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=1
bTexWrap=1
bDarkenCenter=1
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=23.151701
fWaveScale=0.013210
fWaveSmoothing=0.270000
fWaveParam=0.100000
fModWaveAlphaStart=0.750000
fModWaveAlphaEnd=0.950000
fWarpAnimSpeed=5.995790
fWarpScale=1.331000
fZoomExponent=1.010000
fShader=0.000000
zoom=0.996546
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=1.000000
sy=1.000000
wave_r=1.000000
wave_g=0.400000
wave_b=0.200000
wave_x=0.500000
wave_y=0.500000
ob_size=0.010000
ob_r=0.000000
ob_g=0.900000
ob_b=0.200000
ob_a=1.000000
ib_size=0.000000
ib_r=0.300000
ib_g=0.300000
ib_b=0.700000
ib_a=1.000000
nMotionVectorsX=0.000000
nMotionVectorsY=48.000000
mv_dx=0.000000
mv_dy=0.000000
mv_l=5.000000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
per_frame_1=ob_r = 0.7 - 0.3*(0.5*sin(time*0.701)+ 0.3*cos(time*0.438));
per_frame_2=ob_g = 0.5- 0.4*sin(time*5.924);
per_frame_3=ob_b = 0.45 - 0.3*cos(time*0.816);
per_frame_4=warp =0;
per_frame_5=volume = 0.15*(bass_att+bass+mid+mid_att);
per_frame_6=beatrate = if(equal(beatrate,0),1,if(below(volume,0.01),1,beatrate));
per_frame_7=lastbeat = if(equal(lastbeat,0),time,lastbeat);
per_frame_8=meanbass_att = 0.1*(meanbass_att*9 + bass_att);
per_frame_9=peakbass_att = if(above(bass_att,peakbass_att),bass_att,peakbass_att);
per_frame_10=beat = if(above(volume,0.8),if(below(peakbass_att - bass_att, 0.05*peakbass_att),if(above(time - lastbeat,0.1+0.5*(beatrate-0.1)),1,0),0),0);
per_frame_11=beatrate = max(if(beat,if(below(time-lastbeat,2*beatrate),0.1*(beatrate*9 + time - lastbeat),beatrate),beatrate),0.1);
per_frame_12=peakbass_att = if(equal(beat,0),if(above(time - lastbeat,2*beatrate),peakbass_att*0.95,peakbass_att*0.995),bass_att);
per_frame_13=lastbeat = if(beat,time,lastbeat);
per_frame_14=peakbass_att = max(if(beat,bass_att,peakbass_att),1.1*meanbass_att);
per_frame_15=q5 = if(beat,0.1*rand(1000),oldq5);
per_frame_16=oldq5 = q5;
per_frame_17=q3 = if(beat,0.1*rand(1000),oldq3);
per_frame_18=oldq3 = q3;
per_frame_19=my_ib_size = 0.01+abs(0.01*sin(0.1*rand(1000)));
per_frame_20=ib_size = if(beat,my_ib_size,old_ib_size);
per_frame_21=old_ib_size = ib_size;
per_frame_22=ib_r = ib_r + 0.3*sin(time*0.934);
per_frame_23=ib_g = ib_g + 0.3*sin(time*1.547);
per_frame_24=ib_b = ib_b - 0.3*sin(time*1.431);
per_frame_25=wave_r=wave_r+waver*sin(if(Above(bass,bass_Att),sin(bass+bass_Att),sin(treb+Treb_att)))
per_frame_26=-waver*sin(if(above(mid,mid_att),sin(mid-mid_att),sin(bass-treb)))*rand(10)
per_frame_27=*sin(above(Bass,bass_att)+r1-r2);
per_frame_28=wave_b=wave_b+waveb*sin(if(Above(bass,bass_Att),sin(bass+bass_Att),sin(treb+bass)))
per_frame_29=-waveb*sin(if(above(treb,mid),sin(mid*bass),sin(bass*treb)))*rand(10)
per_frame_30=*sin(above(treb,treb_att))*rand(10)*Sin(above(bass,bass_Att)-r2-r3);
per_frame_31=wave_G=wave_g+waveg*sin(if(Above(bass,bass_Att),sin(bass+bass_Att),sin(mid-treb)))
per_frame_32=-waveg*sin(if(Above(mid,bass+1),sin(bass+treb_att),sin(mid-bass))-r3+r1);
per_pixel_1=box=abs(x*2-sin(q3))%2 + abs(y*2+sin(q5))%1.5-.2;
per_pixel_2=q1 = 4.05+(sin(x+0.237*time)-cos(y+0.513*time));
per_pixel_3=zoom = if(above(box,1),q1*.1,zoom*0.90)-.05*sin(above(bass,bass_Att));
per_pixel_4=rot = if(above(box,1),sin(0.885*time),0);
per_pixel_5=dx = if(above(box,1),sin(0.542*time),0);
per_pixel_6=dy= if(above(box,1),sin(0.581*time),0);
per_pixel_7=rot=if(above(bnot(1*bass),bnot(1*treb)),rot*sin(rad*sin(time)),-rot*sin(rad*cos(time))&rad);
per_frame_init_1=waver=time6*rand(10)*sin(rand(time1*sin(rand(5))))*sin(above(bass,bass_Att)-.2*sin
per_frame_init_2=(below(mid,mid_att)));
per_frame_init_3=waveb=time7*rand(10)*sin(rand(time2*sin(rand(10))))*sin(above(treb,treb_Att)-.5*sin
per_frame_init_4=(below(bass,bass_Att)));
per_frame_init_5=waveg=time8*rand(10)*sin(rand(time3*sin(rand(10))))*sin(above(mid,mid_att)+.2*sin
per_frame_init_6=(below(treb,treb_att)));
per_frame_init_7=time1=10*sin(time*.24);
per_frame_init_8=time2=10*sin(time*.14);
per_frame_init_9=time3=10*sin(time*.45);
per_frame_init_10=time6=1*sin(bass);
per_frame_init_11=time7=1*sin(treb);
per_frame_init_12=time8=1*sin(mid);
per_frame_init_13=r1=rand(3*rand(4));
per_frame_init_14=r2=rand(4*rand(5));
per_frame_init_15=r3=rand(5*rand(6));
