MILKDROP_PRESET_VERSION=201
PSVERSION=3
PSVERSION_WARP=2
PSVERSION_COMP=3
[preset00]
fRating=4.000000
fGammaAdj=1.000
fDecay=0.955
fVideoEchoZoom=0.997
fVideoEchoAlpha=0.500
nVideoEchoOrientation=1
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=1.286
fWaveSmoothing=0.630
fWaveParam=0.000
fModWaveAlphaStart=0.710
fModWaveAlphaEnd=1.300
fWarpAnimSpeed=30.965
fWarpScale=2.572
fZoomExponent=1.00000
fShader=1.000
zoom=1.00901
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.00054
sx=1.00000
sy=1.00000
wave_r=0.650
wave_g=0.650
wave_b=0.650
wave_x=0.500
wave_y=0.500
ob_size=0.010
ob_r=0.000
ob_g=0.000
ob_b=0.000
ob_a=0.000
ib_size=0.010
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=20.160
mv_dx=0.000
mv_dy=0.000
mv_l=0.400
mv_r=1.000
mv_g=0.400
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=1
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=1
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.50000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_init1=ma=.5;
wave_0_init2=my=.5;
wave_0_init3=md=0; //direction 0 1 2 3
wave_0_per_point1=oldmd=md;
wave_0_per_point2=md=(md+rand(4))%4;
wave_0_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_0_per_point4=
wave_0_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_0_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_0_per_point7=my=my+(equal(md,2)*.002*treb);
wave_0_per_point8=my=my-(equal(md,3)*.002*treb);
wave_0_per_point9=
wave_0_per_point10=mx=if(above(mx,.9),.5,mx);
wave_0_per_point11=mx=if(below(mx,.1),.5,mx);
wave_0_per_point12=my=if(above(my,.9),.5,my);
wave_0_per_point13=my=if(below(my,.1),.5,my);
wave_0_per_point14=
wave_0_per_point15=x=mx;
wave_0_per_point16=y=my;
wave_0_per_point17=a=bass*.1;
wave_0_per_point18=
wave_0_per_point19=r=bass*.5;
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=1
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.50000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_init1=mx=.5;
wave_1_init2=my=.5;
wave_1_init3=md=1;
wave_1_per_point1=oldmd=md;
wave_1_per_point2=md=(md+rand(4))%4;
wave_1_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_1_per_point4=
wave_1_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_1_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_1_per_point7=my=my+(equal(md,2)*.002*treb);
wave_1_per_point8=my=my-(equal(md,3)*.002*treb);
wave_1_per_point9=
wave_1_per_point10=mx=if(above(mx,.9),.5,mx);
wave_1_per_point11=mx=if(below(mx,.1),.5,mx);
wave_1_per_point12=my=if(above(my,.9),.5,my);
wave_1_per_point13=my=if(below(my,.1),.5,my);
wave_1_per_point14=
wave_1_per_point15=x=mx;
wave_1_per_point16=y=my;
wave_1_per_point17=a=bass*.1;
wave_1_per_point18=
wave_1_per_point19=g=treb*.5;
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=1
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.50000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_init1=mx=.5;
wave_2_init2=my=.5;
wave_2_init3=md=2;
wave_2_per_point1=oldmd=md;
wave_2_per_point2=md=(md+rand(4))%4;
wave_2_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_2_per_point4=
wave_2_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_2_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_2_per_point7=my=my+(equal(md,2)*.002*treb);
wave_2_per_point8=my=my-(equal(md,3)*.002*treb);
wave_2_per_point9=
wave_2_per_point10=mx=if(above(mx,.9),.5,mx);
wave_2_per_point11=mx=if(below(mx,.1),.5,mx);
wave_2_per_point12=my=if(above(my,.9),.5,my);
wave_2_per_point13=my=if(below(my,.1),.5,my);
wave_2_per_point14=
wave_2_per_point15=x=mx;
wave_2_per_point16=y=my;
wave_2_per_point17=a=bass*.1;
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=1.00000
wavecode_3_smoothing=0.50000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_init1=mx=.5;
wave_3_init2=my=.4;
wave_3_init3=md=3;
wave_3_per_point1=oldmd=md;
wave_3_per_point2=md=(md+rand(4))%4;
wave_3_per_point3=md=if(equal(md,oldmd),(md+1)%4,md);
wave_3_per_point4=
wave_3_per_point5=mx=mx+(equal(md,0)*.002*bass);
wave_3_per_point6=mx=mx-(equal(md,1)*.002*bass);
wave_3_per_point7=my=my+(equal(md,2)*.002*treb);
wave_3_per_point8=my=my-(equal(md,3)*.002*treb);
wave_3_per_point9=
wave_3_per_point10=mx=if(above(mx,.9),.5,mx);
wave_3_per_point11=mx=if(below(mx,.1),.5,mx);
wave_3_per_point12=my=if(above(my,.9),.5,my);
wave_3_per_point13=my=if(below(my,.1),.5,my);
wave_3_per_point14=
wave_3_per_point15=x=mx;
wave_3_per_point16=y=my;
wave_3_per_point17=a=bass*.1;
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=1
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=1.20321
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=1.22019
shapecode_0_r=1.000
shapecode_0_g=0.000
shapecode_0_b=0.000
shapecode_0_a=0.000
shapecode_0_r2=0.000
shapecode_0_g2=1.000
shapecode_0_b2=0.000
shapecode_0_a2=0.500
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shapecode_1_enabled=0
shapecode_1_sides=4
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.10000
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=0.000
shapecode_1_b=0.000
shapecode_1_a=1.000
shapecode_1_r2=0.000
shapecode_1_g2=1.000
shapecode_1_b2=0.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.100
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=0.10000
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=1.00000
shapecode_2_r=1.000
shapecode_2_g=0.000
shapecode_2_b=0.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=1.000
shapecode_2_b2=0.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.100
shapecode_3_enabled=0
shapecode_3_sides=4
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.10000
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=1.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=1.000
shapecode_3_b2=0.000
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.100
per_frame_1=wave_r = 0.85 + 0.25*sin(0.437*time+1);
per_frame_2=wave_g = 0.85 + 0.25*sin(0.544*time+2);
per_frame_3=wave_b = 0.85 + 0.25*sin(0.751*time+3);
per_frame_4=rot = rot + 0.010*( 0.60*sin(0.381*time) + 0.40*sin(0.579*time) );
per_frame_5=cx = cx + 0.210*( 0.60*sin(0.374*time) + 0.40*sin(0.294*time) );
per_frame_6=cy = cy + 0.210*( 0.60*sin(0.393*time) + 0.40*sin(0.223*time) );
per_frame_7=dx = dx + 0.003*( 0.60*sin(0.234*time) + 0.40*sin(0.277*time) );
per_frame_8=dy = dy + 0.003*( 0.60*sin(0.284*time) + 0.40*sin(0.247*time) );
per_frame_9=decay = decay - 0.01*equal(frame%6,0);
per_frame_10=dx = dx + dx_residual;
per_frame_11=dy = dy + dy_residual;
per_frame_12=bass_thresh = above(bass_att,bass_thresh)*2 + (1-above(bass_att,bass_thresh))*((bass_thresh-1.3)*0.96+1.3);
per_frame_13=dx_residual = equal(bass_thresh,2.13)*0.016*sin(time*7) + (1-equal(bass_thresh,2.13))*dx_residual;
per_frame_14=dy_residual = equal(bass_thresh,2.13)*0.012*sin(time*9) + (1-equal(bass_thresh,2.13))*dy_residual;
per_frame_15=wave_x = wave_x - dx_residual*7;
per_frame_16=wave_y = wave_y - dy_residual*7;
per_frame_17=wave_mystery = time*0.03;
per_frame_18=
per_frame_19=//zoom = zoom + 0.005*( 0.60*sin(0.1934*time+3) + 0.40*sin(0.307*time+9) );
per_frame_20=//zoom = zoom + max(0,bass_att-1.1)*0.2;
per_frame_21=//warp = warp + max(0,treb_att-1.1)*1.0;
per_frame_22=
per_frame_23=// this is a great way to respond to beats:
per_frame_24=// once you get one, let it decay at a constant rate!!
per_frame_25=rg = max(rg*0.77, 0.02 + 0.5*min(2,max(0,mid_att-1)*1.3));
per_frame_26=q9 = rg;
per_frame_27=
per_frame_28=zoom = zoom + q9*0.1;
warp_1=`shader_body
warp_2=`{
warp_3=`    // sample previous frame
warp_4=`    ret = tex2D( sampler_pw_main, uv ).xyz;
warp_5=`
warp_6=`    // darken over time
warp_7=`    ret -= 0.004;//*= 0.95; //or try: ret -= 0.004;
warp_8=`}
comp_1=`shader_body
comp_2=`{
comp_3=`    float rad_lq = rad * length(texsize.xy)*0.5;
comp_4=`    float ang_lq = ang;
comp_5=`    float2 uv_temp1 = (uv - 0.5) * texsize.xy;
comp_6=`    float rad_hq = length(uv_temp1);
comp_7=`    float ang_hq = atan2(-uv_temp1.y, uv_temp1.x);
comp_8=`
comp_9=`    float2 uv2 = (uv - 0.5);
comp_10=`    float rad2 = rad_lq*0.8;
comp_11=`    float ang2 = ang_lq * M_INV_PI_2 + rad_lq*0.000 + time*0.00;
comp_12=`
comp_13=`
comp_14=`        // FIN TYPE
comp_15=`        float fins = 6;
comp_16=`        ang2 = frac(ang2*fins)/fins;
comp_17=`              // ENABLE THIS TO MAKE THE FINS ALTERNATE: (seamless!)
comp_18=`              ang2 = abs(ang2 - 0.5/fins);
comp_19=`
comp_20=`
comp_21=`    ang2 *= M_PI_2;
comp_22=`    uv = 0.5 + rad2*float2(cos(ang2),sin(ang2))*texsize.zw;
comp_23=`
comp_24=`    ret = 1.4*pow(saturate(GetBlur1(uv))*((tex2D(sampler_pc_main,uv)-GetBlur3(uv))),0.5); //invert
comp_25=`}
