[preset00]
fRating=3.000000
fGammaAdj=1.000000
fDecay=0.750000
fVideoEchoZoom=1.000000
fVideoEchoAlpha=0.000000
nVideoEchoOrientation=0
nWaveMode=1
bAdditiveWaves=1
bWaveDots=0
bWaveThick=1
bModWaveAlphaByVolume=0
bMaximizeWaveColor=1
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=1
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=1.059149
fWaveScale=0.294621
fWaveSmoothing=0.900000
fWaveParam=-0.400000
fModWaveAlphaStart=0.500000
fModWaveAlphaEnd=1.000000
fWarpAnimSpeed=1.000000
fWarpScale=1.000000
fZoomExponent=22.479879
fShader=1.000000
zoom=0.999800
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=0.999900
sy=0.999800
wave_r=0.500000
wave_g=0.500000
wave_b=0.500000
wave_x=0.500000
wave_y=0.500000
ob_size=0.000000
ob_r=0.700000
ob_g=0.700000
ob_b=0.700000
ob_a=0.000000
ib_size=0.000000
ib_r=0.000000
ib_g=0.300000
ib_b=0.000000
ib_a=0.000000
nMotionVectorsX=2.560000
nMotionVectorsY=48.000000
mv_dx=0.360000
mv_dy=-0.800000
mv_l=5.000000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=1.000000
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=1
wavecode_0_scaling=1.000000
wavecode_0_smoothing=0.000000
wavecode_0_r=0.000000
wavecode_0_g=0.000000
wavecode_0_b=0.000000
wavecode_0_a=1.000000
wave_0_per_frame1=hue=.05*time;
wave_0_per_frame2=h=6*(hue-int(hue));
wave_0_per_frame3=sw1=below(h,1); sw2=(1-sw1)*below(h,2); sw3=(1-sw1)*(1-sw2)*below(h,3); sw4=(1-sw1)*(1-sw2)*(1-sw3)*below(h,4);
wave_0_per_frame4=sw6=above(h,5); sw5=(1-sw1)*(1-sw2)*(1-sw3)*(1-sw4)*(1-sw6);
wave_0_per_frame5=r=sw1+sw2*(2-h)+sw5*(h-4)+sw6;
wave_0_per_frame6=g=sw1*h+sw2+sw3+sw4*(4-h);
wave_0_per_frame7=b=sw3*(h-2)+sw4+sw5+sw6*(6-h);
wave_0_per_point1=s1=below(sample,.1667);
wave_0_per_point2=s2=(1-s1)*below(sample,.3333);
wave_0_per_point3=s3=above(sample,.3333)*below(sample,.5);
wave_0_per_point4=s4=above(sample,.5)*below(sample,.6667);
wave_0_per_point5=s5=above(sample,.6667)*below(sample,.8334);
wave_0_per_point6=s6=above(sample,.8334);
wave_0_per_point7=
wave_0_per_point8=// remap sample values
wave_0_per_point9=//sample = s1*sample;
wave_0_per_point10=sample=s2*(sample-.1667) +(1-s2)*sample;
wave_0_per_point11=sample=s3*(sample-.3333)+(1-s3)*sample;
wave_0_per_point12=sample=s4*(sample-.5)+(1-s4)*sample;
wave_0_per_point13=sample=s5*(sample-.6667)+(1-s5)*sample;
wave_0_per_point14=sample=s6*(sample-.8334)+(1-s6)*sample;
wave_0_per_point15=sample=sample*6;
wave_0_per_point16=
wave_0_per_point17=//s1
wave_0_per_point18=x=0;y=0;
wave_0_per_point19=x=x+s1*(.5+.3*cos(7*3.1415/6)+1.732*.3*sample*cos(3.1415/3));
wave_0_per_point20=y=y+s1*( .5+(.3*sin(7*3.1415/6)+1.732*.3*sample*sin(3.1415/3))*1.2 );
wave_0_per_point21=//s2
wave_0_per_point22=x=x+s2*(.5+.3*cos(3.1415/2)+1.732*.3*sample*cos(-3.1415/3));
wave_0_per_point23=y=y+s2*( .5+(.3*sin(3.1415/2)+1.732*.3*sample*sin(-3.1415/3))*1.2 );
wave_0_per_point24=//s3
wave_0_per_point25=x=x+s3*(.5+.3*cos(0-3.1415/6)+1.732*.3*sample*cos(-3.1415));
wave_0_per_point26=y=y+s3*(.5+(.3*sin(0-3.1415/6)+1.732*.3*sample*sin(-3.1415))*1.2 );
wave_0_per_point27=//s4
wave_0_per_point28=x=x+s4*(.5 + .05*cos(6.2831*sample+time));
wave_0_per_point29=y=y+s4*(.737 + .05*sin(6.2831*sample+time)*1.2);
wave_0_per_point30=//s5
wave_0_per_point31=x=x+s5*(.525 + .025*cos(3.1415*sample));
wave_0_per_point32=y=y+s5*(.737 + .025*sin(3.1415*sample)*1.2);
wave_0_per_point33=
wave_0_per_point34=//s6
wave_0_per_point35=x=x+s6*(.475 + .025*cos(-3.1415*sample));
wave_0_per_point36=y=y+s6*(.737 + .025*sin(-3.1415*sample)*1.2);
wave_0_per_point37=
wave_0_per_point38=ox=x-.5;
wave_0_per_point39=oy=(y-.737)/1.2;
wave_0_per_point40=
wave_0_per_point41=x=if(bor(s5,s6),(.5+ox*cos(time)-oy*sin(time)),x);
wave_0_per_point42=y=if(bor(s5,s6),(.737+(ox*sin(time)+oy*cos(time))*1.2),y);
wave_0_per_point43=
wave_0_per_point44=a=(1-s3)*a+s3*above(sample,.02)*below(sample,.98);
wave_0_per_point45=a=(1-s4)*a+s4*above(sample,.02)*below(sample,.98);
wave_0_per_point46=
wave_0_per_point47=distsqr=min(sqr(x-q7)+sqr(y-q8),q6)/q6;
wave_0_per_point48=a=a*(1-distsqr);
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=1
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.500000
wavecode_1_r=0.000000
wavecode_1_g=0.000000
wavecode_1_b=0.000000
wavecode_1_a=1.000000
wave_1_per_frame1=hue=.05*time;
wave_1_per_frame2=h=6*(hue-int(hue));
wave_1_per_frame3=sw1=below(h,1); sw2=(1-sw1)*below(h,2); sw3=(1-sw1)*(1-sw2)*below(h,3); sw4=(1-sw1)*(1-sw2)*(1-sw3)*below(h,4);
wave_1_per_frame4=sw6=above(h,5); sw5=(1-sw1)*(1-sw2)*(1-sw3)*(1-sw4)*(1-sw6);
wave_1_per_frame5=r=sw1+sw2*(2-h)+sw5*(h-4)+sw6;
wave_1_per_frame6=g=sw1*h+sw2+sw3+sw4*(4-h);
wave_1_per_frame7=b=sw3*(h-2)+sw4+sw5+sw6*(6-h);
wave_1_per_point1=s1=below(sample,.1667);
wave_1_per_point2=s2=(1-s1)*below(sample,.3333);
wave_1_per_point3=s3=above(sample,.3333)*below(sample,.5);
wave_1_per_point4=s4=above(sample,.5)*below(sample,.6667);
wave_1_per_point5=s5=above(sample,.6667)*below(sample,.8334);
wave_1_per_point6=s6=above(sample,.8334);
wave_1_per_point7=
wave_1_per_point8=// remap sample values
wave_1_per_point9=//sample = s1*sample;
wave_1_per_point10=sample=s2*(sample-.1667) +(1-s2)*sample;
wave_1_per_point11=sample=s3*(sample-.3333)+(1-s3)*sample;
wave_1_per_point12=sample=s4*(sample-.5)+(1-s4)*sample;
wave_1_per_point13=sample=s5*(sample-.6667)+(1-s5)*sample;
wave_1_per_point14=sample=s6*(sample-.8334)+(1-s6)*sample;
wave_1_per_point15=sample=sample*6;
wave_1_per_point16=
wave_1_per_point17=//s1
wave_1_per_point18=x=0;y=0;
wave_1_per_point19=x=x+s1*(.5+.115*cos(6.2831*sample+2*6.2831/5));
wave_1_per_point20=y=y+s1*(.61+(.055*sin(6.2831*sample+2*6.2831/5))*1.2);
wave_1_per_point21=
wave_1_per_point22=// s2
wave_1_per_point23=ycen=.01+.61+(.055*sin(6.2831*1.4))*1.2;
wave_1_per_point24=x=x+s2*(.5+.85*.09*cos(3.1415*(1+sample)));
wave_1_per_point25=y=y+s2*(ycen+(.85*.07*sin(3.1415*(1+sample)))*1.2);
wave_1_per_point26=
wave_1_per_point27=//s3
wave_1_per_point28=x=x+s3*(.54+.01*cos(6.2831*sample+2*6.2831/5));
wave_1_per_point29=y=y+s3*(ycen-.02+(.01*sin(6.2831*sample+2*6.2831/5))*1.2);
wave_1_per_point30=
wave_1_per_point31=//s4
wave_1_per_point32=ox=.525+.007*cos(6.2831*sample);
wave_1_per_point33=oy=.737+.007*sin(6.2831*sample);
wave_1_per_point34=x=x+s4*(.5+(ox-.5)*cos(time) - (oy-.737)*sin(time) );
wave_1_per_point35=y=y+s4*(.737+((ox-.5)*sin(time) + (oy-.737)*cos(time))*1.2 );
wave_1_per_point36=
wave_1_per_point37=//s5
wave_1_per_point38=ox=.475+.007*cos(6.2831*sample);
wave_1_per_point39=oy=.737+.007*sin(6.2831*sample);
wave_1_per_point40=x=x+s5*(.5+(ox-.5)*cos(time) - (oy-.737)*sin(time) );
wave_1_per_point41=y=y+s5*(.737+((ox-.5)*sin(time) + (oy-.737)*cos(time))*1.2 );
wave_1_per_point42=
wave_1_per_point43=//s6
wave_1_per_point44=x=x+s6*(.5+.3*cos(6.2831*sample));
wave_1_per_point45=y=y+s6*(.5+.3*sin(6.2831*sample)*1.2);
wave_1_per_point46=
wave_1_per_point47=a=(1-s1)*a+s1*above(sample,.01)*below(sample,.99);
wave_1_per_point48=a=(1-s2)*a+s2*above(sample,.01)*below(sample,.99);
wave_1_per_point49=a=(1-s3)*a+s3*above(sample,.01)*below(sample,.99);
wave_1_per_point50=a=(1-s4)*a+s4*above(sample,.01)*below(sample,.99);
wave_1_per_point51=a=(1-s5)*a+s5*above(sample,.01)*below(sample,.99);
wave_1_per_point52=a=(1-s6)*a+s6*above(sample,.0101);
wave_1_per_point53=
wave_1_per_point54=distsqr=min(sqr(x-q7)+sqr(y-q8),q6)/q6;
wave_1_per_point55=a=a*(1-distsqr);
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=0
wavecode_2_bAdditive=1
wavecode_2_scaling=1.000000
wavecode_2_smoothing=0.500000
wavecode_2_r=0.000000
wavecode_2_g=0.000000
wavecode_2_b=0.000000
wavecode_2_a=1.000000
wave_2_per_frame1=hue=.05*time;
wave_2_per_frame2=h=6*(hue-int(hue));
wave_2_per_frame3=sw1=below(h,1); sw2=(1-sw1)*below(h,2); sw3=(1-sw1)*(1-sw2)*below(h,3); sw4=(1-sw1)*(1-sw2)*(1-sw3)*below(h,4);
wave_2_per_frame4=sw6=above(h,5); sw5=(1-sw1)*(1-sw2)*(1-sw3)*(1-sw4)*(1-sw6);
wave_2_per_frame5=r=sw1+sw2*(2-h)+sw5*(h-4)+sw6;
wave_2_per_frame6=g=sw1*h+sw2+sw3+sw4*(4-h);
wave_2_per_frame7=b=sw3*(h-2)+sw4+sw5+sw6*(6-h);
wave_2_per_point1=s1=below(sample,.1);
wave_2_per_point2=s2=(1-s1)*below(sample,.2);
wave_2_per_point3=s3=above(sample,.2)*below(sample,.3);
wave_2_per_point4=s4=above(sample,.3)*below(sample,.4);
wave_2_per_point5=s5=above(sample,.4)*below(sample,.5);
wave_2_per_point6=s6=above(sample,.5)*below(sample,.6);
wave_2_per_point7=s7=above(sample,.6)*below(sample,.7);
wave_2_per_point8=s8=above(sample,.7)*below(sample,.8);
wave_2_per_point9=s9=above(sample,.8)*below(sample,.9);
wave_2_per_point10=s10=above(sample,.9);
wave_2_per_point11=
wave_2_per_point12=// remap sample values
wave_2_per_point13=//sample = s1*sample;
wave_2_per_point14=sample=s2*(sample-.1) +(1-s2)*sample;
wave_2_per_point15=sample=s3*(sample-.2)+(1-s3)*sample;
wave_2_per_point16=sample=s4*(sample-.3)+(1-s4)*sample;
wave_2_per_point17=sample=s5*(sample-.4)+(1-s5)*sample;
wave_2_per_point18=sample=s6*(sample-.5)+(1-s6)*sample;
wave_2_per_point19=sample=s7*(sample-.6)+(1-s7)*sample;
wave_2_per_point20=sample=s8*(sample-.7)+(1-s8)*sample;
wave_2_per_point21=sample=s9*(sample-.8)+(1-s9)*sample;
wave_2_per_point22=sample=s10*(sample-.9)+(1-s10)*sample;
wave_2_per_point23=sample=sample*10;
wave_2_per_point24=
wave_2_per_point25=//s1
wave_2_per_point26=x=0;y=0;an=.735;
wave_2_per_point27=// 6.2831*.75 = 3pi/4
wave_2_per_point28=x=x+s1*(.5+.115*cos(6.2831*an) +.193*sample*cos(6.2831*an) );
wave_2_per_point29=y=y+s1*(.61+(.055*sin(6.2831*an) +.193*sample*sin(6.2831*an))*1.2);
wave_2_per_point30=//s2
wave_2_per_point31=an=.765;
wave_2_per_point32=// 6.2831*.75 = 3pi/4
wave_2_per_point33=x=x+s2*(.5+.115*cos(6.2831*an) +.193*sample*cos(6.2831*an) );
wave_2_per_point34=y=y+s2*(.61+(.055*sin(6.2831*an) +.193*sample*sin(6.2831*an))*1.2);
wave_2_per_point35=//s3
wave_2_per_point36=an=.815;
wave_2_per_point37=// 6.2831*.75 = 3pi/4
wave_2_per_point38=x=x+s3*(.5+.115*cos(6.2831*an) +.213*sample*cos(6.2831*an) );
wave_2_per_point39=y=y+s3*(.61+(.055*sin(6.2831*an) +.213*sample*sin(6.2831*an))*1.2);
wave_2_per_point40=//s4
wave_2_per_point41=an=.845;
wave_2_per_point42=x=x+s4*(.5+.115*cos(6.2831*an) +.24*sample*cos(6.2831*an) );
wave_2_per_point43=y=y+s4*(.61+(.055*sin(6.2831*an) +.24*sample*sin(6.2831*an))*1.2);
wave_2_per_point44=//s5
wave_2_per_point45=an=.895;
wave_2_per_point46=x=x+s5*(.5+.115*cos(6.2831*an) +.11*sample*cos(6.2831*an) );
wave_2_per_point47=y=y+s5*(.61+(.055*sin(6.2831*an) +.11*sample*sin(6.2831*an))*1.2);
wave_2_per_point48=//s6
wave_2_per_point49=an=.925;
wave_2_per_point50=x=x+s6*(.5+.115*cos(6.2831*an) +.055*sample*cos(6.2831*an) );
wave_2_per_point51=y=y+s6*(.61+(.055*sin(6.2831*an) +.055*sample*sin(6.2831*an))*1.2);
wave_2_per_point52=//s7
wave_2_per_point53=an=.655;
wave_2_per_point54=x=x+s7*(.5+.115*cos(6.2831*an) +.24*sample*cos(6.2831*an) );
wave_2_per_point55=y=y+s7*(.61+(.055*sin(6.2831*an) +.24*sample*sin(6.2831*an))*1.2);
wave_2_per_point56=//s8
wave_2_per_point57=an=.685;
wave_2_per_point58=x=x+s8*(.5+.115*cos(6.2831*an) +.213*sample*cos(6.2831*an) );
wave_2_per_point59=y=y+s8*(.61+(.055*sin(6.2831*an) +.213*sample*sin(6.2831*an))*1.2);
wave_2_per_point60=//s9
wave_2_per_point61=an=.575;
wave_2_per_point62=x=x+s9*(.5+.115*cos(6.2831*an) +.053*sample*cos(6.2831*an) );
wave_2_per_point63=y=y+s9*(.61+(.055*sin(6.2831*an) +.053*sample*sin(6.2831*an))*1.2);
wave_2_per_point64=//s10
wave_2_per_point65=an=.605;
wave_2_per_point66=x=x+s10*(.5+.115*cos(6.2831*an) +.11*sample*cos(6.2831*an) );
wave_2_per_point67=y=y+s10*(.61+(.055*sin(6.2831*an) +.11*sample*sin(6.2831*an))*1.2);
wave_2_per_point68=
wave_2_per_point69=
wave_2_per_point70=a=(1-s1)*a+s1*above(sample,.02)*below(sample,.98);
wave_2_per_point71=a=(1-s2)*a+s2*above(sample,.02)*below(sample,.98);
wave_2_per_point72=a=(1-s3)*a+s3*above(sample,.02)*below(sample,.98);
wave_2_per_point73=a=(1-s4)*a+s4*above(sample,.02)*below(sample,.98);
wave_2_per_point74=a=(1-s5)*a+s5*above(sample,.02)*below(sample,.98);
wave_2_per_point75=a=(1-s6)*a+s6*above(sample,.02)*below(sample,.98);
wave_2_per_point76=a=(1-s7)*a+s7*above(sample,.02)*below(sample,.98);
wave_2_per_point77=a=(1-s8)*a+s8*above(sample,.02)*below(sample,.98);
wave_2_per_point78=a=(1-s9)*a+s9*above(sample,.02)*below(sample,.98);
wave_2_per_point79=a=(1-s10)*a+s10*above(sample,.02);
wave_2_per_point80=
wave_2_per_point81=distsqr=min(sqr(x-q7)+sqr(y-q8),q6)/q6;
wave_2_per_point82=a=a*(1-distsqr);
wavecode_3_enabled=0
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=1
wavecode_3_bDrawThick=0
wavecode_3_bAdditive=1
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.000000
wavecode_3_r=1.000000
wavecode_3_g=1.000000
wavecode_3_b=1.000000
wavecode_3_a=1.000000
shapecode_0_enabled=1
shapecode_0_sides=100
shapecode_0_additive=0
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_x=0.500000
shapecode_0_y=0.500000
shapecode_0_rad=0.100591
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.000000
shapecode_0_tex_zoom=0.990000
shapecode_0_r=1.000000
shapecode_0_g=1.000000
shapecode_0_b=1.000000
shapecode_0_a=1.000000
shapecode_0_r2=0.000000
shapecode_0_g2=0.000000
shapecode_0_b2=0.000000
shapecode_0_a2=0.000000
shapecode_0_border_r=0.000000
shapecode_0_border_g=0.000000
shapecode_0_border_b=0.000000
shapecode_0_border_a=0.000000
shape_0_per_frame1=x=.5;
shape_0_per_frame2=y=.1+q1*.8/6;
shape_0_per_frame3=
shape_0_per_frame4=rad=rad+.2*q5*below(q4,2);
shape_0_per_frame5=
shape_0_per_frame6=r=(1-q1)*.6+q1*0;
shape_0_per_frame7=g=(1-q1)*.3+q1*1;
shape_0_per_frame8=b=(1-q1)*.3+q1*0;
shape_0_per_frame9=
shape_0_per_frame10=textured=equal(frame%6,0)+equal(frame%6,3);
shape_0_per_frame11=additive=equal(frame%6,1)+equal(frame%6,4);
shape_0_per_frame12=
shape_0_per_frame13=textured=if( q5*below(q4,2),0,additive );
shape_0_per_frame14=addtive=if( q5*below(q4,2),1,additive );
shapecode_1_enabled=1
shapecode_1_sides=100
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_x=0.500000
shapecode_1_y=0.500000
shapecode_1_rad=0.100591
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=0.990000
shapecode_1_r=1.000000
shapecode_1_g=1.000000
shapecode_1_b=1.000000
shapecode_1_a=1.000000
shapecode_1_r2=0.000000
shapecode_1_g2=0.000000
shapecode_1_b2=0.000000
shapecode_1_a2=0.000000
shapecode_1_border_r=0.000000
shapecode_1_border_g=0.000000
shapecode_1_border_b=0.000000
shapecode_1_border_a=0.000000
shape_1_per_frame1=x=.5;
shape_1_per_frame2=y=.1+(q1+2)*.8/6;
shape_1_per_frame3=
shape_1_per_frame4=rad=rad+.2*q5*above(q4,1)*below(q4,4);
shape_1_per_frame5=
shape_1_per_frame6=r=(1-q1)*1+q1*1;
shape_1_per_frame7=g=(1-q1)*1+q1*1;
shape_1_per_frame8=b=(1-q1)*1+q1*0;
shape_1_per_frame9=
shape_1_per_frame10=textured=equal(frame%6,1)+equal(frame%6,4);
shape_1_per_frame11=additive=equal(frame%6,2)+equal(frame%6,5);
shape_1_per_frame12=
shape_1_per_frame13=textured=if( q5*above(q4,1)*below(q4,4),0,additive );
shape_1_per_frame14=addtive=if( q5*above(q4,1)*below(q4,4),1,additive );
shapecode_2_enabled=1
shapecode_2_sides=100
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=0
shapecode_2_x=0.500000
shapecode_2_y=0.500000
shapecode_2_rad=0.100591
shapecode_2_ang=0.000000
shapecode_2_tex_ang=0.000000
shapecode_2_tex_zoom=0.989996
shapecode_2_r=1.000000
shapecode_2_g=1.000000
shapecode_2_b=1.000000
shapecode_2_a=1.000000
shapecode_2_r2=0.000000
shapecode_2_g2=0.000000
shapecode_2_b2=0.000000
shapecode_2_a2=0.000000
shapecode_2_border_r=0.000000
shapecode_2_border_g=0.000000
shapecode_2_border_b=0.000000
shapecode_2_border_a=0.000000
shape_2_per_frame1=x=.5;
shape_2_per_frame2=y=.1+(q1+4)*.8/6;
shape_2_per_frame3=
shape_2_per_frame4=rad=rad+.2*q5*above(q4,4);
shape_2_per_frame5=
shape_2_per_frame6=r=(1-q1)*1+q1*0;
shape_2_per_frame7=g=(1-q1)*.3+q1*0;
shape_2_per_frame8=b=(1-q1)*.1+q1*1;
shape_2_per_frame9=
shape_2_per_frame10=textured=equal(frame%6,2)+equal(frame%6,5);
shape_2_per_frame11=additive=equal(frame%6,3)+equal(frame%6,0);
shape_2_per_frame12=
shape_2_per_frame13=textured=if( q5*above(q4,4),0,additive );
shape_2_per_frame14=addtive=if( q5*above(q4,4),1,additive );
shapecode_3_enabled=1
shapecode_3_sides=100
shapecode_3_additive=1
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.500000
shapecode_3_y=0.500000
shapecode_3_rad=0.149766
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.000000
shapecode_3_tex_zoom=0.990000
shapecode_3_r=1.000000
shapecode_3_g=1.000000
shapecode_3_b=1.000000
shapecode_3_a=1.000000
shapecode_3_r2=1.000000
shapecode_3_g2=1.000000
shapecode_3_b2=1.000000
shapecode_3_a2=0.000000
shapecode_3_border_r=0.000000
shapecode_3_border_g=0.000000
shapecode_3_border_b=0.000000
shapecode_3_border_a=0.000000
shape_3_per_frame1=x=.5;
shape_3_per_frame2=y=.1+(q1+6)*.8/6;
shape_3_per_frame3=a=1-q1;
shape_3_per_frame4=r=(1-q1)*1+q1*0;
shape_3_per_frame5=g=(1-q1)*1+q1*1;
shape_3_per_frame6=b=(1-q1)*1+q1*0;
per_frame_1=// -------------------------------- beat detection code ----------------------------------
per_frame_2=sure=if(equal(sure,0),.75,sure);
per_frame_3=interval=if(equal(interval,0),.7*FPS,interval);
per_frame_4=avginterval=if(equal(avginterval,0),.7*FPS,avginterval);
per_frame_5=lockinterval=if(equal(lockinterval,0),.7*FPS,lockinterval );
per_frame_6=lastbeat=if(equal(lastbeat,0),frame-FPS,lastbeat);
per_frame_7=dbass=(bass-pbass)*FPS;
per_frame_8=beat=below(dbass,0)*above(pdbass,0)*above(bass,.95*avgbass)*above(frame-lastbeat,FPS/3);
per_frame_9=sure=if(beat*below(abs(frame-(interval+lastbeat)),FPS/5),
per_frame_10=min(.095+sure,1),beat*(sure-.095)+(1-beat)*sure*.9996);
per_frame_11=sure=max(.5,sure);
per_frame_12=avgbass=.995*avgbass+.005*bass;
per_frame_13=maxdbass=max(maxdbass*.999,dbass);
per_frame_14=maxdbass=min(200,maxdbass);
per_frame_15=maxdbass=max(.02,maxdbass);
per_frame_16=interval=if(beat*below(frame-lastbeat,1.8*interval), ((frame-lastbeat)*.25+.75*interval),interval);
per_frame_17=lastbeat=if((1-force)*beat+equal(lastbeat+interval,frame),frame,lastbeat);
per_frame_18=avginterval=if(beat,.9*avginterval+.1*interval, avginterval);
per_frame_19=lockinterval=if(beat,.9*lockinterval+.1*avginterval,lockinterval);
per_frame_20=pbass=bass;
per_frame_21=pdbass=dbass;
per_frame_22=bpm=60*FPS*.3333*( ((2*(1-sure))/interval)+((2*sure)/avginterval)+(1/lockinterval) );
per_frame_23=phase=min( (frame-lastbeat)/(.333*(2*sure*avginterval+2*(1-sure)*interval+lockinterval)), 1 );
per_frame_24=beat=if(equal(phase,0),1,beat);
per_frame_25=interval=min(interval,.7*FPS);
per_frame_26=avginterval=min(avginterval,.7*FPS);
per_frame_27=lockinterval=min(lockinterval,.7*FPS);
per_frame_28=// ----------------------------------------------------------------------------------------------
per_frame_29=
per_frame_30=warp=0;zoom=1;
per_frame_31=decay=.99;
per_frame_32=cvol=((bass+mid+treb)*.3333)*.007 + .993*cvol;
per_frame_33=wave_y=.05+.9*abs(sin(time*.1));
per_frame_34=
per_frame_35=mv_dy=rand(100)/1000;
per_frame_36=
per_frame_37=q1=frame%2;
per_frame_38=
per_frame_39=q2=.1+(frame%7)*.8/6;
per_frame_40=prev=beat*((prev+1+rand(6))%6)+(1-beat)*prev;
per_frame_41=q3=phase;
per_frame_42=q4=prev;
per_frame_43=q5=beat;
per_frame_44=q6=.05;
per_frame_45=q7=.5+.3*cos(.8*time+3.1415*sin(time+2.04));
per_frame_46=q8=.5+.3*sin(.4*time+3.1415*cos(time+.32));
per_pixel_1=x=.5-x;
per_pixel_2=y=1-y-q2;
per_pixel_3=
per_pixel_4=myAng = atan2(y,x);
per_pixel_5=myDist=sqrt(x*x+y*y);
per_pixel_6=
per_pixel_7=myFactor=below(myDist,.3)*abs(log(MyDist))*.005;
per_pixel_8=dx=dx-.25*cos(MyAng)*myFactor;
per_pixel_9=dy=dy-.25*sin(MyAng)*myFactor;
per_pixel_10=
per_pixel_11=zoom = zoom + .1*sqr(abs(x));
per_pixel_12=warp=5*sqr(x);
