MILKDROP_PRESET_VERSION=201
PSVERSION=2
PSVERSION_WARP=0
PSVERSION_COMP=2
[preset00]
fRating=5.000000
fGammaAdj=1.900
fDecay=0.980
fVideoEchoZoom=1.169
fVideoEchoAlpha=0.000
nVideoEchoOrientation=0
nWaveMode=6
bAdditiveWaves=0
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.001
fWaveScale=0.010
fWaveSmoothing=0.900
fWaveParam=0.000
fModWaveAlphaStart=0.750
fModWaveAlphaEnd=0.950
fWarpAnimSpeed=1.000
fWarpScale=1.331
fZoomExponent=1.00000
fShader=0.000
zoom=0.99951
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.01000
sx=1.00000
sy=1.00000
wave_r=1.000
wave_g=0.000
wave_b=0.000
wave_x=0.500
wave_y=0.500
ob_size=0.500
ob_r=0.010
ob_g=0.000
ob_b=0.000
ob_a=0.000
ib_size=0.260
ib_r=0.250
ib_g=0.250
ib_b=0.250
ib_a=0.000
nMotionVectorsX=64.000
nMotionVectorsY=48.000
mv_dx=0.000
mv_dy=0.000
mv_l=0.050
mv_r=0.000
mv_g=0.700
mv_b=1.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=0
wavecode_0_bAdditive=0
wavecode_0_scaling=1.00000
wavecode_0_smoothing=0.00000
wavecode_0_r=1.000
wavecode_0_g=1.000
wavecode_0_b=1.000
wavecode_0_a=1.000
wave_0_per_frame1=t1=q1;
wave_0_per_frame2=
wave_0_per_frame3=t7=.0;
wave_0_per_frame4=t8=.45;
wave_0_per_frame5=
wave_0_per_frame6=ddx=.25*cos(5.7119*t1)+2.5963*t1*sin(5.7119*t1);
wave_0_per_frame7=ddy=.3125*sin(5.7119*t1)-3.2453*t1*cos(5.7119*t1);
wave_0_per_frame8=ddtan=atan2(ddy,ddx);
wave_0_per_frame9=t2=-ddtan;
wave_0_per_frame10=
wave_0_per_frame11=val1=((-.5*cos(5.7119*t1))*cos(t2)-(-.625*sin(5.7119*t1))*sin(t2));
wave_0_per_frame12=val2=((-.5*cos(5.7119*t1))*sin(t2)+(-.625*sin(5.7119*t1))*cos(t2));
wave_0_per_frame13=
wave_0_per_frame14=t6=-sign(t1);
wave_0_per_frame15=t7=t7-val1;
wave_0_per_frame16=t8=t8-val2;
wave_0_per_frame17=
wave_0_per_frame18=t3=q2;
wave_0_per_point1=c1=6.2831*t1/(1.1-sample);
wave_0_per_point2=c=cos(c1);
wave_0_per_point3=s=sin(c1);
wave_0_per_point4=c2=sqrt(1-sample);
wave_0_per_point5=
wave_0_per_point6=ox=t7-.5*c2*c;
wave_0_per_point7=oy=t8-.625*c2*s;
wave_0_per_point8=
wave_0_per_point9=x=t7+((ox-t7)*cos(t2)-(oy-t8)*sin(t2));
wave_0_per_point10=y=t8+((ox-t7)*sin(t2)+(oy-t8)*cos(t2));
wave_0_per_point11=
wave_0_per_point12=x=x*.55;
wave_0_per_point13=y=(y-.5)*.55+.5;
wave_0_per_point14=
wave_0_per_point15=r=sample;
wave_0_per_point16=g=1-sample;
wave_0_per_point17=b=1;
wave_0_per_point18=a=below(sample,.995);
wave_0_per_point19=
wave_0_per_point20=d=above(q3-sample,0)*below(q3-sample,.4)*(sample-q3)*2.5;
wave_0_per_point21=d=sqrt(d)*(1-sqrt((sample-q3)*2.5));
wave_0_per_point22=a=a*(1-d);
wave_0_per_point23=
wave_0_per_point24=y=y+t3;
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=0
wavecode_1_bDrawThick=0
wavecode_1_bAdditive=0
wavecode_1_scaling=1.00000
wavecode_1_smoothing=0.00000
wavecode_1_r=1.000
wavecode_1_g=1.000
wavecode_1_b=1.000
wavecode_1_a=1.000
wave_1_per_frame1=t1=q1;
wave_1_per_frame2=
wave_1_per_frame3=t7=.0;
wave_1_per_frame4=t8=.45;
wave_1_per_frame5=
wave_1_per_frame6=ddx=.25*cos(5.7119*t1)+2.5963*t1*sin(5.7119*t1);
wave_1_per_frame7=ddy=.3125*sin(5.7119*t1)-3.2453*t1*cos(5.7119*t1);
wave_1_per_frame8=ddtan=atan2(ddy,ddx);
wave_1_per_frame9=t2=-ddtan;
wave_1_per_frame10=
wave_1_per_frame11=val1=((-.5*cos(5.7119*t1))*cos(t2)-(-.625*sin(5.7119*t1))*sin(t2));
wave_1_per_frame12=val2=((-.5*cos(5.7119*t1))*sin(t2)+(-.625*sin(5.7119*t1))*cos(t2));
wave_1_per_frame13=
wave_1_per_frame14=t6=-sign(t1);
wave_1_per_frame15=t7=t7-val1;
wave_1_per_frame16=t8=t8-val2;
wave_1_per_frame17=
wave_1_per_frame18=t3=q2;
wave_1_per_frame19=
wave_1_per_point1=c1=6.2831*t1/(1.1-sample);
wave_1_per_point2=c=cos(c1);
wave_1_per_point3=s=sin(c1);
wave_1_per_point4=c2=sqrt(1-sample);
wave_1_per_point5=
wave_1_per_point6=ox=t7-.5*c2*c;
wave_1_per_point7=oy=t8-.625*c2*s;
wave_1_per_point8=
wave_1_per_point9=x=t7+((ox-t7)*cos(t2)-(oy-t8)*sin(t2));
wave_1_per_point10=y=t8+((ox-t7)*sin(t2)+(oy-t8)*cos(t2));
wave_1_per_point11=
wave_1_per_point12=inv=1/sqr(1.1-sample);
wave_1_per_point13=fdx=-.25*pow(1-sample,-.5)*c-c2*s*3.1415*t1*inv;
wave_1_per_point14=fdy=-.3125*c2*s+3.9268*c2*c*t1*inv;
wave_1_per_point15=invMag=1/sqrt(sqr(fdx)+sqr(fdy));
wave_1_per_point16=fdx=fdx*invMag;
wave_1_per_point17=fdy=fdy*invMag;
wave_1_per_point18=
wave_1_per_point19=rdx=fdx*cos(1.5707+t2)-fdy*sin(1.5707+t2);
wave_1_per_point20=rdy=fdx*sin(1.5707+t2)+fdx*cos(1.5707+t2);
wave_1_per_point21=
wave_1_per_point22=x=x+rdx*.15*(1-sample);
wave_1_per_point23=y=y+rdy*.15*(1-sample);
wave_1_per_point24=
wave_1_per_point25=x=x*.55;
wave_1_per_point26=y=(y-.5)*.55+.5;
wave_1_per_point27=
wave_1_per_point28=r=sample;
wave_1_per_point29=g=1-sample;
wave_1_per_point30=b=1;
wave_1_per_point31=a=below(sample,.995);
wave_1_per_point32=d=above(q3-sample,0)*below(q3-sample,.4)*(sample-q3)*2.5;
wave_1_per_point33=d=sqrt(d)*(1-sqrt((sample-q3)*2.5));
wave_1_per_point34=a=a*(1-d);
wave_1_per_point35=
wave_1_per_point36=
wave_1_per_point37=y=y+t3;
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=1
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.00000
wavecode_2_smoothing=0.00000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_per_frame1=t1=q1;
wave_2_per_frame2=
wave_2_per_frame3=t7=.0;
wave_2_per_frame4=t8=.45;
wave_2_per_frame5=
wave_2_per_frame6=ddx=.25*cos(5.7119*t1)+2.5963*t1*sin(5.7119*t1);
wave_2_per_frame7=ddy=.3125*sin(5.7119*t1)-3.2453*t1*cos(5.7119*t1);
wave_2_per_frame8=ddtan=atan2(ddy,ddx);
wave_2_per_frame9=t2=-ddtan;
wave_2_per_frame10=
wave_2_per_frame11=val1=((-.5*cos(5.7119*t1))*cos(t2)-(-.625*sin(5.7119*t1))*sin(t2));
wave_2_per_frame12=val2=((-.5*cos(5.7119*t1))*sin(t2)+(-.625*sin(5.7119*t1))*cos(t2));
wave_2_per_frame13=
wave_2_per_frame14=t6=-sign(t1);
wave_2_per_frame15=t7=t7-val1;
wave_2_per_frame16=t8=t8-val2;
wave_2_per_frame17=
wave_2_per_frame18=t3=q2;
wave_2_per_point1=sample=pow(sample,.85);
wave_2_per_point2=
wave_2_per_point3=c1=6.2831*t1/(1.1-sample);
wave_2_per_point4=c=cos(c1);
wave_2_per_point5=s=sin(c1);
wave_2_per_point6=c2=sqrt(1-sample);
wave_2_per_point7=
wave_2_per_point8=ox=t7-.5*c2*c;
wave_2_per_point9=oy=t8-.625*c2*s;
wave_2_per_point10=
wave_2_per_point11=x=t7+((ox-t7)*cos(t2)-(oy-t8)*sin(t2));
wave_2_per_point12=y=t8+((ox-t7)*sin(t2)+(oy-t8)*cos(t2));
wave_2_per_point13=
wave_2_per_point14=inv=1/sqr(1.1-sample);
wave_2_per_point15=fdx=-.25*pow(1-sample,-.5)*c-c2*s*3.1415*t1*inv;
wave_2_per_point16=fdy=-.3125*c2*s+3.9268*c2*c*t1*inv;
wave_2_per_point17=invMag=1/sqrt(sqr(fdx)+sqr(fdy));
wave_2_per_point18=fdx=fdx*invMag;
wave_2_per_point19=fdy=fdy*invMag;
wave_2_per_point20=
wave_2_per_point21=rdx=fdx*cos(1.5707+t2)-fdy*sin(1.5707+t2);
wave_2_per_point22=rdy=fdx*sin(1.5707+t2)+fdx*cos(1.5707+t2);
wave_2_per_point23=tt=int(rand(100))/100;
wave_2_per_point24=x=x+rdx*(.15*tt)*(1-sample);
wave_2_per_point25=y=y+rdy*(.15*tt)*(1-sample);
wave_2_per_point26=
wave_2_per_point27=x=x*.55;
wave_2_per_point28=y=(y-.5)*.55+.5;
wave_2_per_point29=
wave_2_per_point30=r=sample;
wave_2_per_point31=g=1-sample;
wave_2_per_point32=b=1;
wave_2_per_point33=a=below(sample,.995);
wave_2_per_point34=
wave_2_per_point35=
wave_2_per_point36=y=y+t3;
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=100.00000
wavecode_3_smoothing=0.00000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_per_frame1=t1=q1;
wave_3_per_frame2=
wave_3_per_frame3=t7=.0;
wave_3_per_frame4=t8=.45;
wave_3_per_frame5=
wave_3_per_frame6=ddx=.25*cos(5.7119*t1)+2.5963*t1*sin(5.7119*t1);
wave_3_per_frame7=ddy=.3125*sin(5.7119*t1)-3.2453*t1*cos(5.7119*t1);
wave_3_per_frame8=ddtan=atan2(ddy,ddx);
wave_3_per_frame9=t2=-ddtan;
wave_3_per_frame10=
wave_3_per_frame11=val1=((-.5*cos(5.7119*t1))*cos(t2)-(-.625*sin(5.7119*t1))*sin(t2));
wave_3_per_frame12=val2=((-.5*cos(5.7119*t1))*sin(t2)+(-.625*sin(5.7119*t1))*cos(t2));
wave_3_per_frame13=
wave_3_per_frame14=t6=-sign(t1);
wave_3_per_frame15=t7=t7-val1;
wave_3_per_frame16=t8=t8-val2;
wave_3_per_frame17=
wave_3_per_frame18=t3=q2;
wave_3_per_frame19=t5=-1+2*(frame%2);
wave_3_per_frame20=
wave_3_per_frame21=t4=.4;    // spectrum trail length
wave_3_per_point1=c1=6.2831*t1/(1.1-sample);
wave_3_per_point2=c=cos(c1);
wave_3_per_point3=s=sin(c1);
wave_3_per_point4=c2=sqrt(1-sample);
wave_3_per_point5=
wave_3_per_point6=ox=t7-.5*c2*c;
wave_3_per_point7=oy=t8-.625*c2*s;
wave_3_per_point8=
wave_3_per_point9=x=t7+((ox-t7)*cos(t2)-(oy-t8)*sin(t2));
wave_3_per_point10=y=t8+((ox-t7)*sin(t2)+(oy-t8)*cos(t2));
wave_3_per_point11=
wave_3_per_point12=inv=1/sqr(1.1-sample);
wave_3_per_point13=fdx=-.25*pow(1-sample,-.5)*c-c2*s*3.1415*t1*inv;
wave_3_per_point14=fdy=-.3125*c2*s+3.9268*c2*c*t1*inv;
wave_3_per_point15=invMag=1/sqrt(sqr(fdx)+sqr(fdy));
wave_3_per_point16=fdx=fdx*invMag;
wave_3_per_point17=fdy=fdy*invMag;
wave_3_per_point18=
wave_3_per_point19=rdx=fdx*cos(1.5707+t2)-fdy*sin(1.5707+t2);
wave_3_per_point20=rdy=fdx*sin(1.5707+t2)+fdx*cos(1.5707+t2);
wave_3_per_point21=
wave_3_per_point22=x=x+t5*rdx*.15*(1-sample)*(equal(t5,1)+abs(value1+value2));
wave_3_per_point23=y=y+t5*rdy*.15*(1-sample)*(equal(t5,1)+abs(value1+value2));
wave_3_per_point24=
wave_3_per_point25=x=x*.55;
wave_3_per_point26=y=(y-.5)*.55+.5;
wave_3_per_point27=
wave_3_per_point28=r=1;
wave_3_per_point29=g=1;
wave_3_per_point30=b=0;
wave_3_per_point31=a=below(sample,.995);
wave_3_per_point32=d=above(q3-sample,0)*below(q3-sample,t4)*(sample-q3)/t4;
wave_3_per_point33=d=sqrt(d)*(1-sqrt((sample-q3)/t4));
wave_3_per_point34=a=a*d;
wave_3_per_point35=
wave_3_per_point36=
wave_3_per_point37=y=y+t3;
shapecode_0_enabled=1
shapecode_0_sides=100
shapecode_0_additive=1
shapecode_0_thickOutline=0
shapecode_0_textured=0
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=0.10000
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=1.00000
shapecode_0_r=1.000
shapecode_0_g=1.000
shapecode_0_b=1.000
shapecode_0_a=1.000
shapecode_0_r2=0.000
shapecode_0_g2=0.000
shapecode_0_b2=1.000
shapecode_0_a2=0.000
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shape_0_per_frame1=t1=q1;//.2*sin(time*.34);
shape_0_per_frame2=
shape_0_per_frame3=t7=.0; // start x
shape_0_per_frame4=t8=.45; // start y
shape_0_per_frame5=
shape_0_per_frame6=ddx=.25*cos(5.7119*t1)+2.5963*t1*sin(5.7119*t1);
shape_0_per_frame7=ddy=.3125*sin(5.7119*t1)-3.2453*t1*cos(5.7119*t1);
shape_0_per_frame8=
shape_0_per_frame9=ddtan=atan2(ddy,ddx);
shape_0_per_frame10=t2=-ddtan;
shape_0_per_frame11=
shape_0_per_frame12=val1=((-.5*cos(5.7119*t1))*cos(t2)-(-.625*sin(5.7119*t1))*sin(t2));
shape_0_per_frame13=val2=((-.5*cos(5.7119*t1))*sin(t2)+(-.625*sin(5.7119*t1))*cos(t2));
shape_0_per_frame14=
shape_0_per_frame15=t6=-sign(t1);
shape_0_per_frame16=t7=t7-val1;
shape_0_per_frame17=t8=t8-val2;
shape_0_per_frame18=t5=frame%2;
shape_0_per_frame19=
shape_0_per_frame20=sample=q3;
shape_0_per_frame21=rad=(t5*.15+(1-t5)*.3)*(1.1-sample);
shape_0_per_frame22=sides=t5*100+(1-t5)*4;
shape_0_per_frame23=ang=4*6.2831*sqrt(sample);
shape_0_per_frame24=a=1;//pow(1-sample,.25);
shape_0_per_frame25=
shape_0_per_frame26=
shape_0_per_frame27=c1=6.2831*t1/(1.1-sample);
shape_0_per_frame28=c=cos(c1);
shape_0_per_frame29=s=sin(c1);
shape_0_per_frame30=c2=sqrt(1-sample);
shape_0_per_frame31=c3=t1/sqr(1.1-sample);
shape_0_per_frame32=
shape_0_per_frame33=ox=t7-.5*c2*c;
shape_0_per_frame34=oy=t8-.625*c2*s;
shape_0_per_frame35=
shape_0_per_frame36=x=t7+((ox-t7)*cos(t2)-(oy-t8)*sin(t2));
shape_0_per_frame37=y=t8+((ox-t7)*sin(t2)+(oy-t8)*cos(t2));
shape_0_per_frame38=
shape_0_per_frame39=fdx=-.25*pow(1-sample,-.5)*c-3.1415*c2*s*c3;
shape_0_per_frame40=fdy=-.3125*c2*s+1.9634*c2*c*c3;
shape_0_per_frame41=invMag=1/sqrt(sqr(fdx)+sqr(fdy));
shape_0_per_frame42=fdx=fdx*invMag;
shape_0_per_frame43=fdy=fdy*invMag;
shape_0_per_frame44=
shape_0_per_frame45=rdx=fdx*cos(1.5707+t2)-fdy*sin(1.5707+t2);
shape_0_per_frame46=rdy=fdx*sin(1.5707+t2)+fdx*cos(1.5707+t2);
shape_0_per_frame47=
shape_0_per_frame48=x=x+rdx*+.152*sqrt(.995-sample);
shape_0_per_frame49=y=y+rdy*+.152*sqrt(.995-sample);
shape_0_per_frame50=
shape_0_per_frame51=x=(x-0)*.55+0;
shape_0_per_frame52=y=(y-.5)*.55+.5;
shape_0_per_frame53=y=y+q2;
shape_0_per_frame54=
shape_0_per_frame55=
shapecode_1_enabled=1
shapecode_1_sides=100
shapecode_1_additive=1
shapecode_1_thickOutline=0
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.10000
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=1.00000
shapecode_1_r=1.000
shapecode_1_g=1.000
shapecode_1_b=1.000
shapecode_1_a=1.000
shapecode_1_r2=0.000
shapecode_1_g2=0.000
shapecode_1_b2=1.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.000
shape_1_per_frame1=t1=q1;//.2*sin(time*.34);
shape_1_per_frame2=
shape_1_per_frame3=t7=.0; // start x
shape_1_per_frame4=t8=.45; // start y
shape_1_per_frame5=
shape_1_per_frame6=ddx=.25*cos(5.7119*t1)+2.5963*t1*sin(5.7119*t1);
shape_1_per_frame7=ddy=.3125*sin(5.7119*t1)-3.2453*t1*cos(5.7119*t1);
shape_1_per_frame8=
shape_1_per_frame9=ddtan=atan2(ddy,ddx);
shape_1_per_frame10=t2=-ddtan;
shape_1_per_frame11=
shape_1_per_frame12=val1=((-.5*cos(5.7119*t1))*cos(t2)-(-.625*sin(5.7119*t1))*sin(t2));
shape_1_per_frame13=val2=((-.5*cos(5.7119*t1))*sin(t2)+(-.625*sin(5.7119*t1))*cos(t2));
shape_1_per_frame14=
shape_1_per_frame15=t6=-sign(t1);
shape_1_per_frame16=t7=t7-val1;
shape_1_per_frame17=t8=t8-val2;
shape_1_per_frame18=t5=frame%2;
shape_1_per_frame19=
shape_1_per_frame20=sample=q3;
shape_1_per_frame21=rad=(t5*.15+(1-t5)*.3)*(1.1-sample);
shape_1_per_frame22=sides=t5*100+(1-t5)*4;
shape_1_per_frame23=ang=4*6.2831*sqrt(sample);
shape_1_per_frame24=a=1;//pow(1-sample,.25);
shape_1_per_frame25=
shape_1_per_frame26=
shape_1_per_frame27=c1=6.2831*t1/(1.1-sample);
shape_1_per_frame28=c=cos(c1);
shape_1_per_frame29=s=sin(c1);
shape_1_per_frame30=c2=sqrt(1-sample);
shape_1_per_frame31=c3=t1/sqr(1.1-sample);
shape_1_per_frame32=
shape_1_per_frame33=ox=t7-.5*c2*c;
shape_1_per_frame34=oy=t8-.625*c2*s;
shape_1_per_frame35=
shape_1_per_frame36=x=t7+((ox-t7)*cos(t2)-(oy-t8)*sin(t2));
shape_1_per_frame37=y=t8+((ox-t7)*sin(t2)+(oy-t8)*cos(t2));
shape_1_per_frame38=
shape_1_per_frame39=fdx=-.25*pow(1-sample,-.5)*c-3.1415*c2*s*c3;
shape_1_per_frame40=fdy=-.3125*c2*s+1.9634*c2*c*c3;
shape_1_per_frame41=invMag=1/sqrt(sqr(fdx)+sqr(fdy));
shape_1_per_frame42=fdx=fdx*invMag;
shape_1_per_frame43=fdy=fdy*invMag;
shape_1_per_frame44=
shape_1_per_frame45=rdx=fdx*cos(1.5707+t2)-fdy*sin(1.5707+t2);
shape_1_per_frame46=rdy=fdx*sin(1.5707+t2)+fdx*cos(1.5707+t2);
shape_1_per_frame47=
shape_1_per_frame48=x=x+rdx*-.075*sqrt(.995-sample);
shape_1_per_frame49=y=y+rdy*-.075*sqrt(.995-sample);
shape_1_per_frame50=
shape_1_per_frame51=x=(x-0)*.55+0;
shape_1_per_frame52=y=(y-.5)*.55+.5;
shape_1_per_frame53=y=y+q2;
shape_1_per_frame54=
shape_1_per_frame55=
shapecode_2_enabled=1
shapecode_2_sides=100
shapecode_2_additive=0
shapecode_2_thickOutline=0
shapecode_2_textured=1
shapecode_2_num_inst=1
shapecode_2_x=0.500
shapecode_2_y=0.500
shapecode_2_rad=1.52770
shapecode_2_ang=3.14159
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=0.65190
shapecode_2_r=1.000
shapecode_2_g=1.000
shapecode_2_b=1.000
shapecode_2_a=1.000
shapecode_2_r2=1.000
shapecode_2_g2=1.000
shapecode_2_b2=1.000
shapecode_2_a2=0.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.000
shape_2_per_frame1=ang=3.1415;
shape_2_per_frame2=additive=equal(frame%20,0);
shapecode_3_enabled=1
shapecode_3_sides=100
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=1
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=1.09998
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=0.34480
shapecode_3_r=1.000
shapecode_3_g=1.000
shapecode_3_b=1.000
shapecode_3_a=1.000
shapecode_3_r2=0.000
shapecode_3_g2=0.000
shapecode_3_b2=0.500
shapecode_3_a2=0.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.000
shape_3_per_frame1=ang=6.2831*(.02*time-int(.02*time));
shape_3_per_frame2=
shape_3_per_frame3=r=abs(cos(2.43*time+4.343+sin(1.754*time+.753)));
shape_3_per_frame4=g=abs(cos(1.95*time+.932+cos(2.254*time+3.534)));
shape_3_per_frame5=b=abs(sin(1.95*time+.932+cos(2.254*time+3.534)));
shape_3_per_frame6=
shape_3_per_frame7=r2=1-r;
shape_3_per_frame8=g2=1-g;
shape_3_per_frame9=b2=1-b;
shape_3_per_frame10=
shape_3_per_frame11=additive=frame%2;
per_frame_1=decay=.90;
per_pixel_1=zoom=1.01;
comp_1=`shader_body
comp_2=`{
comp_3=`    float rad_lq = rad * length(texsize.xy)*0.5;
comp_4=`    float ang_lq = ang;
comp_5=`    float2 uv_temp1 = (uv - 0.5) * texsize.xy;
comp_6=`    float rad_hq = length(uv_temp1);
comp_7=`    float ang_hq = atan2(-uv_temp1.y, uv_temp1.x);
comp_8=`
comp_9=`    float2 uv2 = (uv - 0.5);
comp_10=`    float rad2 = rad_lq*0.8;
comp_11=`    float ang2 = ang_lq * M_INV_PI_2;
comp_12=`
comp_13=`        // ROTATION OVER TIME
comp_14=`        #if 1
comp_15=`          ang2 += time*0.025;   //rotate over time
comp_16=`        #endif
comp_17=`
comp_18=`        // FIN TYPE
comp_19=`        float fins = 3 + floor(rand_preset.z*5.95);
comp_20=`        #if 1     // SHARP FINS
comp_21=`          ang2 = frac(ang2*fins)/fins;
comp_22=`              // ENABLE THIS TO MAKE THE FINS ALTERNATE: (seamless!)
comp_23=`              ang2 = abs(ang2 - 0.5/fins);
comp_24=`        #else     // COSINE FINS - a bit slow
comp_25=`          ang2 = cos(ang2*M_PI_2*fins) * 0.023;
comp_26=`        #endif
comp_27=`
comp_28=`        // RADIAL KALEIDOSCOPING?
comp_29=`        #if 0
comp_30=`          rad2 *= g_fTexSize.z;
comp_31=`            // choose one:
comp_32=`            //rad2 = lerp(rad2, frac(rad2*3)/3.0, 0.5);
comp_33=`            rad2 = cos(rad2*5);
comp_34=`            //rad2 = sqrt(rad2)*0.5;
comp_35=`            //rad2 += abs(frac(rad2*7)-0.5)/7.0 * 1.15;  // stepifier
comp_36=`            //rad2 += cos(rad2*61)*0.02;
comp_37=`          rad2 *= g_fTexSize.x;
comp_38=`        #endif
comp_39=`
comp_40=`    ang2 *= M_PI_2;
comp_41=`    uv2 = 0.5 + rad2*float2(cos(ang2),sin(ang2))*texsize.zw;
comp_42=`
comp_43=`    ret = tex2D(sampler_main, uv2).xyz;
comp_44=`    ret *= 1.333; // a little bit of overbright
comp_45=`}
