MILKDROP_PRESET_VERSION=201
PSVERSION=2
PSVERSION_WARP=2
PSVERSION_COMP=2
[preset00]
fRating=1.000000
fGammaAdj=1.000
fDecay=0.900
fVideoEchoZoom=1.000
fVideoEchoAlpha=0.000
nVideoEchoOrientation=3
nWaveMode=6
bAdditiveWaves=0
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=0
bMaximizeWaveColor=0
bTexWrap=1
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=0
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=0.005
fWaveScale=0.167
fWaveSmoothing=0.000
fWaveParam=0.000
fModWaveAlphaStart=1.000
fModWaveAlphaEnd=1.000
fWarpAnimSpeed=1.000
fWarpScale=0.107
fZoomExponent=1.00183
fShader=1.000
zoom=0.96098
rot=0.00000
cx=0.500
cy=0.500
dx=0.00000
dy=0.00000
warp=0.01000
sx=1.00000
sy=1.00000
wave_r=1.000
wave_g=1.000
wave_b=1.000
wave_x=0.950
wave_y=1.000
ob_size=0.040
ob_r=0.000
ob_g=0.000
ob_b=0.000
ob_a=1.000
ib_size=0.000
ib_r=1.000
ib_g=1.000
ib_b=1.000
ib_a=1.000
nMotionVectorsX=64.000
nMotionVectorsY=48.000
mv_dx=-0.002
mv_dy=0.000
mv_l=0.000
mv_r=1.000
mv_g=0.000
mv_b=0.000
mv_a=0.000
b1n=0.000
b2n=0.000
b3n=0.000
b1x=1.000
b2x=1.000
b3x=1.000
b1ed=0.250
wavecode_0_enabled=1
wavecode_0_samples=457
wavecode_0_sep=0
wavecode_0_bSpectrum=0
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=3.80064
wavecode_0_smoothing=1.00000
wavecode_0_r=0.000
wavecode_0_g=1.000
wavecode_0_b=0.000
wavecode_0_a=1.000
wave_0_init1=t8 = 1;
wave_0_per_frame1=t1 = q1;
wave_0_per_frame2=t2 = q2;
wave_0_per_frame3=t3 = q3;
wave_0_per_frame4=t4 = q4;
wave_0_per_frame5=t5 = q5;
wave_0_per_frame6=t6 = q6;
wave_0_per_frame7=
wave_0_per_frame8=pi3 = 3.1415*2*0.3333;
wave_0_per_frame9=
wave_0_per_frame10=t = (q4+q5+q6)*0.005;
wave_0_per_frame11=c=5;
wave_0_per_frame12=r = 1-sin(t)*c;
wave_0_per_frame13=
wave_0_per_frame14=g = 1-sin(t+pi3)*c;
wave_0_per_frame15=
wave_0_per_frame16=b = 1-sin(t-pi3)*c;
wave_0_per_frame17=
wave_0_per_frame18=
wave_0_per_frame19=r = if(above(r,1),1,r);
wave_0_per_frame20=r = if(below(r,0),0,r);
wave_0_per_frame21=g = if(above(g,1),1,g);
wave_0_per_frame22=g = if(below(g,0),0,g);
wave_0_per_frame23=b = if(above(b,1),1,b);
wave_0_per_frame24=b = if(below(b,0),0,b);
wave_0_per_point1=t8 = -t8;
wave_0_per_point2=d = sqrt(1-sqr((sample-0.5)*2));
wave_0_per_point3=z = sample*0.4 - 0.2;
wave_0_per_point4=x = sin(sample*100)*d*0.2;
wave_0_per_point5=y = cos(sample*100)*d*0.2;
wave_0_per_point6=
wave_0_per_point7=p = 0.1;
wave_0_per_point8=x = x*(1+t8*p);
wave_0_per_point9=y = y*(1+t8*p);
wave_0_per_point10=z = z*(1+t8*p);
wave_0_per_point11=
wave_0_per_point12=
wave_0_per_point13=dir = (t4-t6)*0.4 + (t1-t3)*(t8+1)*0.2;
wave_0_per_point14=d = 2 + pow(t2,3);
wave_0_per_point15=w = t5*0.4 + (t8+1)*t2*0.2;
wave_0_per_point16=
wave_0_per_point17=zz = z;
wave_0_per_point18=yy = y;
wave_0_per_point19=y = cos(w)*yy - sin(w)*zz;
wave_0_per_point20=z = sin(w)*yy + cos(w)*zz;
wave_0_per_point21=
wave_0_per_point22=xx = cos(dir)*x - sin(dir)*y;
wave_0_per_point23=yy = sin(dir)*x + cos(dir)*y;
wave_0_per_point24=
wave_0_per_point25=d = 0.5;
wave_0_per_point26=zoom = 2 - sqrt(t2)*1.1;
wave_0_per_point27=zm = sqrt(x*x+y*y+sqr(z+d))/d;
wave_0_per_point28=
wave_0_per_point29=x = 0.5 + zoom*xx*0.55/zm;
wave_0_per_point30=y = 0.5 + zoom*yy*0.55/zm;
wave_0_per_point31=
wave_0_per_point32=a = sigmoid(-z+0.1,25);
wavecode_1_enabled=1
wavecode_1_samples=457
wavecode_1_sep=0
wavecode_1_bSpectrum=0
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=3.80064
wavecode_1_smoothing=1.00000
wavecode_1_r=0.000
wavecode_1_g=1.000
wavecode_1_b=0.000
wavecode_1_a=1.000
wave_1_init1=t8 = 1;
wave_1_per_frame1=t1 = q1;
wave_1_per_frame2=t2 = q2;
wave_1_per_frame3=t3 = q3;
wave_1_per_frame4=t4 = q4;
wave_1_per_frame5=t5 = q5;
wave_1_per_frame6=t6 = q6;
wave_1_per_frame7=
wave_1_per_frame8=pi3 = 3.1415*2*0.3333;
wave_1_per_frame9=
wave_1_per_frame10=t = (q4+q5+q6)*0.005 + 2;
wave_1_per_frame11=c=5;
wave_1_per_frame12=r = 1-sin(t)*c;
wave_1_per_frame13=
wave_1_per_frame14=g = 1-sin(t+pi3)*c;
wave_1_per_frame15=
wave_1_per_frame16=b = 1-sin(t-pi3)*c;
wave_1_per_frame17=
wave_1_per_frame18=
wave_1_per_frame19=r = if(above(r,1),1,r);
wave_1_per_frame20=r = if(below(r,0),0,r);
wave_1_per_frame21=g = if(above(g,1),1,g);
wave_1_per_frame22=g = if(below(g,0),0,g);
wave_1_per_frame23=b = if(above(b,1),1,b);
wave_1_per_frame24=b = if(below(b,0),0,b);
wave_1_per_point1=t8 = -t8;
wave_1_per_point2=d = sqrt(1-sqr((sample-0.5)*2));
wave_1_per_point3=z = sample*0.4 - 0.2;
wave_1_per_point4=x = sin(sample*100)*d*0.2;
wave_1_per_point5=y = cos(sample*100)*d*0.2;
wave_1_per_point6=
wave_1_per_point7=p = 0.1;
wave_1_per_point8=x = x*(1+t8*p);
wave_1_per_point9=y = y*(1+t8*p);
wave_1_per_point10=z = z*(1+t8*p);
wave_1_per_point11=
wave_1_per_point12=
wave_1_per_point13=dir = (t4-t6)*0.4 + (t1-t3)*(t8+1)*0.2;
wave_1_per_point14=d = 2 + pow(t2,3);
wave_1_per_point15=w = t5*0.4 + (t8+1)*t2*0.2;
wave_1_per_point16=
wave_1_per_point17=zz = z;
wave_1_per_point18=yy = y;
wave_1_per_point19=y = cos(w)*yy - sin(w)*zz;
wave_1_per_point20=z = sin(w)*yy + cos(w)*zz;
wave_1_per_point21=
wave_1_per_point22=xx = cos(dir)*x - sin(dir)*y;
wave_1_per_point23=yy = sin(dir)*x + cos(dir)*y;
wave_1_per_point24=
wave_1_per_point25=d = 0.5;
wave_1_per_point26=zoom = 2 - sqrt(t2)*1.1;
wave_1_per_point27=zm = sqrt(x*x+y*y+sqr(z+d))/d;
wave_1_per_point28=
wave_1_per_point29=x = 0.5 + zoom*xx*0.55/zm;
wave_1_per_point30=y = 0.5 + zoom*yy*0.55/zm;
wave_1_per_point31=
wave_1_per_point32=a = sigmoid(-z+0.1,25);
wavecode_2_enabled=0
wavecode_2_samples=512
wavecode_2_sep=4
wavecode_2_bSpectrum=0
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=1
wavecode_2_scaling=1.37242
wavecode_2_smoothing=1.00000
wavecode_2_r=1.000
wavecode_2_g=1.000
wavecode_2_b=1.000
wavecode_2_a=1.000
wave_2_init1=t2 = 0;
wave_2_init2=t3 = 0;
wave_2_init3=t4 = 0;
wave_2_init4=ab = 1;
wave_2_per_frame1=t1 = q1*0.5;
wave_2_per_frame2=t2 = q2*0.5;
wave_2_per_frame3=t3 = q3*0.5;
wave_2_per_frame4=t4 = q4;
wave_2_per_frame5=t5 = q5;
wave_2_per_frame6=t6 = q6;
wave_2_per_point1=s8 = sample*383;
wave_2_per_point2=
wave_2_per_point3=s = 0.3;
wave_2_per_point4=xx = ((sample*343)%7 - 3.5)*s + value1;
wave_2_per_point5=yy = ((sample*49)%7 - 3.5)*s*0.5;
wave_2_per_point6=zz = ((sample*7)%7 - 3.5)*s*0.5;
wave_2_per_point7=
wave_2_per_point8=n = 300;
wave_2_per_point9=xx = (-0.5+sample)*2;
wave_2_per_point10=zz = cos(sample*n)*0.02;
wave_2_per_point11=yy = sin(sample*n)*0.02;
wave_2_per_point12=
wave_2_per_point13=d = sqrt( xx*xx + yy*yy + zz*zz);
wave_2_per_point14=d1 = 1;
wave_2_per_point15=xx = xx*d1*(1+value1);
wave_2_per_point16=yy = yy*d1*(1+value2);
wave_2_per_point17=zz = zz*d1;
wave_2_per_point18=
wave_2_per_point19=w = .3;//+0*(d)*(t6);//(sample*sin(time*0.3)*0.02-1);
wave_2_per_point20=m = d*d*2;
wave_2_per_point21=s1 = sin(t4*w + m*t1);
wave_2_per_point22=s2 = sin(t5*w + m*t2);
wave_2_per_point23=s3 = sin(t6*w + m*t3);
wave_2_per_point24=c1 = cos(t4*w + m*t1);
wave_2_per_point25=c2 = cos(t5*w + m*t2);
wave_2_per_point26=c3 = cos(t6*w + m*t3);
wave_2_per_point27=
wave_2_per_point28=z = (c3*s1*c2 + s3*s2)*xx - (c3*s1*s2-s3*c2)*yy + c3*c1*zz;
wave_2_per_point29=x1 = (c1*c2*xx + c1*s2*yy - s1*zz);
wave_2_per_point30=y1 = ((s3*s1*c2 - c3*s2)*xx + (s3*s1*s2+c3*c2)*yy + s3*c1*zz);
wave_2_per_point31=
wave_2_per_point32=a = 2;
wave_2_per_point33=zoom = 0.3*atan2(a-z,a);//0.5*(1/(z+a));
wave_2_per_point34=x = 0.5 + zoom*x1;
wave_2_per_point35=y = 0.5 + zoom*y1;
wave_2_per_point36=
wave_2_per_point37=pi3 = 3.1415*2*0.3333;
wave_2_per_point38=t = -xx+t5*.2;
wave_2_per_point39=c = 10;
wave_2_per_point40=r = sin(t)*c;
wave_2_per_point41=
wave_2_per_point42=g = sin(t+pi3)*c;
wave_2_per_point43=
wave_2_per_point44=b = sin(t-pi3)*c;
wave_2_per_point45=
wave_2_per_point46=j = 0.81;
wave_2_per_point47=//r = 0.25+xx*j;
wave_2_per_point48=//g = 0.25+yy*j;
wave_2_per_point49=//b = 0.25+zz*j;
wave_2_per_point50=
wave_2_per_point51=r = if(above(r,1),1,r);
wave_2_per_point52=r = if(below(r,0),0,r);
wave_2_per_point53=g = if(above(g,1),1,g);
wave_2_per_point54=g = if(below(g,0),0,g);
wave_2_per_point55=b = if(above(b,1),1,b);
wave_2_per_point56=b = if(below(b,0),0,b);
wave_2_per_point57=
wave_2_per_point58=
wave_2_per_point59=a = 2;//sigmoid(-z,1)*5.0+0.0;
wavecode_3_enabled=0
wavecode_3_samples=512
wavecode_3_sep=4
wavecode_3_bSpectrum=0
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=1
wavecode_3_bAdditive=1
wavecode_3_scaling=1.37242
wavecode_3_smoothing=1.00000
wavecode_3_r=1.000
wavecode_3_g=1.000
wavecode_3_b=1.000
wavecode_3_a=1.000
wave_3_init1=t2 = 0;
wave_3_init2=t3 = 0;
wave_3_init3=t4 = 0;
wave_3_init4=ab = 1;
wave_3_per_frame1=t1 = q1*0.5;
wave_3_per_frame2=t2 = q2*0.5;
wave_3_per_frame3=t3 = q3*0.5;
wave_3_per_frame4=t4 = q4;
wave_3_per_frame5=t5 = q5;
wave_3_per_frame6=t6 = q6;
wave_3_per_point1=s8 = sample*383;
wave_3_per_point2=
wave_3_per_point3=s = 0.3;
wave_3_per_point4=xx = ((sample*343)%7 - 3.5)*s + value1;
wave_3_per_point5=yy = ((sample*49)%7 - 3.5)*s*0.5;
wave_3_per_point6=zz = ((sample*7)%7 - 3.5)*s*0.5;
wave_3_per_point7=
wave_3_per_point8=n = 300;
wave_3_per_point9=zz = (-0.5+sample)*2;
wave_3_per_point10=xx = cos(sample*n)*0.02;
wave_3_per_point11=yy = sin(sample*n)*0.02;
wave_3_per_point12=
wave_3_per_point13=d = sqrt( xx*xx + yy*yy + zz*zz);
wave_3_per_point14=d1 = 1;
wave_3_per_point15=xx = xx*d1*(1+value1);
wave_3_per_point16=yy = yy*d1*(1+value2);
wave_3_per_point17=zz = zz*d1;
wave_3_per_point18=
wave_3_per_point19=w = .3;//+0*(d)*(t6);//(sample*sin(time*0.3)*0.02-1);
wave_3_per_point20=m = d*d*2;
wave_3_per_point21=s1 = sin(t4*w + m*t1);
wave_3_per_point22=s2 = sin(t5*w + m*t2);
wave_3_per_point23=s3 = sin(t6*w + m*t3);
wave_3_per_point24=c1 = cos(t4*w + m*t1);
wave_3_per_point25=c2 = cos(t5*w + m*t2);
wave_3_per_point26=c3 = cos(t6*w + m*t3);
wave_3_per_point27=
wave_3_per_point28=z = (c3*s1*c2 + s3*s2)*xx - (c3*s1*s2-s3*c2)*yy + c3*c1*zz;
wave_3_per_point29=x1 = (c1*c2*xx + c1*s2*yy - s1*zz);
wave_3_per_point30=y1 = ((s3*s1*c2 - c3*s2)*xx + (s3*s1*s2+c3*c2)*yy + s3*c1*zz);
wave_3_per_point31=
wave_3_per_point32=a = 2;
wave_3_per_point33=zoom = 0.3*atan2(a-z,a);//0.5*(1/(z+a));
wave_3_per_point34=x = 0.5 + zoom*x1;
wave_3_per_point35=y = 0.5 + zoom*y1;
wave_3_per_point36=
wave_3_per_point37=pi3 = 3.1415*2*0.3333;
wave_3_per_point38=t = -zz+t6*.2;
wave_3_per_point39=c = 10;
wave_3_per_point40=r = sin(t)*c;
wave_3_per_point41=
wave_3_per_point42=g = sin(t+pi3)*c;
wave_3_per_point43=
wave_3_per_point44=b = sin(t-pi3)*c;
wave_3_per_point45=
wave_3_per_point46=j = 0.81;
wave_3_per_point47=//r = 0.25+xx*j;
wave_3_per_point48=//g = 0.25+yy*j;
wave_3_per_point49=//b = 0.25+zz*j;
wave_3_per_point50=
wave_3_per_point51=r = if(above(r,1),1,r);
wave_3_per_point52=r = if(below(r,0),0,r);
wave_3_per_point53=g = if(above(g,1),1,g);
wave_3_per_point54=g = if(below(g,0),0,g);
wave_3_per_point55=b = if(above(b,1),1,b);
wave_3_per_point56=b = if(below(b,0),0,b);
wave_3_per_point57=
wave_3_per_point58=
wave_3_per_point59=a = 2;//sigmoid(-z,1)*5.0+0.0;
shapecode_0_enabled=0
shapecode_0_sides=100
shapecode_0_additive=0
shapecode_0_thickOutline=1
shapecode_0_textured=0
shapecode_0_num_inst=1
shapecode_0_x=0.500
shapecode_0_y=0.500
shapecode_0_rad=0.42324
shapecode_0_ang=0.00000
shapecode_0_tex_ang=0.00000
shapecode_0_tex_zoom=0.50330
shapecode_0_r=1.000
shapecode_0_g=0.000
shapecode_0_b=0.000
shapecode_0_a=1.000
shapecode_0_r2=1.000
shapecode_0_g2=1.000
shapecode_0_b2=1.000
shapecode_0_a2=0.000
shapecode_0_border_r=1.000
shapecode_0_border_g=1.000
shapecode_0_border_b=1.000
shapecode_0_border_a=0.000
shape_0_init1=vx = 0;
shape_0_init2=vy = 0;
shape_0_per_frame1=t = -(q4+q5)*0.2;
shape_0_per_frame2=x = 0.5 + sin(t)*0.2;
shape_0_per_frame3=y = 0.5 + cos(t)*0.1;
shape_0_per_frame4=rad = 0.4 - cos(t)*0.3;
shapecode_1_enabled=0
shapecode_1_sides=100
shapecode_1_additive=0
shapecode_1_thickOutline=1
shapecode_1_textured=0
shapecode_1_num_inst=1
shapecode_1_x=0.500
shapecode_1_y=0.500
shapecode_1_rad=0.42324
shapecode_1_ang=0.00000
shapecode_1_tex_ang=0.00000
shapecode_1_tex_zoom=0.50330
shapecode_1_r=0.000
shapecode_1_g=0.000
shapecode_1_b=1.000
shapecode_1_a=1.000
shapecode_1_r2=1.000
shapecode_1_g2=1.000
shapecode_1_b2=1.000
shapecode_1_a2=0.000
shapecode_1_border_r=1.000
shapecode_1_border_g=1.000
shapecode_1_border_b=1.000
shapecode_1_border_a=0.000
shape_1_init1=vx = 0;
shape_1_init2=vy = 0;
shape_1_per_frame1=t = -(q4+q5)*0.2;
shape_1_per_frame2=pi = asin(1)*2;
shape_1_per_frame3=x = 0.5 + sin(t+pi)*0.2;
shape_1_per_frame4=y = 0.5 + cos(t+pi)*0.1;
shape_1_per_frame5=rad = 0.4 - cos(t+pi)*0.3;
shapecode_2_enabled=0
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=1
shapecode_2_textured=0
shapecode_2_num_inst=1
shapecode_2_x=1.000
shapecode_2_y=0.500
shapecode_2_rad=1.00591
shapecode_2_ang=0.00000
shapecode_2_tex_ang=0.00000
shapecode_2_tex_zoom=0.50330
shapecode_2_r=0.000
shapecode_2_g=0.000
shapecode_2_b=1.000
shapecode_2_a=1.000
shapecode_2_r2=0.000
shapecode_2_g2=0.000
shapecode_2_b2=1.000
shapecode_2_a2=1.000
shapecode_2_border_r=1.000
shapecode_2_border_g=1.000
shapecode_2_border_b=1.000
shapecode_2_border_a=0.000
shape_2_init1=vx = 0;
shape_2_init2=vy = 0;
shape_2_per_frame1=x = 1.2;
shape_2_per_frame2=y = q3- 0.4;
shapecode_3_enabled=0
shapecode_3_sides=100
shapecode_3_additive=0
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_num_inst=1
shapecode_3_x=0.500
shapecode_3_y=0.500
shapecode_3_rad=0.99595
shapecode_3_ang=0.00000
shapecode_3_tex_ang=0.00000
shapecode_3_tex_zoom=1.00000
shapecode_3_r=0.000
shapecode_3_g=0.000
shapecode_3_b=0.000
shapecode_3_a=0.100
shapecode_3_r2=1.000
shapecode_3_g2=1.000
shapecode_3_b2=1.000
shapecode_3_a2=1.000
shapecode_3_border_r=1.000
shapecode_3_border_g=1.000
shapecode_3_border_b=1.000
shapecode_3_border_a=0.000
shape_3_per_frame1=rad = 0.5 + (q1-q2+q3)*1;
shape_3_per_frame2=ang = -(q4-q5)*0.2;
shape_3_per_frame3=
shape_3_per_frame4=pi3 = 3.1415*2*0.3333;
shape_3_per_frame5=
shape_3_per_frame6=t = (q4-2*q5+q6)*0.2;
shape_3_per_frame7=c=3;
shape_3_per_frame8=r = sin(t)*c;
shape_3_per_frame9=
shape_3_per_frame10=g = sin(t+pi3)*c;
shape_3_per_frame11=
shape_3_per_frame12=b = sin(t-pi3)*c;
shape_3_per_frame13=
shape_3_per_frame14=
shape_3_per_frame15=r = if(above(r,1),1,r);
shape_3_per_frame16=r = if(below(r,0),0,r);
shape_3_per_frame17=g = if(above(g,1),1,g);
shape_3_per_frame18=g = if(below(g,0),0,g);
shape_3_per_frame19=b = if(above(b,1),1,b);
shape_3_per_frame20=b = if(below(b,0),0,b);
shape_3_per_frame21=
shape_3_per_frame22=r2 = 1-r;
shape_3_per_frame23=g2 = 1-g;
shape_3_per_frame24=b2 = 1-b;
per_frame_init_1=x1 = 0;
per_frame_init_2=y1 = 0;
per_frame_1=vb = vb*0.95 + (1-vb)*pow(bass,2)*0.02;
per_frame_2=vvb = vvb*0.95 + (1-vvb)*vb*0.01;
per_frame_3=vm = vm*0.95 + (1-vm)*pow(mid,2)*0.02;
per_frame_4=vvm = vvm*0.95 + (1-vvm)*vm*0.01;
per_frame_5=vt = vt*0.95 + (1-vt)*pow(treb,2)*0.02;
per_frame_6=vvt = vvt*0.95 + (1-vvt)*vt*0.01;
per_frame_7=vvb = min(1,max(0,vvb));
per_frame_8=vvm = min(1,max(0,vvm));
per_frame_9=vvt = min(1,max(0,vvt));
per_frame_10=
per_frame_11=q1 = vvb*2;//0.5 + vb - vvb;
per_frame_12=q2 = vvm*2;//0.5 + vm - vvm;
per_frame_13=q3 = vvt*2;//0.5 + vt - vvt;
per_frame_14=
per_frame_15=v=2;
per_frame_16=
per_frame_17=bb = bb - vvb*v;
per_frame_18=mm = mm - vvm*v;
per_frame_19=tt = tt - vvt*v;
per_frame_20=
per_frame_21=q4 = bb;
per_frame_22=q5 = mm;
per_frame_23=q6 = tt;
per_frame_24=
per_frame_25=pi3 = 3.1415*2*0.3333;
per_frame_26=
per_frame_27=t = (q4+q5+q6)*0.005;
per_frame_28=c=3;
per_frame_29=r = sin(t)*c;
per_frame_30=
per_frame_31=g = sin(t+pi3)*c;
per_frame_32=
per_frame_33=b = sin(t-pi3)*c;
per_frame_34=
per_frame_35=ob_r = min(1,max(0,r));
per_frame_36=ob_g = min(1,max(0,g));
per_frame_37=ob_b = min(1,max(0,b));
per_pixel_1=pi = asin(1);
per_pixel_2=
per_pixel_3=x = x-0.5;
per_pixel_4=y = y- 0.5;
per_pixel_5=
per_pixel_6=d = (q4-q6)*0.4 +  (rad-0.3)*(q1-q3)*2 + pi;
per_pixel_7=xx = sin(d)*x - cos(d)*y;
per_pixel_8=yy = cos(d)*x + sin(d)*y;
per_pixel_9=
per_pixel_10=
per_pixel_11=x = xx;
per_pixel_12=y = yy;
per_pixel_13=
per_pixel_14=
per_pixel_15=t = time*.2;
per_pixel_16=xh = x;
per_pixel_17=yh = y;
per_pixel_18=
per_pixel_19=w = (q4-q6)*0.8;
per_pixel_20=m = -1 + q2*2;
per_pixel_21=wv = pi-sin(w)*m;
per_pixel_22=wh = pi-cos(w)*m;
per_pixel_23=d = 8*sqrt(q2);
per_pixel_24=ww = 1.2;
per_pixel_25=ddx = sin(2*pi - wv -(x)*ww);
per_pixel_26=ddy = sin(2*pi - wh -(y)*ww);
per_pixel_27=rx = if(above(ddx*ddy,0),sin(wv)/ddx,0);
per_pixel_28=ry = if(above(ddy*ddy,0),sin(wh)/ddy,0);
per_pixel_29=
per_pixel_30=v = -(q2)*.1*(d/ww);
per_pixel_31=
per_pixel_32=ax = ax + sin(w)*v;
per_pixel_33=ay = ay + cos(w)*v;
per_pixel_34=
per_pixel_35=vx = if(equal(rx*ry,0),0,ax);
per_pixel_36=vy = if(equal(rx*ry,0),0,ay);
per_pixel_37=
per_pixel_38=dx = (-xh*rx*ry*d + vx*.001);
per_pixel_39=dy = (-yh*rx*ry*d + vy*.001);
per_pixel_40=
per_pixel_41=//zoom = 0.93;
warp_1=`shader_body
warp_2=`{
warp_3=`    // sample previous frame
warp_4=`   float3 pre = tex2D( sampler_main, uv_orig);
warp_5=`   float3 warped = tex2D( sampler_main, uv -floor(uv));
warp_6=`    
warp_7=`  ret = lerp( pre, warped, 0.5);
warp_8=`    // darken (decay) over time
warp_9=`    ret *= 0.90; //or try: ret -= 0.004;
warp_10=`}
comp_1=`shader_body
comp_2=`{
comp_3=`    ret = tex2D(sampler_main, uv).xyz;
comp_4=`    ret *= 1.00; //gamma
comp_5=`    ret *= hue_shader; //old hue shader effect
comp_6=`}
